{"text_format":"1","workbook":"xlsx","n_sheets":13,"sheets":["CV195B-dresser (2)","Data","Fluides","Property GasPak","Property HePak","Dump_Case_A","Dump_Case_B","Dump_Case_C","Dump_Case_D","Dump_Case_E","Dump_Case_D2","Dump_Baking","Dump_STS"],"not_rendered":{"charts":5,"images":16,"macros":0,"external_links":4,"defined_names":62,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"CV195B-dresser (2)","index":0,"n_rows":142,"n_cols":31,"rows_kept":142,"cut":false,"hidden":false,"merged":[[118,1,122,1],[1,9,1,10],[4,9,4,10],[8,1,13,1],[72,1,98,1],[101,1,110,1]]}
[]
[null,null,null,null,null,null,"Job nbr :","C1243",null,"Document number",null," "]
[null,null,null,null,null,null,"Name :","JT60SA",null,"C1243-SP-452 A1(4)",null," "]
[null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,"Reference",null," "]
[null,null,"Valves Datasheet",null,"WARM VALVES",null,null,null,null,{"$f":" [4]!nom_p()","v":"CV195B-dresser (2)"},null," "]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"[4]!Collar_From_DN(J7,\"V\")","v":60}]
[null,null,null,null,null,null,null,null,null," ",null,{"$f":"[4]!Collar_From_DN(J8,\"V\")","v":250}]
[null,"PROJECT",null,null,null,null,null,null,null,null,null,{"$f":"[4]!Collar_From_DN(J9,\"V\")","v":60}]
[null,null,"Tag Number",null,{"$f":"J6","v":"CV195B-dresser (2)"},null,null,"PID Number",null,null,null,{"$f":"[4]!Collar_From_DN(J10,\"V\")","v":60},null,{"$f":"[4]!vlookup_colonne(J6,\"_table_main\",\"col_description\")","v":{"$error":"#VALUE!"}}]
[null,null,"Valve Description",null,{"$f":"[4]!vlookup_colonne(J6,\"_table_main\",\"col_description\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"[4]!Collar_From_DN(J11,\"V\")","v":60}]
[null,null,"Equipement / Line",null,null,null,null,null,null,null,null,{"$f":"[4]!Collar_From_DN(J12,\"V\")","v":60}]
[null,null,"Remarks for the design :",null,{"$f":"[4]!vlookup_colonne(J6,\"_table_main\",\"col_type\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"[4]!Collar_From_DN(J13,\"V\")","v":60}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"[4]!Collar_From_DN(J14,\"V\")","v":60}]
[null,"PROCESS",null,null,null,null,null,null,null,null,null,{"$f":"[4]!Collar_From_DN(J15,\"V\")","v":60}]
[null,null,"Case",null,null,null,null,"Minimum flow","Minimum Flow","Max Flow","Max Flow",{"$f":"[4]!Collar_From_DN(J16,\"V\")","v":250},null,{"$f":"J26+#REF!","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"[4]!Collar_From_DN(J17,\"V\")","v":60}]
[null,null,"Fluid Composition",null,null," ",null,"Helium","Helium","Helium","Helium",{"$f":"[4]!Collar_From_DN(J18,\"V\")","v":250}]
[null,null,"Number",null,null,null,null,10,10,10,10,{"$f":"[4]!Collar_From_DN(J19,\"V\")","v":60}]
[null,null,"Inlet Fluid",null,null,null,null,null,null,null,null,{"$f":"[4]!Collar_From_DN(J20,\"V\")","v":60}]
[null,null,"Outlet Fluid",null,null,null,null,null,null,null,null,{"$f":"[4]!Collar_From_DN(J21,\"V\")","v":60}]
[null,null,null,null,null,null,null,{"$f":"[4]!Flow_Test(H19,H31,H32,H27,H36,$K$60)","v":"Chocked Flow"},{"$f":"[4]!Flow_Test(I19,I31,I32,I27,I36,$K$60)","v":"Chocked Flow"},{"$f":"[4]!Flow_Test(J19,J31,J32,J27,J36,$K$60)","v":"Chocked Flow"},{"$f":"[4]!Flow_Test(K19,K31,K32,K27,K36,$K$60)","v":"Chocked Flow"},{"$f":"[4]!Collar_From_DN(J22,\"V\")","v":250}]
[null,null,null,null,null,null,"g/s",{"$f":"IF($G$26=\"Nm3/h\",44.6153*H26*H48/3600,H26)","v":600},{"$f":"IF($G$26=\"Nm3/h\",44.6153*I26*I48/3600,I26)","v":30},{"$f":"IF($G$26=\"Nm3/h\",44.6153*J26*J48/3600,J26)","v":50},{"$f":"IF($G$26=\"Nm3/h\",44.6153*K26*K48/3600,K26)","v":70},{"$f":"[4]!Collar_From_DN(J23,\"V\")","v":120}]
[null,null,null,null,null,null,"Nm3/h",{"$f":"IF($G$26=\"g/s\",H26*3.6/H41,H26)","v":12104.65227741896},{"$f":"IF($G$26=\"g/s\",I26*3.6/I41,I26)","v":605.23261387094794},{"$f":"IF($G$26=\"g/s\",J26*3.6/J41,J26)","v":1008.7210231182466},{"$f":"IF($G$26=\"g/s\",K26*3.6/K41,K26)","v":1412.2094323655451},{"$f":"[4]!Collar_From_DN(J24,\"V\")","v":250}]
[null,null,null,null,null,null,"m3/h",{"$f":"H23*3.6/H39","v":659.9328615973883},{"$f":"I23*3.6/I39","v":43.21199990571921},{"$f":"J23*3.6/J39","v":72.019999842865346},{"$f":"K23*3.6/K39","v":100.82799978001148},{"$f":"[4]!Collar_From_DN(J25,\"V\")","v":160}]
[null,null,"Flowrate",null,null,null,"g/s",600,30,50,70,{"$f":"[4]!Collar_From_DN(J26,\"V\")","v":120},{"$f":"[4]!ESTFORMULE(H26)","v":false},{"$f":"[4]!ESTFORMULE(I26)","v":false},{"$f":"[4]!ESTFORMULE(J26)","v":false},{"$f":"[4]!ESTFORMULE(K26)","v":false}]
[null,null,null,null,null,null,"K",{"$f":"IF($G$29=\"K\",H29,273.15+H29)","v":306},{"$f":"IF($G$29=\"K\",I29,273.15+I29)","v":306},306,306,{"$f":"[4]!Collar_From_DN(J27,\"V\")","v":250}]
[null,null,null,null,null,null,"°C",{"$f":"IF($G$29=\"K\",H29-273.15,H29)","v":32.850000000000023},{"$f":"IF($G$29=\"K\",I29-273.15,I29)","v":32.850000000000023},32.850000000000023,32.850000000000023,{"$f":"[4]!Collar_From_DN(J28,\"V\")","v":80}]
[null,null,"Inlet Temperature ",null,null,null,"K",{"$f":"273.15+32.85","v":306},306,306,306,{"$f":"[4]!Collar_From_DN(J29,\"V\")","v":250},{"$f":"[4]!ESTFORMULE(H29)","v":true},{"$f":"[4]!ESTFORMULE(I29)","v":false},{"$f":"[4]!ESTFORMULE(J29)","v":false},{"$f":"[4]!ESTFORMULE(K29)","v":false}]
[null,null,"Outlet Temperature",null,null,null,"K",{"$f":"[4]!Tout(H19,H31,H32,H29)","v":307.22999308706414},{"$f":"[4]!Tout(I19,I31,I32,I29)","v":306.91936979171641},{"$f":"[4]!Tout(J19,J31,J32,J29)","v":306.91936979171641},{"$f":"[4]!Tout(K19,K31,K32,K29)","v":306.91936979171641},{"$f":"[4]!Collar_From_DN(J30,\"V\")","v":250}]
[null,null,"Pressure",null,"Inlet","Pin","bar abs",21,16,16,16,{"$f":"[4]!Collar_From_DN(J31,\"V\")","v":60},{"$f":"[4]!ESTFORMULE(H31)","v":false},{"$f":"[4]!ESTFORMULE(I31)","v":false},{"$f":"[4]!ESTFORMULE(J31)","v":false},{"$f":"[4]!ESTFORMULE(K31)","v":false}]
[null,null,null,null,"Outlet","Pout","bar abs",1.2,1.2,1.2,1.2,{"$f":"[4]!Collar_From_DN(J32,\"V\")","v":60},{"$f":"[4]!ESTFORMULE(H32)","v":false},{"$f":"[4]!ESTFORMULE(I32)","v":false},{"$f":"[4]!ESTFORMULE(J32)","v":false},{"$f":"[4]!ESTFORMULE(K32)","v":false}]
[null,null,"Differential Pressure",null,null,"DP","bar",{"$f":"H31-H32","v":19.8},{"$f":"I31-I32","v":14.8},{"$f":"J31-J32","v":14.8},{"$f":"K31-K32","v":14.8},{"$f":"[4]!Collar_From_DN(J33,\"V\")","v":60},{"$f":"[4]!ESTFORMULE(H33)","v":true},{"$f":"[4]!ESTFORMULE(I33)","v":true},{"$f":"[4]!ESTFORMULE(J33)","v":true},{"$f":"[4]!ESTFORMULE(K33)","v":true}]
[null,null,"Maximum Effective Differential Pressure",null,null,"DP","bar",{"$f":"[4]!dp_max(H19,H23*H36,H31,H32,H27,$K$60)","v":17.010000000000002},{"$f":"[4]!dp_max(I19,I23*I36,I31,I32,I27,$K$60)","v":12.96},{"$f":"[4]!dp_max(J19,J23*J36,J31,J32,J27,$K$60)","v":12.96},{"$f":"[4]!dp_max(K19,K23*K36,K31,K32,K27,$K$60)","v":12.96},{"$f":"[4]!Collar_From_DN(J34,\"V\")","v":60}]
[null,null,"Phase State",null,"Inlet",null,null,{"$f":"+[4]!PhaseState(H36)","v":"Gas"},{"$f":"+[4]!PhaseState(I36)","v":"Gas"},{"$f":"+[4]!PhaseState(J36)","v":"Gas"},{"$f":"+[4]!PhaseState(K36)","v":"Gas"},{"$f":"[4]!Collar_From_DN(J35,\"V\")","v":250}]
[null,null,"Vapour Fraction",null,"Inlet",null,"%",{"$f":"+[4]!VapourFraction_in(H19,H31,H32,H27)","v":1},{"$f":"+[4]!VapourFraction_in(I19,I31,I32,I27)","v":1},{"$f":"+[4]!VapourFraction_in(J19,J31,J32,J27)","v":1},{"$f":"+[4]!VapourFraction_in(K19,K31,K32,K27)","v":1},{"$f":"[4]!Collar_From_DN(J36,\"V\")","v":60}]
[null,null,"Phase State",null,"Outlet",null,null,{"$f":"+[4]!PhaseState(H38)","v":"Gas"},{"$f":"+[4]!PhaseState(I38)","v":"Gas"},{"$f":"+[4]!PhaseState(J38)","v":"Gas"},{"$f":"+[4]!PhaseState(K38)","v":"Gas"},{"$f":"[4]!Collar_From_DN(J37,\"V\")","v":250}]
[null,null,"Vapour Fraction",null,"Outlet",null,"%",{"$f":"+[4]!VapourFraction_out(H19,H31,H32,H27,H36)","v":1},{"$f":"+[4]!VapourFraction_out(I19,I31,I32,I27,I36)","v":1},{"$f":"+[4]!VapourFraction_out(J19,J31,J32,J27,J36)","v":1},{"$f":"+[4]!VapourFraction_out(K19,K31,K32,K27,K36)","v":1},{"$f":"[4]!Collar_From_DN(J38,\"V\")","v":60}]
[null,null,"Fluid density",null,"Inlet",null,"kg/m3",{"$f":"[4]!densite(H19,H31,H27,H23,H36)","v":3.273060224295623},{"$f":"[4]!densite(I19,I31,I27,I23,I36)","v":2.4993057538562558},{"$f":"[4]!densite(J19,J31,J27,J23,J36)","v":2.4993057538562558},{"$f":"[4]!densite(K19,K31,K27,K23,K36)","v":2.4993057538562558},{"$f":"[4]!Collar_From_DN(J39,\"V\")","v":60},null,null,{"$f":"378/3600","v":0.105}]
[null,null,"Fluid density",null,"Outlet",null,"kg/m3",{"$f":"[4]!densite_out(H19,H31,H32,H29,H36)","v":0.1879327973168575},{"$f":"[4]!densite_out(I19,I31,I32,I29,I36)","v":0.1881228827190905},{"$f":"[4]!densite_out(J19,J31,J32,J29,J36)","v":0.1881228827190905},{"$f":"[4]!densite_out(K19,K31,K32,K29,K36)","v":0.1881228827190905},{"$f":"[4]!Collar_From_DN(J40,\"V\")","v":60},{"$f":"[4]!g_(11,J31,H29)","v":1.4067728793654866}]
[null,null,"Normal fluid density",null,null,null,"kg/Nm3",{"$f":"[4]!densite(H19,1.013,273.15,H23,0)","v":0.17844378760300669},{"$f":"[4]!densite(I19,1.013,273.15,I23,0)","v":0.17844378760300669},{"$f":"[4]!densite(J19,1.013,273.15,J23,0)","v":0.17844378760300669},{"$f":"[4]!densite(K19,1.013,273.15,K23,0)","v":0.17844378760300669},{"$f":"[4]!Collar_From_DN(J41,\"V\")","v":60}]
[null,null,"Compressibility z (gas phase)",null,null,null,null,{"$f":"IF(AND(H36>0,H36<1),[4]!Z_(H19,H31,H44+0.01),[4]!Z_(H19,H31,H27))","v":1.0093883558684966},{"$f":"IF(AND(I36>0,I36<1),[4]!Z_(I19,I31,I44+0.01),[4]!Z_(I19,I31,I27))","v":1.0071486851467781},{"$f":"IF(AND(J36>0,J36<1),[4]!Z_(J19,J31,J44+0.01),[4]!Z_(J19,J31,J27))","v":1.0071486851467781},{"$f":"IF(AND(K36>0,K36<1),[4]!Z_(K19,K31,K44+0.01),[4]!Z_(K19,K31,K27))","v":1.0071486851467781},{"$f":"[4]!Collar_From_DN(J42,\"V\")","v":60}]
[null,null,"Saturation Pression",null,"Inlet",null,"bar abs",{"$f":"[4]!P_saturation(H19,H27)","v":0},{"$f":"[4]!P_saturation(I19,I27)","v":0},{"$f":"[4]!P_saturation(J19,J27)","v":0},{"$f":"[4]!P_saturation(K19,K27)","v":0},{"$f":"[4]!Collar_From_DN(J43,\"V\")","v":60}]
[null,null,"Saturation Temperature",null,"Inlet",null,"K",{"$f":"[4]!T_saturation(H19,H31)","v":0},{"$f":"[4]!T_saturation(I19,I31)","v":0},{"$f":"[4]!T_saturation(J19,J31)","v":0},{"$f":"[4]!T_saturation(K19,K31)","v":0},{"$f":"[4]!Collar_From_DN(J44,\"V\")","v":60}]
[null,null,"Saturation Temperature",null,"Outlet",null,"K",{"$f":"[4]!T_saturation(H19,H32)","v":4.4068423378845276},{"$f":"[4]!T_saturation(I19,I32)","v":4.4068423378845276},{"$f":"[4]!T_saturation(J19,J32)","v":4.4068423378845276},{"$f":"[4]!T_saturation(K19,K32)","v":4.4068423378845276},{"$f":"[4]!Collar_From_DN(J45,\"V\")","v":60}]
[null,null,"Critical Pressure",null,null,null,"bar abs",{"$f":"[4]!Pc_(H19)","v":2.2749999999999999},{"$f":"[4]!Pc_(I19)","v":2.2749999999999999},{"$f":"[4]!Pc_(J19)","v":2.2749999999999999},{"$f":"[4]!Pc_(K19)","v":2.2749999999999999},{"$f":"[4]!Collar_From_DN(J46,\"V\")","v":60}]
[null,null,"Critical Temperature",null,null,null,"K",{"$f":"[4]!Tc_(H19)","v":5.1952999999999996},{"$f":"[4]!Tc_(I19)","v":5.1952999999999996},{"$f":"[4]!Tc_(J19)","v":5.1952999999999996},{"$f":"[4]!Tc_(K19)","v":5.1952999999999996},{"$f":"[4]!Collar_From_DN(J47,\"V\")","v":60}]
[null,null,"Molar Mass",null,null,null,null,{"$f":"[4]!M_(H19)","v":4.0026000000000002},{"$f":"[4]!M_(I19)","v":4.0026000000000002},{"$f":"[4]!M_(J19)","v":4.0026000000000002},{"$f":"[4]!M_(K19)","v":4.0026000000000002},{"$f":"[4]!Collar_From_DN(J48,\"V\")","v":60}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"[4]!Collar_From_DN(J49,\"V\")","v":60}]
[null,null,"Gravity /Air",null,"Inlet","dg",null,{"$f":"[4]!FConstant(H19,12)/28.959*H42","v":{"$error":"#VALUE!"}},{"$f":"[4]!FConstant(I19,12)/28.959*I42","v":{"$error":"#VALUE!"}},{"$f":"[4]!FConstant(J19,12)/28.959*J42","v":{"$error":"#VALUE!"}},{"$f":"[4]!FConstant(K19,12)/28.959*K42","v":{"$error":"#VALUE!"}},{"$f":"[4]!Collar_From_DN(J50,\"V\")","v":{"$error":"#VALUE!"}}]
[null,null,"Gravity /Water",null,"Inlet","dg",null,{"$f":"H39/1000","v":3.2730602242956233E-3},{"$f":"I39/1000","v":2.4993057538562559E-3},{"$f":"J39/1000","v":2.4993057538562559E-3},{"$f":"K39/1000","v":2.4993057538562559E-3},{"$f":"[4]!Collar_From_DN(J51,\"V\")","v":60}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"[4]!Collar_From_DN(J52,\"V\")","v":60}]
[null,null,"Gaseous Cv (considering 100% gas flow)",null,null,null,"Usgpm PSI",{"$f":"[4]!cv_gaz(H19,H23*H36,H31,H32,H27,$K$60)","v":17.458692692683272},{"$f":"[4]!cv_gaz(I19,I23*I36,I31,I32,I27,$K$60)","v":1.144454904596045},{"$f":"[4]!cv_gaz(J19,J23*J36,J31,J32,J27,$K$60)","v":1.9074248409934083},{"$f":"[4]!cv_gaz(K19,K23*K36,K31,K32,K27,$K$60)","v":2.6703947773907717},{"$f":"[4]!Collar_From_DN(J53,\"V\")","v":60}]
[null,null,"Liquid Cv (considering 100% liquid flow)",null,null,null,"Usgpm PSI",{"$f":"[4]!CvLiq(H19,H23*(1-H36),H31,H32,H27,H36,$K$60)","v":0},{"$f":"[4]!CvLiq(I19,I23*(1-I36),I31,I32,I27,I36,$K$60)","v":0},{"$f":"[4]!CvLiq(J19,J23*(1-J36),J31,J32,J27,J36,$K$60)","v":0},{"$f":"[4]!CvLiq(K19,K23*(1-K36),K31,K32,K27,K36,$K$60)","v":0},{"$f":"[4]!Collar_From_DN(J54,\"V\")","v":60}]
[null,null,"Estimated Cv",null,null,null,"Usgpm PSI",{"$f":"H53+H54","v":17.458692692683272},{"$f":"I53+I54","v":1.144454904596045},{"$f":"J53+J54","v":1.9074248409934083},{"$f":"K53+K54","v":2.6703947773907717},{"$f":"[4]!Collar_From_DN(J55,\"V\")","v":60}]
[null,null,"Estimated Kv",null,null,null,"m3/h bar",{"$f":"H55*0.864978","v":15.101385087931792},{"$f":"I55*0.864978","v":0.98992831446767793},{"$f":"J55*0.864978","v":1.6498805241127963},{"$f":"K55*0.864978","v":2.309832733757915},{"$f":"[4]!Collar_From_DN(J56,\"V\")","v":60}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"[4]!Collar_From_DN(J57,\"V\")","v":60}]
[null,null,null,null,null,null,"%Cv",{"$f":"P68","v":1.0330587392120281},{"$f":"Q68","v":6.7719225124026339E-2},0.11286537520671056,0.1580115252893948,"  ",null,null,"Estimation"]
[null,null,null,null,null,null,"%Trim",{"$f":"P69","v":1.0070625079962068},0.41535599002939944,0.52628036483757756,0.59934438267669665,"  ",null,null,null,{"$f":"H16","v":"Minimum flow"},{"$f":"I16","v":"Minimum Flow"},{"$f":"J16","v":"Max Flow"},{"$f":"K16","v":"Max Flow"},null,"DN",40,"CVs"]
[null,null,null,null,null,null,"Cvs",{"$f":"P70","v":16.899999999999999},100,"XT",0.67,"  ",null,null,"Cv",{"$f":"H55","v":17.458692692683272},{"$f":"I55","v":1.144454904596045},{"$f":"J55","v":1.9074248409934083},{"$f":"K55","v":2.6703947773907717},null,"Supplier","V",{"$f":"[4]!Cv_From_DN($V$59,V60)","v":40}]
[null,null,null,null,null,null,null,null,null,null,null,"  ",null,null,"%Cv",{"$f":"[4]!Cv_From_Trim(P62,I60)","v":0.25118864315095796},{"$f":"Q60/P63","v":1.6465956511933822E-2},{"$f":"R60/P63","v":2.7443260853223034E-2},{"$f":"S60/P63","v":3.842056519451225E-2},null,"Supplier","W",{"$f":"[4]!Cv_From_DN($V$59,V61)","v":52}]
[null,null,null,null,null,null,null,"Inlet","1\"",{"$f":"VLOOKUP(I62,INDIRECT(VLOOKUP($E$83,Table_Piping_Class,7,FALSE)),4,FALSE)","v":27.86},"Seat",{"$f":"[4]!Collar_From_DN(#REF!,\"V\")","v":{"$error":"#VALUE!"}},{"$f":"4/1000*H26/(PI()*(25/2000)^2*H40)/[4]!Sound_speed(11,H32,H30)","v":19.483989678850318},null,"% OPEN",0.7,{"$f":"[4]!Trim_From_Cv(Q61,$I$60)","v":0.10829348203319261},{"$f":"[4]!Trim_From_Cv(R61,$I$60)","v":0.2192178568413708},{"$f":"[4]!Trim_From_Cv(S61,$I$60)","v":0.29228187468048983},null,"Supplier","F",{"$f":"[4]!Cv_From_DN($V$59,V62)","v":46.8}]
[null,null,null,null,null,null,null,"Valve","1\"",{"$f":"VLOOKUP(I63,INDIRECT(VLOOKUP($E$83,Table_Piping_Class,7,FALSE)),4,FALSE)","v":27.86},null,{"$f":"[4]!Collar_From_DN(#REF!,\"V\")","v":{"$error":"#VALUE!"}},{"$f":"[4]!Sound_speed(11,H32,H30)","v":1335.2447345184689},null,"Cvmax",{"$f":"IF(I60=\"Linear\",MAX(H55:K55),P60/P61)","v":69.504307494471576}]
[null,null,null,null,null,null,null,"outlet","4\"",{"$f":"VLOOKUP(I64,INDIRECT(VLOOKUP($E$83,Table_Piping_Class,7,FALSE)),4,FALSE)","v":108.2},null,{"$f":"[4]!Collar_From_DN(#REF!,\"V\")","v":{"$error":"#VALUE!"}},{"$f":"M62/M63","v":1.4592073778801947E-2}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"[4]!Collar_From_DN(I64,\"V\")","v":250},null,null,"Vérification du % d'ouverture pour un Cv Donné"]
[null,null,null,null,null,null,"Inlet piping",{"$f":"[4]!speed_and_mach(H19,H31,H29,H39,H26,$J$62)","v":"301 m/s ; 0.29"},{"$f":"[4]!speed_and_mach(I19,I31,I29,I39,I26,$J$62)","v":"20 m/s ; 0.02"},{"$f":"[4]!speed_and_mach(J19,J31,J29,J39,J26,$J$62)","v":"33 m/s ; 0.03"},{"$f":"[4]!speed_and_mach(K19,K31,K29,K39,K26,$J$62)","v":"46 m/s ; 0.04"},{"$f":"[4]!Collar_From_DN(#REF!,\"V\")","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"P59","v":"Minimum flow"},"Minimum Flow","Max Flow","Max Flow",null,null,"Inch.","DN"]
[null,null,null,null,null,null,"valve seat",{"$f":"[4]!Speed_valve(H24,H29,H31,25,H19)","v":0.33435511358876285},{"$f":"[4]!Speed_valve(I24,I29,I31,25,I19)","v":2.1987126312871332E-2},{"$f":"[4]!Speed_valve(J24,J29,J31,25,J19)","v":3.6645210521452226E-2},{"$f":"[4]!Speed_valve(K24,K29,K31,25,K19)","v":5.130329473003311E-2},{"$f":"[4]!Collar_From_DN(#REF!,\"V\")","v":{"$error":"#VALUE!"}},null,null,"Cv",17.458692692683272,1.144454904596045,1.9074248409934083,2.6703947773907717,null,"V",{"$f":"VLOOKUP(W67,table_DN_to_inch,3,FALSE)","v":"1\""},{"$f":"[4]!DN_From_Cv($P$70,U67)","v":25}]
[null,null,null,null,null,null,"valve outlet",{"$f":"[4]!speed_and_mach(H19,H32,H30,H39,H26,$J$63)","v":"301 m/s ; 0.29"},{"$f":"[4]!speed_and_mach(I19,I32,I30,I39,I26,$J$63)","v":"20 m/s ; 0.02"},{"$f":"[4]!speed_and_mach(J19,J32,J30,J39,J26,$J$63)","v":"33 m/s ; 0.03"},{"$f":"[4]!speed_and_mach(K19,K32,K30,K39,K26,$J$63)","v":"46 m/s ; 0.04"},{"$f":"[4]!Collar_From_DN(J70,\"V\")","v":250},null,null,"%Cv",{"$f":"P67/P70","v":1.0330587392120281},{"$f":"Q67/P70","v":6.7719225124026339E-2},{"$f":"R67/P70","v":0.11286537520671056},{"$f":"S67/P70","v":0.1580115252893948},null,"W",{"$f":"VLOOKUP(W68,table_DN_to_inch,3,FALSE)","v":"1\""},{"$f":"[4]!DN_From_Cv($P$70,U68)","v":25}]
[null,null,null,null,null,null,"piping outlet",{"$f":"[4]!speed_and_mach(H19,H32,H30,H40,H26,$J$64)","v":"347 m/s ; 0.34"},{"$f":"[4]!speed_and_mach(I19,I32,I30,I40,I26,$J$64)","v":"17 m/s ; 0.02"},{"$f":"[4]!speed_and_mach(J19,J32,J30,J40,J26,$J$64)","v":"29 m/s ; 0.03"},{"$f":"[4]!speed_and_mach(K19,K32,K30,K40,K26,$J$64)","v":"40 m/s ; 0.04"},{"$f":"[4]!Collar_From_DN(#REF!,\"V\")","v":{"$error":"#VALUE!"}},null,null,"% OPEN",{"$f":"[4]!Trim_From_Cv(P68,$I$60)","v":1.0070625079962068},{"$f":"[4]!Trim_From_Cv(Q68,$I$60)","v":0.41535599002939944},{"$f":"[4]!Trim_From_Cv(R68,$I$60)","v":0.52628036483757756},{"$f":"[4]!Trim_From_Cv(S68,$I$60)","v":0.59934438267669665},null,"F",{"$f":"VLOOKUP(W69,table_DN_to_inch,3,FALSE)","v":"1\""},{"$f":"[4]!DN_From_Cv($P$70,U69)","v":25}]
[null,null,null,null,null,null,"Tvc",{"$f":"[4]!T_vc(H19,H31,H32,H30,$K$60)","v":230.63363141807528},{"$f":"[4]!T_vc(I19,I31,I32,I30,$K$60)","v":230.35103100832728},{"$f":"[4]!T_vc(J19,J31,J32,J30,$K$60)","v":230.35103100832728},{"$f":"[4]!T_vc(K19,K31,K32,K30,$K$60)","v":230.35103100832728},{"$f":"[4]!Collar_From_DN(#REF!,\"V\")","v":{"$error":"#VALUE!"}},null,null,"Cvmax",16.899999999999999]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"[4]!Collar_From_DN(J71,\"V\")","v":60}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"[4]!Collar_From_DN(#REF!,\"V\")","v":{"$error":"#VALUE!"}}]
[null,"DESIGN SPECIFICATION","1. Design ",null,null,null,"5. Actuator",null,null,null,null,{"$f":"[4]!Collar_From_DN(#REF!,\"V\")","v":{"$error":"#VALUE!"}},null,null,"% Supplier",{"$f":"[4]!bary_(P68,1,$Y$88,$X$89:$X$99,$Y$89:$Y$99)","v":3.4435291307067604},{"$f":"[4]!bary_(Q68,1,$Y$88,$X$89:$X$99,$Y$89:$Y$99)","v":0.30274580467137302},{"$f":"[4]!bary_(R68,1,$Y$88,$X$89:$X$99,$Y$89:$Y$99)","v":0.41275466249736847},{"$f":"[4]!bary_(S68,1,$Y$88,$X$89:$X$99,$Y$89:$Y$99)","v":0.48596463560442399}]
[null,null,"Regulation",null,"Refrigeration Ordinance",null,"Actuator type",null,null,"Single Effect",null,{"$f":"[4]!Collar_From_DN(#REF!,\"V\")","v":{"$error":"#VALUE!"}}]
[null,null,"Construction Code",null,"ASME",null,"Shut-Off Pressure (Mpa)",null,null,{"$f":"[4]!vlookup_colonne(J6,\"_table_main\",\"col_shutoff_DP\")","v":{"$error":"#VALUE!"}},null,{"$f":"[4]!Collar_From_DN(#REF!,\"V\")","v":{"$error":"#VALUE!"}}]
[null,null,"Design Pressure",null,1,null,"Power supply",null,null,"NA",null,{"$f":"[4]!Collar_From_DN(#REF!,\"V\")","v":{"$error":"#VALUE!"}}]
[null,null,"Design Temperature (min / max)",null,273,400,"Failure position (FO/FC)",null,null,{"$f":"[4]!vlookup_colonne(J6,\"_table_main\",\"col_FO_FC\")","v":{"$error":"#VALUE!"}},null,{"$f":"[4]!Collar_From_DN(#REF!,\"V\")","v":{"$error":"#VALUE!"}}]
[null,null,"Equipment Conditions (location / temp.)",null,"Inside ","10°C/+40°C","Medium and pressure min.",null,null,"air @ 5-7barg (-40°C)",null,{"$f":"[4]!Collar_From_DN(#REF!,\"V\")","v":{"$error":"#VALUE!"}}]
[null,null,"Electrical Code",null,"IEC",null,"Filter / Regulator / Air Instru. Tubing",null,null,"YES / YES / acc. ambient temp.",null,{"$f":"[4]!Collar_From_DN(#REF!,\"V\")","v":{"$error":"#VALUE!"}}]
[null,null,"Moisture",null,"30%-87%",null,"6. Positioner",null,null,null,null,{"$f":"[4]!Collar_From_DN(#REF!,\"V\")","v":{"$error":"#VALUE!"}}]
[null,null,"Insulation Class",null,"IP54",null,"Positioner type",null,null,"Electro-Pneumatic",null,{"$f":"[4]!Collar_From_DN(#REF!,\"V\")","v":{"$error":"#VALUE!"}}]
[null,null,"2. Piping",null,null,null,"Positionner input signal",null,null,"4-20mA",null,{"$f":"[4]!Collar_From_DN(#REF!,\"V\")","v":{"$error":"#VALUE!"}}]
[null,null,"Piping Class",null,{"$f":"IF(E76<=1,\"A-01-S-5H-Y(0)\",\"A-03-S-5H-Y(0)\")","v":"A-01-S-5H-Y(0)"},null,"7. Accessories",null,null,null,null,{"$f":"[4]!Collar_From_DN(#REF!,\"V\")","v":{"$error":"#VALUE!"}}]
[null,null,"Piping nominal size in/ out (mm)",null,{"$f":"I62","v":"1\""},{"$f":"I64","v":"4\""},"Fully Close (ZSL) / Fully open (ZSH)",null,null,{"$f":"[4]!vlookup_colonne(J6,\"_table_main\",\"col_ZSL\")","v":{"$error":"#VALUE!"}},{"$f":"[4]!vlookup_colonne(J6,\"_table_main\",\"col_ZSH\")","v":{"$error":"#VALUE!"}},{"$f":"[4]!Collar_From_DN(J72,\"V\")","v":60}]
[null,null,"Piping Size (Øxmm)",null,{"$f":"VLOOKUP(E84,INDIRECT(VLOOKUP($E$83,Table_Piping_Class,7,FALSE)),5,FALSE)","v":"33.4x2.77mm"},{"$f":"VLOOKUP(F84,INDIRECT(VLOOKUP($E$83,Table_Piping_Class,7,FALSE)),5,FALSE)","v":"114.3x3.05mm"},"Tag of Switch",null,null,{"$f":"IF(J84=\"YES\",\"ZSL\"&RIGHT(J6,LEN(J6)-2),\"\")","v":{"$error":"#VALUE!"}},{"$f":"IF(K84=\"YES\",\"ZSH\"&RIGHT(J6,LEN(J6)-2),\"\")","v":{"$error":"#VALUE!"}},{"$f":"[4]!Collar_From_DN(J73,\"V\")","v":60}]
[null,null,"3. Valve body/Assembly",null,null,null,"Fast Closing (Dedicated Solenoïd valve)",null,null,{"$f":"[4]!vlookup_colonne(J6,\"_table_main\",\"col_EV\")","v":{"$error":"#VALUE!"}},null,{"$f":"[4]!Collar_From_DN(J74,\"V\")","v":250}]
[null,null,"Valve type",null,"Globe",null,"Tag of Electrovalve",null,null,{"$f":"IF(J86=\"YES\",\"EV\"&RIGHT(J6,LEN(J6)-2),\"\")","v":{"$error":"#VALUE!"}},null,"-",null,null,null,null,null,"h (%)","F (%)",null,null,null,null,"%Cv","%trim","Cv","%Cv"]
[null,null,"Body pattern",null,"Straight",null,"Positionner feedback signal",null,null,{"$f":"[4]!vlookup_colonne(J6,\"_table_main\",\"col_4_20_FeedBack\")","v":{"$error":"#VALUE!"}},null," ",null,null,null,null,null,0,{"$f":"[4]!Cv_From_Trim(R88,$I$60)","v":0},null,null,null,null,1,1,0,0,null,null,"Lineaire","=%"]
[null,null,"Estimated size",null,{"$f":"[4]!DN_From_Cv(P70,V60)","v":25},null,"Slow Opening/ Closing (~2min)",null,null,{"$f":"[4]!vlookup_colonne(J6,\"_table_main\",\"col_Slow_Opening\")","v":{"$error":"#VALUE!"}},null," ",null,null,null,null,null,0.05,{"$f":"[4]!Cv_From_Trim(R89,$I$60)","v":7.9244659623055689E-3},null,null,null,null,0,0,null,null,null,null,0,0]
[null,null,"Body / bonnet material",null,"304L or 316L",null,"8. Special Design",null,null,null,null," ",null,null,null,null,null,0.1,{"$f":"[4]!Cv_From_Trim(R90,$I$60)","v":1.5848931924611138E-2},null,null,null,null,{"$f":"+AA90","v":0.03},0.1,0.18,{"$f":"Z90/$Z$99","v":0.03},null,null,0.54,0.18]
[null,null,"Piping end connexion EN1092-1",null,"BW: Butt-Welded",null,"Interface to vaccum enclosure",null,null,"-",null," ",null,null,null,null,null,0.15,{"$f":"[4]!Cv_From_Trim(R91,$I$60)","v":1.9952623149688795E-2},null,null,null,null,{"$f":"+AA91","v":4.5000000000000005E-2},0.2,0.27,{"$f":"Z91/$Z$99","v":4.5000000000000005E-2},null,null,1.1000000000000001,0.27]
[null,null,"Packing",null,"See spec",null,"Thermalisation",null,null,{"$f":"[4]!vlookup_colonne(J6,\"_table_main\",\"col_Intercept\")","v":{"$error":"#VALUE!"}},null," ",null,null,null,null,null,0.2,{"$f":"[4]!Cv_From_Trim(R92,$I$60)","v":2.5118864315095805E-2},null,null,null,null,6.6666666666666666E-2,0.3,0.4,6.6666666666666666E-2,null,null,1.6,0.4]
[null,null,"Cleanliness",null,"See spec",null,"Handwheel",null,null,"-",null," ",null,null,null,null,null,0.25,{"$f":"[4]!Cv_From_Trim(R93,$I$60)","v":3.1622776601683798E-2},null,null,null,null,0.105,0.4,0.63,0.105,null,null,2.1,0.63]
[null,null,"Leakage to atmosphere",null,"See spec",null,"Locker ",null,null,"-",null," ",null,null,null,null,null,0.3,{"$f":"[4]!Cv_From_Trim(R94,$I$60)","v":3.981071705534972E-2},null,null,null,null,0.16666666666666666,0.5,1,0.16666666666666666,null,null,2.7,1]
[null,null,"4. Plug",null,null,null,"9. Quality Control",null,null,null,null," ",null,null,null,null,null,0.35,{"$f":"[4]!Cv_From_Trim(R95,$I$60)","v":5.011872336272722E-2},null,null,null,null,0.3,0.6,1.8,0.3,null,null,3.3,1.8]
[null,null,"Flow Tend to Open / To Close",null,{"$f":"[4]!vlookup_colonne(J6,\"_table_main\",\"col_FTO_FTC\")","v":{"$error":"#VALUE!"}},null,"Inspection Test Plan (ITP)",null,null,"Yes",null," ",null,null,null,null,null,0.4,{"$f":"[4]!Cv_From_Trim(R96,$I$60)","v":6.3095734448019344E-2},null,null,null,null,0.46666666666666662,0.7,2.8,0.46666666666666662,null,null,4,2.8]
[null,null,"Characteristic",null,"Equal % ",null,"Material Certificat",null,null,"3.1",null," ",null,null,null,null,null,0.45,{"$f":"[4]!Cv_From_Trim(R97,$I$60)","v":7.9432823472428166E-2},null,null,null,null,0.66666666666666663,0.8,4,0.66666666666666663,null,null,4.5999999999999996,4]
[null,null,"Rangeability",null,{"$f":"I60","v":100},null,null,null,null,null,null," ",null,null,null,null,null,0.5,{"$f":"[4]!Cv_From_Trim(R98,$I$60)","v":0.10000000000000002},null,null,null,null,0.8666666666666667,0.9,5.2,0.8666666666666667,null,null,5.3,5.2]
[null,null,"Seal",null,"See spec",null,null,null,null,null,null," ",null,null,null,null,null,0.55000000000000004,{"$f":"[4]!Cv_From_Trim(R99,$I$60)","v":0.12589254117941678},null,null,null,null,1,1,6,1,null,null,6,6]
[null,null,"Leakage class ANSI-FCI-70-2",null,"VI",null,null,null,null,null,null," ",null,null,null,null,null,0.6,{"$f":"[4]!Cv_From_Trim(R100,$I$60)","v":0.15848931924611134}]
[null,null,null,null,null,null,null,null,null,null,null," ",null,null,null,null,null,0.65,{"$f":"[4]!Cv_From_Trim(R101,$I$60)","v":0.199526231496888}]
[null,"VENDOR","Valve Main Characteristic",null,null,null,"Actuator and Positionner",null,null,null,null," ",null,null,null,null,null,0.7,{"$f":"[4]!Cv_From_Trim(R102,$I$60)","v":0.25118864315095796}]
[null,null,"Valve Manufacturer & Model",null,null,null,"Actuator Manufacturer & Model",null,null,null,null," ",null,null,null,null,null,0.75,{"$f":"[4]!Cv_From_Trim(R103,$I$60)","v":0.31622776601683794}]
[null,null,"Seat Size (mm) / Valve Cv (Usgpm PSI)",null,null,null,"Air Pressure",null,null,null,null," ",null,null,null,null,null,0.8,{"$f":"[4]!Cv_From_Trim(R104,$I$60)","v":0.39810717055349748}]
[null,null,"DN and PN",null,null,null,"Positionner Manufacturer & Model",null,null,null,null," ",null,null,null,null,null,0.85,{"$f":"[4]!Cv_From_Trim(R105,$I$60)","v":0.50118723362727235}]
[null,null,"Interfaces (BW Ø x mm / Flanges)",null,null,null,null,null,null,null,null," ",null,null,null,null,null,0.85,{"$f":"[4]!Cv_From_Trim(R106,$I$60)","v":0.50118723362727235}]
[null,null,"Cryogenic extension bonnet length",null,null,null,"Vendor Remark",null,null,null,null," ",null,null,null,null,null,0.9,{"$f":"[4]!Cv_From_Trim(R107,$I$60)","v":0.63095734448019347}]
[null,null,"Cold box cover plate diameter",null,null,null,null,null,null,null,null," ",null,null,null,null,null,0.95,{"$f":"[4]!Cv_From_Trim(R108,$I$60)","v":0.79432823472428171}]
[null,null,"Heat Leak",null,null,null,null,null,null,null,null," ",null,null,null,null,null,1,{"$f":"[4]!Cv_From_Trim(R109,$I$60)","v":1.0000000000000002}]
[null,null,"Plug seal material"]
[null,null,null,null,null,null,null,null,null,null,null," "]
[]
[null,"Gaseous Phase : Normal Flow (ΔP< Pin/2) :",null,null,null,null,null,"Critical Flow (ΔP ≥ Pin/2) :",null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null," "]
[null,"Liquid phase : ",null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,"Nm3 = m3 reduced to 0°C and 1.013 bar abs.",null,null,null,null,null,null,null,null," "]
[null,null,"ref : C.P. A0001. Use these formula with AL Normal Units only ! Nm3 = m3 reduced to 0°C and 1.013 bar abs.",null,null,null,null,null,null,null,null," "]
[null,"REMARKS","3\"",null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null," "]
[]
[null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null," "]
[null,"Revision",null,"DATE","BY","CHECKED","EVOLUTION",null,null,null,"Page"," "]
[null,1,null,"2013-07-05","V.HELOIN","A.MACHEFEL","Major Revision",null,null,null,null," "]
[null,2,null,"2013-08-05","V.HELOIN","A.MACHEFEL","Issue For Order",null,null,null,{"$f":"+[4]!Nb_pageauto()","v":"4/2"}," "]
[null,3,null," 20/09/2013","V.HELOIN","A.MACHEFEL","Issue For PIM",null,null,null,null," "]
[null,4,null," 21/10/2013","V.HELOIN","A.MACHEFEL","Issue After VELAN datasheet Review",null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null," "]

{"sheet":"Data","index":1,"n_rows":387,"n_cols":37,"rows_kept":387,"cut":false,"hidden":false,"merged":[[214,21,214,22],[214,23,214,24],[214,25,214,26],[214,27,214,28],[215,19,216,19],[80,3,80,6],[254,2,254,4],[254,5,254,7],[258,5,258,7],[212,19,212,20],[259,5,259,7],[255,2,255,4],[256,2,256,4],[257,2,257,4],[258,2,258,4],[259,2,259,4],[255,5,255,7],[256,5,256,7],[257,5,257,7]]}
[]
[]
[]
[]
[null,"Data"]
[null,"Gaspak Local =1, Gaspak Serveur = 2",null,null,1]
[null,"Regulation","ConstructionCode","MaterialCertificat","Etat","ValveFunction","ValveType","PlugType","BodyPattern","EndConnection","Cleanliness","PlugCharacteristic","ActuatorType","FailureType","PositionerType","Type","ElectricalCode","YESNO","Oring"]
[null,"ASME","ASME","2.2","Gaseous","TOR","Globe Valve","FTO ","Straight","BW: Butt-Welded","Oxygen Service","Equal % ","Single Effect","FC : Failure Close","Electro-Pneumatic","Manual","IEC","YES","NBR","A01S5HA"]
[null,"97/23/CE","CODAP 2005","3.1","Liquid","Manual","Eccentric rotary plug","FTC ","Angle","Flanged","Oil and grease free","Quick Opening","Double Effect","FO: Failure Open","Electric","TOR","UL","NO","FPM","A03S5HA"]
[null,"SELO","AD Merckblatt",null,null,null,"Butterfly valve",null,null,null,"Passivating","Linear"]
[null,"HPGSL",null,null,null,null,"Ball valve",null,null,null,null,"Dig"]
[null,null,null,null,null,null,"Synchronized block and bleed "]
[null,null,null,null,null,null,"Three Lever Valve"]
[]
[]
[]
[null,"PIPE DIMENSIONS WITH (Small thickness)"]
[]
[null,null,null,null,"DN\n(inch)","Din\n(mm)","Dim\n(Øxmm)"]
[null,null,null,"A03S5HA(5)","1/4\"",{"$f":"VLOOKUP(E20,INDIRECT(VLOOKUP(D20,Table_Piping_Class,7,FALSE)),4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(E20,INDIRECT(VLOOKUP(D20,Table_Piping_Class,7,FALSE)),5,FALSE)","v":{"$error":"#N/A"}}]
[]
[]
[null,null,"Table_Piping_Class"]
[null,null,null,"DN\n(inch)","DN\n(mm)","Dext\n(mm)","e\n(mm)","Din\n(mm)","TABLE"]
[null,null,"E42S5H(2)",4,5,6,7,8,"Piping_Class_01"]
[null,null,"E44S5H-A(0)",30,30,31,32,33,"Piping_Class_05"]
[null,null,"E46S5H-A(2)",10,11,12,13,14,"Piping_Class_02"]
[null,"LP","A-01-S-5H-Y(0)",16,17,18,19,20,"Piping_Class_03"]
[null,"HP","A-03-S-5H-Y(0)",23,24,25,26,27,"Piping_Class_04"]
[]
[null,null,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34]
[null,null,null,null,null,{"$f":"C25","v":"E42S5H(2)"},null,null,null,"Piping_Class_01",null,{"$f":"C27","v":"E46S5H-A(2)"},null,null,null,"Piping_Class_02",null,{"$f":"C28","v":"A-01-S-5H-Y(0)"},null,null,null,null,"Piping_Class_03",null,{"$f":"C29","v":"A-03-S-5H-Y(0)"},null,null,null,null,"Piping_Class_04",null,{"$f":"AC25","v":0},null,null,null,"Piping_Class_05"]
[null,null,null,null,"SEAT","DN\n(mm)","Dext\n(mm)","e\n(mm)","Din\n(mm)","dim",null,"DN\n(mm)","Dext\n(mm)","e\n(mm)","Din\n(mm)","dim",null,"DN\n(inch)","Dext\n(mm)","e\n(mm)","Din\n(mm)","dim","SCHEDULE",null,"DN\n(inch)","Dext\n(mm)","e\n(mm)","Din\n(mm)","dim","SCHEDULE",null,"DN\n(mm)","Dext\n(mm)","e\n(mm)","Din\n(mm)","dim"]
[null,null,"DN06","1/8\"",6,"6OD",6,1,{"$f":"G34-H34*2","v":4},{"$f":"CONCATENATE(G34,\"x\",H34)","v":"6x1"},null,"6OD",6,1,{"$f":"M34-N34*2","v":4},{"$f":"CONCATENATE(M34,\"x\",N34)","v":"6x1"},null,"1/8\"",10.3,1.65,{"$f":"+S34-2*T34","v":7.0000000000000009},{"$f":"CONCATENATE(S34,\"x\",T34)","v":"10.3x1.65"},10,null,"1/8\"",10.3,1.65,{"$f":"+Z34-2*AA34","v":7.0000000000000009},{"$f":"CONCATENATE(Z34,\"x\",AA34)","v":"10.3x1.65"},10,null,"6OD",6,1,{"$f":"AG34-AH34*2","v":4},{"$f":"CONCATENATE(AG34,\"x\",AH34)","v":"6x1"}]
[null,8,"DN08","1/4\"",8,"DN08",13.5,1.6,{"$f":"G35-H35*2","v":10.3},{"$f":"CONCATENATE(G35,\"x\",H35,\"mm\")","v":"13.5x1.6mm"},null,"DN08",13.5,1.6,{"$f":"M35-N35*2","v":10.3},{"$f":"CONCATENATE(M35,\"x\",N35,\"mm\")","v":"13.5x1.6mm"},null,"1/4\"",13.7,1.65,{"$f":"+S35-2*T35","v":10.399999999999999},{"$f":"CONCATENATE(S35,\"x\",T35,\"mm\")","v":"13.7x1.65mm"},10,null,"1/4\"",13.7,1.65,{"$f":"+Z35-2*AA35","v":10.399999999999999},{"$f":"CONCATENATE(Z35,\"x\",AA35,\"mm\")","v":"13.7x1.65mm"},10,null,"DN08",13.5,1.6,{"$f":"AG35-AH35*2","v":10.3},{"$f":"CONCATENATE(AG35,\"x\",AH35,\"mm\")","v":"13.5x1.6mm"}]
[null,10,"DN10","3/8\"",10,"DN10",17.2,1.6,14,{"$f":"CONCATENATE(G36,\"x\",H36,\"mm\")","v":"17.2x1.6mm"},null,"DN10",17.2,1.6,14,{"$f":"CONCATENATE(M36,\"x\",N36,\"mm\")","v":"17.2x1.6mm"},null,"3/8\"",17.149999999999999,1.65,13.849999999999998,{"$f":"CONCATENATE(S36,\"x\",T36,\"mm\")","v":"17.15x1.65mm"},10,null,"3/8\"",17.149999999999999,1.65,13.849999999999998,{"$f":"CONCATENATE(Z36,\"x\",AA36,\"mm\")","v":"17.15x1.65mm"},10,null,"DN10",17.2,1.6,{"$f":"AG36-AH36*2","v":14},{"$f":"CONCATENATE(AG36,\"x\",AH36,\"mm\")","v":"17.2x1.6mm"}]
[null,15,"DN15","1/2\"",15,"DN15",21.3,1.6,18.100000000000001,"21.3x1.6mm",null,"DN15",21.3,1.6,18.100000000000001,"21.3x1.6mm",null,"1/2\"",21.34,1.65,18.04,"21.34x1.65mm",5,null,"1/2\"",21.34,1.65,18.04,"21.34x1.65mm",5,null,"DN15",21.3,1.6,18.100000000000001,"21.3x1.6mm"]
[null,20,"DN20","3/4\"",20,"DN20",26.9,1.6,23.7,"26.9x1.6mm",null,"DN20",26.9,1.6,23.7,"26.9x1.6mm",null,"3/4\"",26.67,1.65,23.37,"26.67x1.65mm",5,null,"3/4\"",26.67,1.65,23.37,"26.67x1.65mm",5,null,"DN20",26.9,1.6,23.7,"26.9x1.6mm"]
[null,25,"DN25","1\"",25,"DN25",33.700000000000003,1.6,30.5,"33.7x1.6mm",null,"DN25",33.700000000000003,1.6,30.5,"33.7x1.6mm",null,"1\"",33.4,2.77,27.86,"33.4x2.77mm",5,null,"1\"",33.4,2.77,27.86,"33.4x2.77mm",5,null,"DN25",33.700000000000003,1.6,30.500000000000004,"33.7x1.6mm"]
[null,32,"DN32","1\"1/4",32,"DN32",42.4,1.6,39.200000000000003,"42.4x1.6mm",null,"DN32",42.4,1.6,39.200000000000003,"42.4x1.6mm",null,"1\"1/4",42.16,2.77,36.619999999999997,"42.16x2.77mm",10,null,"1\"1/4",42.16,2.77,36.619999999999997,"42.16x2.77mm",10,null,"DN32",42.4,1.6,39.199999999999996,"42.4x1.6mm"]
[null,40,"DN40","1\"1/2",40,"DN40",48.3,1.6,45.1,"48.3x1.6mm",null,"DN40",48.3,1.6,45.1,"48.3x1.6mm",null,"1\"1/2",48.26,2.77,42.72,"48.26x2.77mm",10,null,"1\"1/2",48.26,2.77,42.72,"48.26x2.77mm",10,null,"DN40",48.3,1.6,45.099999999999994,"48.3x1.6mm"]
[null,50,"DN50","2\"",50,"DN50",60.3,1.6,57.1,"60.3x1.6mm",null,"DN50",60.3,2,57.1,"60.3x2mm",null,"2\"",60.3,2.77,54.76,"60.3x2.77mm",10,null,"2\"",60.3,2.77,54.76,"60.3x2.77mm",10,null,"DN50",60.3,1.6,57.099999999999994,"60.3x1.6mm"]
[null,65,"DN65","2\"1/2",65,"DN65",76.099999999999994,1.6,72.900000000000006,"76.1x1.6mm",null,"DN65",76.099999999999994,2.9,72.900000000000006,"76.1x2.9mm",null,"2\"1/2",73.03,3.05,66.930000000000007,"73.03x3.05mm",10,null,"2\"1/2",73.03,3.05,66.930000000000007,"73.03x3.05mm",10,null,"DN65",76.099999999999994,2,72.099999999999994,"76.1x2mm"]
[null,80,"DN80","3\"",80,"DN80",86.9,1.6,83.7,"86.9x1.6mm",null,"DN80",86.9,3.05,83.7,"86.9x3.05mm",null,"3\"",88.9,3.05,82.800000000000011,"88.9x3.05mm",10,null,"3\"",88.9,3.05,82.800000000000011,"88.9x3.05mm",10,null,"DN80",86.9,2,82.9,"86.9x2mm"]
[null,100,"DN100","4\"",100,"DN100",114.3,2,111.1,"114.3x2mm",null,"DN100",114.3,6.02,111.1,"114.3x6.02mm",null,"4\"",114.3,3.05,108.2,"114.3x3.05mm",10,null,"4\"",114.3,3.05,108.2,"114.3x3.05mm",10,null,"DN100",114.3,2,110.3,"114.3x2mm"]
[null,125,"DN125","5\"",125,"DN125",null,null,null,null,null,null,null,null,null,null,null,"5\"",141.30000000000001,3.4,{"$f":"+S46-2*T46","v":134.5},{"$f":"CONCATENATE(S46,\"x\",T46,\"mm\")","v":"141.3x3.4mm"},10,null,"5\"",141.30000000000001,3.4,134.5,"141.3x3.4mm",10,null,"DN125",139.69999999999999,2,135.69999999999999,"139.7x2mm"]
[null,150,"DN150","6\"",150,"DN150",null,null,null,null,null,null,null,null,null,null,null,"6\"",168.3,3.4,161.5,"168.3x3.4mm",10,null,"6\"",168.3,3.4,161.5,"168.3x3.4mm",10,null,"DN150",168.3,2,164.3,"168.3x2mm"]
[null,200,"DN200","8\"",200,"DN200",null,null,null,null,null,null,null,null,null,null,null,"8\"",219.1,3.76,211.57999999999998,"219.1x3.76mm",10,null,"8\"",219.1,3.76,211.57999999999998,"219.1x3.76mm",10,null,"DN200",219.1,2,215.1,"219.1x2mm"]
[null,250,"DN250","10\"",250,"DN250",null,null,null,null,null,null,null,null,null,null,null,"10\"",273,4.1900000000000004,264.62,"273x4.19mm",10,null,"10\"",273,4.1900000000000004,264.62,"273x4.19mm",10,null,"DN250",273,3,267,"273x3mm"]
[null,300,"DN300","12\"",300,"DN300",null,null,null,null,null,null,null,null,null,null,null,"12\"",323.89999999999998,4.57,314.76,"323.9x4.57mm",10,null,"12\"",323.89999999999998,4.57,314.76,"323.9x4.57mm",10,null,"DN300",323.89999999999998,3,317.89999999999998,"323.9x3mm"]
[null,350,"DN350","14\"",null,null,null,null,null,null,null,null,null,null,null,null,null,"14\"",355.6,4.7699999999999996,346.06,"355.6x4.77mm",10,null,"14\"",355.6,4.7699999999999996,346.06,"355.6x4.77mm",10]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Cv Estimation Regulation Globe Valve"]
[]
[]
[null,"DN",0.5,{"$f":"3/4","v":0.75},1,1.25,1.5,2,2.5,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24]
[null,"KV",9.1999999999999993,8.5,7.8,7.5,7.1,6.5,6.1,6.1,5.8,5.8,5.0999999999999996,5.0999999999999996,4.8,4.8,4.8,4.8,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996]
[]
[null,null,"d",0.5,"inches",null,null,null,"d",1,"inches"]
[null,null,"K",{"$f":"HLOOKUP(D69,C66:AE67,2,FALSE)","v":9.1999999999999993},null,null,null,null,"K",7.0000000000000007E-2]
[null,null,"Cv",{"$f":"29.9*D69^2/D70^0.5","v":2.4644345193167538},null,null,null,null,"Cv",{"$f":"29.9*J69^2/J70^0.5","v":113.01137742975892},null,null,"K=894,01*d^4/Cv^2"]
[null,null,"Pourcentage min",0.1,null,null,null,null,"Pourcentage min",0.1]
[null,null,"Cvmax",{"$f":"D72*D71","v":0.24644345193167538},null,null,null,null,"Cvmax",{"$f":"J72*J71","v":11.301137742975893}]
[null,null,"Pourcentage max",0.95,null,null,null,null,"Pourcentage max",0.95]
[null,null,"Cvmax",{"$f":"D74*D71","v":2.3412127933509161},null,null,null,null,"Cvmax",{"$f":"J74*J71","v":107.36080855827097}]
[]
[]
[]
[null,"Manufacturer Data"]
[]
[null,null,null,"Coéfficient de débit Cv des vannes de régulation"]
[null,null,null,"VELAN","WEKA","FLOWSERVE","TRUCHOT"]
[null,null,"DN2",0.1,null,0.01]
[null,null,"DN4",0.3,null,0.28999999999999998]
[null,null,"DN6",1.3,1.1200000000000001,1.86]
[null,null,"DN8",2.1,2.4,1.86]
[null,null,"DN10",2.5,3.5,2.9,3.1]
[null,null,"DN15",5,7,{"$f":"E88*1.16","v":8.1199999999999992},7]
[null,null,"DN20",11,14,{"$f":"E89*1.16","v":16.239999999999998},15]
[null,null,"DN25",16.2,17.399999999999999,{"$f":"E90*1.16","v":20.183999999999997},18.5]
[null,null,"DN32",24,27.3,null,22]
[null,null,"DN40",46.4,58,46.4,35]
[null,null,"DN50",69.599999999999994,87,73.08,50]
[null,null,"DN65",120,116]
[null,null,"DN80",186,198,185.6]
[null,null,"DN100",250,302,290]
[null,null,"DN125",430,430]
[null,null,"DN150",null,650]
[null,null,"DN200"]
[null,null,"DN250"]
[]
[]
[null,null,"WEKA"]
[]
[]
[null,null,"CV max","vanne size",null,"CV max","vanne size",null,"CV max","vanne size",null,"- for a linear flow characteristic Kvs, min-max = ca. 1.1...1.3*Kv(calc)"]
[null,null,5.0000000000000001E-3,"DN2",null,0.5,"DN10",null,7.9,"DN25",null,"- for an equal-% flow characteristic Kvs, min-max = ca. 1.1...2.0*Kv(calc)"]
[null,null,8.0000000000000002E-3,"DN2",null,0.64,"DN10",null,9.1,"DN25",null,"- for a specific modified flow characteristic Kvs, min-max = ca. 1.1...1.6*Kv(calc)"]
[null,null,1.7000000000000001E-2,"DN2",null,0.73,"DN10",null,10.3,"DN25"]
[null,null,2.5999999999999999E-2,"DN2",null,1,"DN10",null,11.5,"DN25"]
[null,null,3.5000000000000003E-2,"DN2",null,1.2,"DN10",null,12.7,"DN25"]
[null,null,4.7E-2,"DN2",null,1.3,"DN10",null,15.8,"DN25"]
[null,null,5.8000000000000003E-2,"DN2",null,1.6,"DN10",null,16,"DN25",null,null,"ON/OFF VALVES"]
[null,null,7.0000000000000007E-2,"DN2",null,2.1,"DN10",null,16.5,"DN25"]
[null,null,8.1000000000000003E-2,"DN2",null,2.7,"DN10",null,16.8,"DN25",null,null,1.39,"DN6"]
[null,null,0.06,"DN4",null,3.3,"DN10",null,17.100000000000001,"DN25",null,null,2.44,"DN8"]
[null,null,0.09,"DN4",null,1.2,"DN15",null,13.1,"DN32",null,null,3.5,"DN10"]
[null,null,0.12,"DN4",null,1.7,"DN15",null,14.7,"DN32",null,null,7,"DN15"]
[null,null,0.2,"DN4",null,2.7,"DN15",null,16.2,"DN32",null,null,14,"DN20"]
[null,null,0.28999999999999998,"DN4",null,3.6,"DN15",null,17.600000000000001,"DN32",null,null,17.399999999999999,"DN25"]
[null,null,0.38,"DN4",null,4.7,"DN15",null,19.100000000000001,"DN32",null,null,27.3,"DN32"]
[null,null,0.52,"DN4",null,5.8,"DN15",null,23.6,"DN32",null,null,58,"DN40"]
[null,null,0.7,"DN4",null,5.9,"DN15",null,24,"DN32"]
[null,null,0.14000000000000001,"DN6",null,6.2,"DN15",null,24.5,"DN32"]
[null,null,0.17,"DN6",null,6.5,"DN15",null,24.9,"DN32"]
[null,null,0.23,"DN6",null,6.7,"DN15",null,25.3,"DN32"]
[null,null,0.28999999999999998,"DN6",null,6.2,"DN20",null,24,"DN40"]
[null,null,0.42,"DN6",null,6.3,"DN20",null,{"$f":"22*1.16","v":25.52},"DN40"]
[null,null,0.57999999999999996,"DN6",null,7,"DN20",null,28,"DN40"]
[null,null,0.65,"DN6",null,8.1,"DN20",null,{"$f":"27.6*1.16","v":32.015999999999998},"DN40"]
[null,null,0.8,"DN6",null,9.1999999999999993,"DN20",null,35,"DN40"]
[null,null,0.93,"DN6",null,10.7,"DN20",null,{"$f":"35*1.16","v":40.599999999999994},"DN40"]
[null,null,1.28,"DN6",null,11.4,"DN20",null,48,"DN40"]
[null,null,0.28999999999999998,"DN8",null,11.7,"DN20",null,49,"DN40"]
[null,null,0.87,"DN8",null,12.2,"DN20",null,50,"DN40"]
[null,null,1.28,"DN8",null,12.8,"DN20",null,51,"DN40"]
[null,null,1.63,"DN8",null,null,null,null,52,"DN40"]
[null,null,2.09,"DN8"]
[null,null,2.33,"DN8"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DN","Seat","BW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,2,"13.0x1,5",{"$f":"CONCATENATE(\"BW : \",R156)","v":"BW : 13.0x1,5"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,4,"13.0x1,5",{"$f":"CONCATENATE(\"BW : \",R157)","v":"BW : 13.0x1,5"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,6,"13.0x1,5","BW : 13.0x1,5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,8,"13.0x1,5","BW : 13.0x1,5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,10,"17.2x1.6","BW : 17.2x1.6"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,15,"21.3x2.0","BW : 21.3x2.0"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,20,"26.9x2.0","BW : 26.9x2.0"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,25,"33.7x2.0","BW : 33.7x2.0"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,32,32,"42.4x2.0","BW : 42.4x2.0"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"40-36",36,"48.3x2.0","BW : 48.3x2.0"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,40,40,"48.3x2.0","BW : 48.3x2.0"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,50,50,"60.3x2.0","BW : 60.3x2.0"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,65,65,"76.1x2.0","BW : 76.1x2.0"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,80,80,"88.9x2.0","BW : 88.9x2.0"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100,100,"114.3x2.6","BW : 114.3x2.6"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,125,120,"139.7x2.6","BW : 139.7x2.6"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,144,"168.3x2.6","BW : 168.3x2.6"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,200,190,"219.3x2.9","BW : 219.3x2.9"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,250,240,"273.0x3.2","BW : 273.0x3.2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,300,285,"323.9x3.2","BW : 323.9x3.2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,380,"406.4x4.8","BW : 406.4x4.8"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"As a general rule it is assumed that the min Kvs value by flow plug should be at 5...10% of the max rated Kvs value for the given valve size DN."]
[null,null,null,null,null,null,null,null,null,null,"="]
[null,null,null,null,null,null,null,null,null,null,"Cvmin = Cvmax/200"]
[]
[null,null,"VELAN"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NT13068",null,"rev A",null,"2004-06-13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vannes cryogéniques ACRG - ACRG Cryogenic valves"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DN","Seat diameter\n(mm)","Standard plug tolerances (mm)",null,"Minimal plug\nTolerances (mm)",null,"Standard seat tolerances (mm)",null,"Minimal Seat tolerances (mm)",null,"Standard\nRangeability","CV0*","Rmax pour CV\nmax",null,"Standard\nPlug/seat","Minimal\nPlug/seat","Section"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 - 15",6,0,-6.0000000000000001E-3,0,-4.0000000000000001E-3,0,0.01,0,6.0000000000000001E-3,100,6.0000000000000001E-3,239,null,{"$f":"AA216-W216","v":1.6E-2},{"$f":"AC216-Y216","v":0.01},null,{"$f":"AI216/AH216","v":0.625}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13,0,-0.01,0,-4.0000000000000001E-3,0,1.4999999999999999E-2,0,8.0000000000000002E-3,100,2.1000000000000001E-2,281,null,{"$f":"AA217-W217","v":2.5000000000000001E-2},{"$f":"AC217-Y217","v":1.2E-2},null,0.48]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 - 32",25,0,-1.2999999999999999E-2,0,-6.0000000000000001E-3,0,2.1000000000000001E-2,0,1.2E-2,100,6.2E-2,292,null,{"$f":"AA218-W218","v":3.4000000000000002E-2},1.8000000000000002E-2,null,0.52941176470588236]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"40 - 50",45,0,-1.6E-2,0,-8.0000000000000002E-3,0,2.5000000000000001E-2,0,1.4999999999999999E-2,100,0.21199999999999999,330,null,4.1000000000000002E-2,2.3E-2,null,0.5609756097560975]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,65,65,0,-1.9E-2,0,-8.0000000000000002E-3,0,0.03,0,0.02,100,0.33100000000000002,363,null,4.9000000000000002E-2,2.8000000000000001E-2,null,0.5714285714285714]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,80,92,0,-2.1999999999999999E-2,0,-1.2E-2,0,3.5000000000000003E-2,0,2.5000000000000001E-2,100,0.59899999999999998,311,null,5.7000000000000002E-2,3.7000000000000005E-2,null,0.64912280701754388]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100,116,0,-2.1999999999999999E-2,0,-1.7999999999999999E-2,0,3.5000000000000003E-2,0,0.03,100,0.85,318,null,5.7000000000000002E-2,4.8000000000000001E-2,null,0.84210526315789469]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125 - 150",140,0,-2.5000000000000001E-2,0,-0.02,0,0.04,0,0.03,100,1.57,382,null,6.5000000000000002E-2,0.05,null,0.76923076923076927]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,250,230,0,-2.9000000000000001E-2,0,-2.5000000000000001E-2,0,0.05,0,0.04,100,3.1819999999999999,377,null,7.9000000000000001E-2,6.5000000000000002E-2,null,0.82278481012658233]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CV0 = CV for 0% opening"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rmaxi = Cvplug / CV0"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* this value can be greatly reduced (rangeability increased) by fitting the plug with the seat"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"SPEED LIMITATIONS"]
[]
[]
[]
[null,null,"Fluid Type","Valve Type","Continuous duty","Infrequent duty","Pipe velocity"]
[null,null,"LIQUID","Globe, Eccentric","< or = 10 m/s","< or = 12 m/s","2 to 3 m/s"]
[null,null,null,"Ex-centred Butterfly","< or = 7 m/s","< or = 8,5 m/s"]
[null,null,null,"Centred Butterfly","< or = 7 m/s","< or = 8,5 m/s"]
[null,null,"Superheated STEAM"]
[null,null,null,"Butterfly","< 0,5 mach","< 0,7 mach"]
[null,null,"GAS","Globe, Eccentric","< 0,3 mach","< 0,5 mach"]
[null,null,null,"Butterfly","< 0,5 mach","< 0,7 mach"]
[]
[]
[null,null,"·          For water or fluids containing erosive particles, the speed is limited to 6 m/s."]
[null,null,"·          Gas speed is expressed in Mach, which is the ratio between the flow speed, and the sonic speed of the gas."]
[null,null,"·          For gas or steam, the flow velocity V (m/s) and the sound speed can be calculated with the equations:"]
[null,null,"Standard formula for fluid speed in the valve",null,null,"Formula for sound speed in a gas"]
[null,null,"V = 1,23 x (QxT) / (P2xD²)",null,null,"V = 91 x √ (K x T / M)"]
[null,null,"-      Q = volume flow rate (Nm3/h)",null,null,"-          K = ratio of specific heat"]
[null,null,"-      T = temperature (°K)",null,null,"-          M = molecular weight"]
[null,null,"-      P2 = downstream pressure (barabs)",null,null,"-          T = temperature °K"]
[null,null,"-      D = internal diameter of valve port (mm)"]
[]
[null,"EQUAL PERCENTAGE AND LINEAR - VALVES"]
[null,"(Extract from Weka documentation no. 20080118 Rev. June 2009 - FHo)"]
[]
[null,"- Kv:      SI units: Numerical value in m3/h of H 2 O at 5-40°C flowing through the valve at Δp=1bar"]
[null,"- Cv:      Customary US units: Numerical value in US gal/min of H2O at 60°F/16°C flowing through the valve at Δp=1psi"]
[null,"- Conversion: Cv=1.16*Kv or Kv=0.86*Cv"]
[]
[null,"d) Equal percentage flow characteristics (eq-%, = %):"]
[null,"The equal percentage flow characteristic is designed to linearize the installed flow characteristic in normal control valve applications, "]
[null,"where the amount of pressure drop available to the control valve decrease with the opening of the valve, due to the increase in "]
[null,"pressure losses in other parts of the system, such as pipes, pumps, heat exchanger etc. "]
[null,"However a control valve is always part of a real systems where pressure drop varies with losses in the process piping and the other "]
[null,"operating equipments in series with the control valve the resulting installed flow characteristic may by quit different. In any case where "]
[null,"process piping is attached to the valve, the piping pressure loss, a function of flow rate, will cause the valve pressure drop to vary as a "]
[null,"function of flow rate, even if the pressures at the source and receiver are constant."]
[null,"Values of an ideal inherent equal percentage flow characteristic:"]
[]
[null,"Expressed mathematically: Φ = Φo*e^(n/h)"]
[null,null,"- Φ = fraction of KV"]
[null,null,"- Φ(0) = lowest fraction of rated Kv (usually at h(0)) conform to the specific flow characteristic"]
[null,null,"- e = 2.7183, the base of the natural logarithms"]
[null,null,"- n = log(1/Φo)"]
[null,null,"- h = rated travel"]
[]
[null,"pressure losses in other parts of the system, such as pipes, pumps, heat exchanger etc. "]
[null,"An ideal inherent equal percentage flow characteristics would yield the same percentage of Kv-flow increase for each percentage "]
[null,"increment of travel. "]
[null,"Common are equal percentages flow characteristics of about 1:20 up to 1:50 in some special case up to 1:100."]
[null,"Values of an ideal inherent equal percentage flow characteristic:"]
[null,null,"For Φo =1:20=",{"$f":"1/20","v":0.05}]
[null,null,"h%",0,0.05,0.1,0.2,0.3,0.4,0.5,0.6,0.7,0.8,0.9,1]
[null,null,"Φ%",0.05,{"$f":"$D$293*EXP(1)^(LOG(1/$D$293,EXP(1))*E292)","v":5.8079317482077113E-2},6.7464142383678163E-2,9.1028210151304023E-2,0.12282280261157903,0.16572270086699936,0.22360679774997894,0.30170881682725814,0.40709053153690422,0.54928027165305893,0.7411344491069477,0.99999999999999989]
[null,null,"Increase is of about 35% over the previous Kv-value for each 10% increase in travel, for inherent rangeability 1:20."]
[null,null,"For Φo =1:50=",{"$f":"1/50","v":0.02}]
[null,null,"h%",0,0.05,0.1,0.2,0.3,0.4,0.5,0.6,0.7,0.8,0.9,1]
[null,null,"Φ%",0.02,{"$f":"$D$297*EXP(1)^(LOG(1/$D$297,EXP(1))*E296)","v":2.4320835813173149E-2},2.9575152732566275E-2,4.3734482957731129E-2,6.4672700657735741E-2,9.5635249979003717E-2,0.1414213562373095,0.20912791051825466,0.30924949471099167,0.45730505192732646,0.67624333780624146,0.99999999999999989]
[null,null,"Increase is of about 48% over the previous Kv-value for each 10% increase in travel, for inherent rangeability 1:50."]
[null,null,"For Φo =1:100=",{"$f":"1/100","v":0.01}]
[null,null,"h%",0,0.05,0.1,0.2,0.3,0.4,0.5,0.6,0.7,0.8,0.9,1]
[null,null,"Φ%",0.01,{"$f":"$D$301*EXP(1)^(LOG(1/$D$301,EXP(1))*E300)","v":1.2589254117941673E-2},1.5848931924611138E-2,2.5118864315095805E-2,3.9810717055349727E-2,6.3095734448019344E-2,0.10000000000000002,0.15848931924611137,0.25118864315095801,0.39810717055349754,0.63095734448019369,1.0000000000000004]
[null,null,"Increase is 58% over the previous Kv-value for each 10% increase in travel, for inherent rangeability 1:100."]
[]
[null,"e) Modified equal percentage flow characteristics (eq-% mod.,  = % mod.): e) Modified equal percentage flow characteristics (eq-% mod.,  = % mod.):"]
[]
[null,"Equal percentage flow plugs for WEKA control Valves are linear modified at the beginning of the vlave travel for an exact fine flow "]
[null,"control down to valve closing, see flow line schema following for further details."]
[null,"Values of the modified equal percentage inherent flow characteristic i.e. equal percentage, linear modified to zero:"]
[null,null,"For Φo =1:20=",{"$f":"1/20","v":0.05}]
[null,null,"h%",0,0.05,0.1,0.2,0.3,0.4,0.5,0.6,0.7,0.8,0.9,1]
[null,null,"Φ%",0,2.0500000000000001E-2,4.0899999999999999E-2,8.1900000000000001E-2,{"$f":"H293","v":0.12282280261157903},{"$f":"I293","v":0.16572270086699936},{"$f":"J293","v":0.22360679774997894},0.30170881682725814,0.40709053153690422,0.54928027165305893,0.7411344491069477,0.99999999999999989]
[null,null,"Until of about 30% travel linear, afterwards ideal eq-%, rangeability 1:20 as above "]
[null,null,"For Φo =50=",{"$f":"1/50","v":0.02}]
[null,null,"h%",0,0.05,0.1,0.2,0.3,0.4,0.5,0.6,0.7,0.8,0.9,1]
[null,null,"Φ%",0,1.0800000000000001E-2,2.1600000000000001E-2,4.3099999999999999E-2,{"$f":"H297","v":6.4672700657735741E-2},{"$f":"I297","v":9.5635249979003717E-2},0.1414213562373095,0.20912791051825466,0.30924949471099167,0.45730505192732646,0.67624333780624146,0.99999999999999989]
[null,null,"Until of about 20% travel linear, afterwards ideal eq-%, rangeability 1:50 as above "]
[null,null,"For Φo =100=",{"$f":"1/100","v":0.01}]
[null,null,"h%",0,0.05,0.1,0.2,0.3,0.4,0.5,0.6,0.7,0.8,0.9,1]
[null,null,"Φ%",0,6.3E-3,1.26E-2,2.5100000000000001E-2,{"$f":"H301","v":3.9810717055349727E-2},{"$f":"I301","v":6.3095734448019344E-2},0.10000000000000002,0.15848931924611137,0.25118864315095801,0.39810717055349754,0.63095734448019369,1.0000000000000004]
[null,null,"Until of about 15% travel linear, afterwards ideal eq-%, rangeability 1:100 as above "]
[null,null,null,null,null,null,{"$f":"D319+(H319-D317)/H318*G318","v":1.9873811370233155E-2}]
[null,null,null,null,null,null,{"$f":"G319/G318*F318","v":1.255E-2},{"$f":"H319/H318*G318","v":2.6540478036899819E-2},null,{"$f":"1/200","v":5.0000000000000001E-3}]
[null,"f) Linear flow characteristics (lin):"]
[]
[null,null,"Expressed mathematically: Φ = Φo  + m*h"]
[null,null,"- Φ = fraction of Kv "]
[null,null,"- m = the slope Φ versus travel, (Φ-Φo)/h"]
[null,null,"- h = rated travel"]
[]
[null,"If the pressure drop across the valve remains constant independent of the flow, the linear flow characteristic will be an optimal inherent "]
[null,"flow characteristic, because in that case the inherent flow characteristic equals in the installed flow characteristic. "]
[null,"In an ideal linear flow characteristics the Kv values increases by the same increment for each fraction of travel:"]
[null,"An ideal inherent linear flow characteristic:"]
[]
[null,null,"For Φo =0"]
[null,null,"h%",0,0.05,0.1,0.2,0.3,0.4,0.5,0.6,0.7,0.8,0.9,1]
[null,null,"Φ%",0,{"$f":"$D$337+E336","v":0.05},{"$f":"$D$337+F336","v":0.1},0.2,0.3,0.4,0.5,0.6,0.7,0.8,0.9,1]
[null,null,"Due to the exact tolerances for WEKA Control valves it is possible to assume Φ 0 =0!"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,82.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,77.930000000000007,null,88.9]
[null,null,"For Φo =0,01",{"$f":"1/100","v":0.01},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AB340-AB341","v":4.8699999999999903},null,{"$f":"77.93","v":77.930000000000007}]
[null,null,"h%",0,0.05,0.1,0.2,0.3,0.4,0.5,0.6,0.7,0.8,0.9,1,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AB342/2","v":2.4349999999999952},null,{"$f":"AD341-AD342","v":10.969999999999999}]
[null,null,"Φ%",0.01,0.06,0.109,0.20799999999999999,0.307,0.40600000000000003,0.505,0.60399999999999998,0.70299999999999996,0.80200000000000005,0.90100000000000002,{"$f":"$D$344+(O343-$D$344)/1*O343","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AD343/2","v":5.4849999999999994}]
[]
[null,"For Φo  = 0.01 ==>: Φ (%) =    1.00%      6.00%     10.90%    20.80%    30.70%    40.60%    50.50%    60.40%    70.30%    80.20%    90.10%      100%"]
[]
[]
[]
[]
[]
[]
[null,"As a general rule it is assumed that the min Kvs value by flow plug should be at 5...10% of the max rated Kvs value for the given valve size DN."]
[]
[null,null,null,null,"Linear","Generic 1:20\ncontrol valve","Generic 1:50\ncontrol valve","Generic 1:100\ncontrol valve","Generic 1:200\ncontrol valve","Weka 1:20\nControl Valve","Weka 1:50\nControl Valve","Weka 1:100\nControl Valve","Weka 1:200\nControl Valve"]
[null,"Valve_Range",null,"h (%)","F (%)","F (%)","F (%)","F (%)","F (%)",null,null,null,null,null,"Cv","Linear",null,"EQUAL PERCENTAGE"]
[null,"Linear","Linear",0,{"$f":"D357","v":0},{"$f":"1/20","v":0.05},{"$f":"1/50","v":0.02},0.01,{"$f":"1/200","v":5.0000000000000001E-3},{"$f":"[4]!Cv_From_Trim($D357,$B$358)","v":0},{"$f":"[4]!Cv_From_Trim($D357,$B$359)","v":0},{"$f":"[4]!Cv_From_Trim($D357,$B$360)","v":0},{"$f":"[4]!Cv_From_Trim($D357,$B$361)","v":0},null,null,"% OPEN","Cvmax","% OPEN","%Cv","Cvmax"]
[null,20,{"$f":"1/20","v":0.05},0.05,{"$f":"D358","v":0.05},{"$f":"$F$357*EXP(1)^(LOG(1/$F$357,EXP(1))*D358)","v":5.8079317482077113E-2},{"$f":"$G$357*EXP(1)^(LOG(1/$G$357,EXP(1))*D358)","v":2.4320835813173149E-2},{"$f":"$H$357*EXP(1)^(LOG(1/$H$357,EXP(1))*D358)","v":1.2589254117941673E-2},{"$f":"$I$357*EXP(1)^(LN(1/$I$357)*E358)","v":6.5166066028153171E-3},{"$f":"[4]!Cv_From_Trim($D358,$B$358)","v":3.3732071191839082E-2},{"$f":"[4]!Cv_From_Trim($D358,$B$359)","v":1.4787576366283138E-2},{"$f":"[4]!Cv_From_Trim($D358,$B$360)","v":7.9244659623055689E-3},{"$f":"[4]!Cv_From_Trim($D358,$B$361)","v":4.2466161615856181E-3},null,0.26910653187996919,0.8,0.33638316484996145,0.52,0.10964781961431853,2.454280740160085]
[null,50,{"$f":"1/50","v":0.02},0.1,0.1,{"$f":"$F$357*EXP(1)^(LOG(1/$F$357,EXP(1))*D359)","v":6.7464142383678163E-2},{"$f":"$G$357*EXP(1)^(LOG(1/$G$357,EXP(1))*D359)","v":2.9575152732566275E-2},1.5848931924611138E-2,{"$f":"$I$357*EXP(1)^(LN(1/$I$357)*E359)","v":8.4932323231712362E-3},{"$f":"[4]!Cv_From_Trim($D359,$B$358)","v":6.7464142383678163E-2},{"$f":"[4]!Cv_From_Trim($D359,$B$359)","v":2.9575152732566275E-2},{"$f":"[4]!Cv_From_Trim($D359,$B$360)","v":1.5848931924611138E-2},{"$f":"[4]!Cv_From_Trim($D359,$B$361)","v":8.4932323231712362E-3},null,0.12524710804170122,0.37233465027170959,null,0.35392173374773789,5.1032103211440978E-2]
[null,100,{"$f":"1/100","v":0.01},0.15,0.15,7.8365426883153982E-2,3.596462168791318E-2,1.9952623149688799E-2,1.1069410767284429E-2,{"$f":"[4]!Cv_From_Trim($D360,$B$358)","v":7.8365426883153982E-2},{"$f":"[4]!Cv_From_Trim($D360,$B$359)","v":3.596462168791318E-2},{"$f":"[4]!Cv_From_Trim($D360,$B$360)","v":1.9952623149688795E-2},{"$f":"[4]!Cv_From_Trim($D360,$B$361)","v":1.1069410767284429E-2},null,4.0397445154585911E-2,0.12009354027156671,null,0.10821483035592878,1.6459993550677055E-2]
[null,200,{"$f":"1/200","v":5.0000000000000001E-3},0.2,0.2,9.1028210151304023E-2,4.3734482957731129E-2,2.5118864315095805E-2,1.4426999059072134E-2,{"$f":"[4]!Cv_From_Trim($D361,$B$358)","v":9.1028210151304023E-2},{"$f":"[4]!Cv_From_Trim($D361,$B$359)","v":4.3734482957731129E-2},{"$f":"[4]!Cv_From_Trim($D361,$B$360)","v":2.5118864315095805E-2},{"$f":"[4]!Cv_From_Trim($D361,$B$361)","v":1.4426999059072134E-2},null,4.0397445154585911E-2,0.12009354027156671,null,0.10821483035592878,1.6459993550677055E-2]
[null,null,null,0.25,0.25,0.10573712634405641,5.3182958969449884E-2,3.1622776601683798E-2,1.8803015465431967E-2,{"$f":"[4]!Cv_From_Trim($D362,$B$358)","v":0.10573712634405641},{"$f":"[4]!Cv_From_Trim($D362,$B$359)","v":5.3182958969449884E-2},{"$f":"[4]!Cv_From_Trim($D362,$B$360)","v":3.1622776601683798E-2},{"$f":"[4]!Cv_From_Trim($D362,$B$361)","v":1.8803015465431967E-2}]
[null,null,null,0.3,0.3,0.12282280261157903,6.4672700657735741E-2,3.9810717055349727E-2,2.4506370946974491E-2,{"$f":"[4]!Cv_From_Trim($D363,$B$358)","v":0.12282280261157903},{"$f":"[4]!Cv_From_Trim($D363,$B$359)","v":6.4672700657735741E-2},{"$f":"[4]!Cv_From_Trim($D363,$B$360)","v":3.981071705534972E-2},{"$f":"[4]!Cv_From_Trim($D363,$B$361)","v":2.4506370946974491E-2}]
[null,null,null,0.35,0.35,0.14266929093832778,7.8644706714564291E-2,5.0118723362727227E-2,3.1939675744819082E-2,{"$f":"[4]!Cv_From_Trim($D364,$B$358)","v":0.14266929093832775},{"$f":"[4]!Cv_From_Trim($D364,$B$359)","v":7.8644706714564291E-2},{"$f":"[4]!Cv_From_Trim($D364,$B$360)","v":5.011872336272722E-2},{"$f":"[4]!Cv_From_Trim($D364,$B$361)","v":3.1939675744819075E-2}]
[null,null,null,0.4,0.4,0.16572270086699936,9.5635249979003717E-2,6.3095734448019344E-2,4.1627660370093661E-2,{"$f":"[4]!Cv_From_Trim($D365,$B$358)","v":0.16572270086699933},{"$f":"[4]!Cv_From_Trim($D365,$B$359)","v":9.5635249979003703E-2},{"$f":"[4]!Cv_From_Trim($D365,$B$360)","v":6.3095734448019344E-2},{"$f":"[4]!Cv_From_Trim($D365,$B$361)","v":4.1627660370093647E-2}]
[null,null,null,0.45,0.45,0.19250122715283502,0.11629646063455598,7.943282347242818E-2,5.4254217285501158E-2,{"$f":"[4]!Cv_From_Trim($D366,$B$358)","v":0.19250122715283502},{"$f":"[4]!Cv_From_Trim($D366,$B$359)","v":0.11629646063455598},{"$f":"[4]!Cv_From_Trim($D366,$B$360)","v":7.9432823472428166E-2},{"$f":"[4]!Cv_From_Trim($D366,$B$361)","v":5.4254217285501144E-2}]
[null,null,null,0.5,0.5,0.22360679774997894,0.1414213562373095,0.10000000000000002,7.0710678118654738E-2,{"$f":"[4]!Cv_From_Trim($D367,$B$358)","v":0.22360679774997894},{"$f":"[4]!Cv_From_Trim($D367,$B$359)","v":0.14142135623730948},{"$f":"[4]!Cv_From_Trim($D367,$B$360)","v":0.10000000000000002},{"$f":"[4]!Cv_From_Trim($D367,$B$361)","v":7.0710678118654724E-2}]
[null,null,null,0.55000000000000004,0.55000000000000004,0.25973860395343273,0.17197427927619377,0.12589254117941681,9.2158734383514837E-2,{"$f":"[4]!Cv_From_Trim($D368,$B$358)","v":0.25973860395343273},{"$f":"[4]!Cv_From_Trim($D368,$B$359)","v":0.17197427927619374},{"$f":"[4]!Cv_From_Trim($D368,$B$360)","v":0.12589254117941678},{"$f":"[4]!Cv_From_Trim($D368,$B$361)","v":9.2158734383514823E-2}]
[null,null,null,0.6,0.6,0.30170881682725814,0.20912791051825466,0.15848931924611137,0.12011244339814309,{"$f":"[4]!Cv_From_Trim($D369,$B$358)","v":0.30170881682725814},{"$f":"[4]!Cv_From_Trim($D369,$B$359)","v":0.20912791051825463},{"$f":"[4]!Cv_From_Trim($D369,$B$360)","v":0.15848931924611134},{"$f":"[4]!Cv_From_Trim($D369,$B$361)","v":0.12011244339814306}]
[null,null,null,0.65,0.65,0.3504608431930436,0.25430827878332185,0.19952623149688806,0.1565451083457241,{"$f":"[4]!Cv_From_Trim($D370,$B$358)","v":0.35046084319304355},{"$f":"[4]!Cv_From_Trim($D370,$B$359)","v":0.2543082787833218},{"$f":"[4]!Cv_From_Trim($D370,$B$360)","v":0.199526231496888},{"$f":"[4]!Cv_From_Trim($D370,$B$361)","v":0.15654510834572408}]
[null,null,null,0.7,0.7,0.40709053153690422,0.30924949471099167,0.25118864315095801,0.20402857733683685,{"$f":"[4]!Cv_From_Trim($D371,$B$358)","v":0.40709053153690422},{"$f":"[4]!Cv_From_Trim($D371,$B$359)","v":0.30924949471099167},{"$f":"[4]!Cv_From_Trim($D371,$B$360)","v":0.25118864315095796},{"$f":"[4]!Cv_From_Trim($D371,$B$361)","v":0.20402857733683682}]
[null,null,null,0.75,0.75,0.47287080450158792,0.37606030930863932,0.31622776601683805,0.26591479484724928,{"$f":"[4]!Cv_From_Trim($D372,$B$358)","v":0.47287080450158786},{"$f":"[4]!Cv_From_Trim($D372,$B$359)","v":0.37606030930863926},{"$f":"[4]!Cv_From_Trim($D372,$B$360)","v":0.31622776601683794},{"$f":"[4]!Cv_From_Trim($D372,$B$361)","v":0.26591479484724923}]
[null,null,null,0.8,0.8,0.54928027165305893,0.45730505192732646,0.39810717055349754,0.34657242157757318,{"$f":"[4]!Cv_From_Trim($D373,$B$358)","v":0.54928027165305882},{"$f":"[4]!Cv_From_Trim($D373,$B$359)","v":0.45730505192732634},{"$f":"[4]!Cv_From_Trim($D373,$B$360)","v":0.39810717055349748},{"$f":"[4]!Cv_From_Trim($D373,$B$361)","v":0.34657242157757312}]
[null,null,null,0.85,0.85,0.63803646567959138,0.556102054222956,0.50118723362727235,0.4516952261612211,{"$f":"[4]!Cv_From_Trim($D374,$B$358)","v":0.63803646567959138},{"$f":"[4]!Cv_From_Trim($D374,$B$359)","v":0.55610205422295589},{"$f":"[4]!Cv_From_Trim($D374,$B$360)","v":0.50118723362727235},{"$f":"[4]!Cv_From_Trim($D374,$B$361)","v":0.45169522616122104}]
[null,null,null,0.9,0.9,0.7411344491069477,0.67624333780624146,0.63095734448019369,0.58870401865247457,{"$f":"[4]!Cv_From_Trim($D375,$B$358)","v":0.74113444910694759},{"$f":"[4]!Cv_From_Trim($D375,$B$359)","v":0.67624333780624124},{"$f":"[4]!Cv_From_Trim($D375,$B$360)","v":0.63095734448019347},{"$f":"[4]!Cv_From_Trim($D375,$B$361)","v":0.58870401865247435}]
[null,null,null,0.95,0.95,0.86089165933173462,0.82234015942688876,0.79432823472428193,0.76727049901092503,{"$f":"[4]!Cv_From_Trim($D376,$B$358)","v":0.86089165933173462},{"$f":"[4]!Cv_From_Trim($D376,$B$359)","v":0.82234015942688854},{"$f":"[4]!Cv_From_Trim($D376,$B$360)","v":0.79432823472428171},{"$f":"[4]!Cv_From_Trim($D376,$B$361)","v":0.7672704990109247}]
[null,null,null,1,1,0.99999999999999989,0.99999999999999989,1.0000000000000004,0.99999999999999956,{"$f":"[4]!Cv_From_Trim($D377,$B$358)","v":0.99999999999999967},{"$f":"[4]!Cv_From_Trim($D377,$B$359)","v":0.99999999999999978},{"$f":"[4]!Cv_From_Trim($D377,$B$360)","v":1.0000000000000002},{"$f":"[4]!Cv_From_Trim($D377,$B$361)","v":0.99999999999999933}]
[]
[]
[null,null,null,null,null,null,null,"=$H$357*EXP(1)^(LOG(1/$H$357;EXP(1))*D361)"]
[null,null,null,null,null,null,null,null,{"$f":"EXP(1)","v":2.7182818284590451}]
[]
[]
[]
[null,null,null,null,null,null,null,null,{"$f":"LOG(5,EXP(1))","v":1.6094379124341003}]
[null,null,null,null,null,null,null,null,{"$f":"EXP(3*LN(5))","v":124.99999999999994}]
[null,null,null,null,null,null,null,null,{"$f":"5*EXP(3)","v":100.42768461593835}]

{"sheet":"Fluides","index":2,"n_rows":75,"n_cols":11,"rows_kept":75,"cut":false,"hidden":false,"merged":[]}
[null,null,"Liste des fluides disponibles"]
[1,1,"Ammoniac","C:\\Program files\\GaspakDemo5\\NH379.gas",null,null,null,1]
[2,2,"Argon","C:\\Program files\\GaspakDemo5\\ARGON83.gas",null,null,null,2]
[3,21,"Azote","C:\\Program files\\GaspakDemo5\\N273.gas",null,null,null,21]
[4,22,"Azote","C:\\Program files\\GaspakDemo5\\N286.gas",null,null,null,22]
[5,4,"Butane Normal","C:\\Program files\\GaspakDemo5\\NORB86.gas",null,null,null,4]
[6,7,"Deutérium","C:\\Program files\\GaspakDemo5\\D286.gas",null,null,null,7]
[7,5,"Dioxide de carbone","C:\\Program files\\GaspakDemo5\\CO289.gas",null,null,null,5]
[8,27,"Eau","C:\\Program files\\GaspakDemo5\\H2O89.gas",null,null,null,27]
[9,8,"Ethane","C:\\Program files\\GaspakDemo5\\C2H686.gas",null,null,null,8]
[10,9,"Ethylène","C:\\Program files\\GaspakDemo5\\C2H481.gas",null,null,null,9]
[11,10,"Ethylène","C:\\Program files\\GaspakDemo5\\C2H486.gas",null,null,null,10,null,1,"Ammonia"]
[12,11,"Helium","C:\\Program files\\GaspakDemo5\\HE89.gas",null,null,null,11]
[13,16,"Hydrogen Sulfide","C:\\Program files\\GaspakDemo5\\H2S93.gas",null,null,null,16,null,18]
[14,3,"Isobutane","C:\\Program files\\GaspakDemo5\\ISOB86.gas",null,null,null,3,null,"Neon"]
[15,17,"Krypton","C:\\Program files\\GaspakDemo5\\KR90.gas",null,null,null,17,null,2]
[16,18,"Méthane","C:\\Program files\\GaspakDemo5\\METH86.gas",null,null,null,18,null,"Argon"]
[17,19,"Méthane","C:\\Program files\\GaspakDemo5\\CH489.gas",null,null,null,19,null,19]
[18,6,"Monoxide de carbone","C:\\Program files\\GaspakDemo5\\CO85.gas",null,null,null,6,null,"Nitrogen"]
[19,20,"Néon","C:\\Program files\\GaspakDemo5\\NE91.gas",null,null,null,20,null,3]
[20,23,"Nitrogene Trifluoride","C:\\Program files\\GaspakDemo5\\NF380.gas",null,null,null,23,null,"iso-Butane"]
[21,13,"Normal Hydrogene","C:\\Program files\\GaspakDemo5\\NH291.gas",null,null,null,13,null,20]
[22,24,"Oxygène","C:\\Program files\\GaspakDemo5\\O278.gas",null,null,null,24,null,"Nitrogen Trifluoride"]
[23,25,"Oxygène","C:\\Program files\\GaspakDemo5\\O285.gas",null,null,null,25,null,4]
[24,15,"ParaHydrogène","C:\\Program files\\GaspakDemo5\\PH275.gas",null,null,null,15,null,"n-Butane"]
[25,26,"Propane","C:\\Program files\\GaspakDemo5\\C3H886.gas",null,null,null,26,null,21]
[26,29,"R11","C:\\Program files\\GaspakDemo5\\R1191.gas",null,null,null,29,null,"Oxygen"]
[27,30,"R12","C:\\Program files\\GaspakDemo5\\R1291.gas",null,null,null,30,null,5]
[28,33,"R123","C:\\Program files\\GaspakDemo5\\R123N93.gas",null,null,null,33,null,"Carbon Dioxide"]
[29,34,"R124","C:\\Program files\\GaspakDemo5\\R124N93.gas",null,null,null,34,null,22]
[30,35,"R125","C:\\Program files\\GaspakDemo5\\R125N93.gas",null,null,null,35,null,"Propane"]
[31,36,"R134","C:\\Program files\\GaspakDemo5\\R134AN92.gas",null,null,null,36,null,6]
[32,37,"R134","C:\\Program files\\GaspakDemo5\\R134AT93.gas",null,null,null,37,null,"Carbon Monoxide"]
[33,38,"R152","C:\\Program files\\GaspakDemo5\\R152AT94.gas",null,null,null,38,null,23]
[34,31,"R22","C:\\Program files\\GaspakDemo5\\R2291.gas",null,null,null,31,null,"Water"]
[35,32,"R32","C:\\Program files\\GaspakDemo5\\R32N93.gas",null,null,null,32,null,7]
[36,50,"R32","C:\\Program files\\GaspakDemo5\\R32N94.gas",null,null,null,50,null,"Deuterium"]
[37,28,"Xénon","C:\\Program files\\GaspakDemo5\\\\XE90.gas",null,null,null,28,null,24]
[38,"Phosphine",1.45,10.6,null,null,null,null,null,"Xenon"]
[39,"Protoxyde d'azote",1.8720000000000001,13.6,null,null,null,null,null,8]
[40,"R11 gaz",6.2,10.16,null,null,null,null,null,"Ethane"]
[41,"R12 gaz",5.75,11.99,null,null,null,null,null,25]
[42,"R22 gaz",4.2300000000000004,11.8,null,null,null,null,null,"Refrigerant-11"]
[43,"Silane",1.36,10.8,null,null,null,null,null,9]
[44,"Sulfure d'hydrogène",1.45,11.79,null,null,null,null,null,"Ethylene"]
[45,"R11 liq",1500,567.5,null,null,null,null,null,26]
[46,"R12 liq",1350,260,null,null,null,null,null,"Refrigerant-12"]
[47,"R22 liq",1250,210,null,null,null,null,null,10]
[48,"R32 liq",1000,193.2,null,null,null,null,null,"Helium-4"]
[49,"R123 liq",1500,569.6,null,null,null,null,null,27]
[50,"R124 liq",1400,346,null,null,null,null,null,"Refrigerant-22"]
[51,"R125 liq",1250,205,null,null,null,null,null,11]
[52,"R152a liq",950,214,null,null,null,null,null,"equil Hydrogen"]
[null,null,null,null,null,null,null,null,null,28]
[null,null,null,null,null,null,null,null,null,"Refrigerant-32"]
[null,null,null,null,null,null,null,null,null,12]
[null,null,null,null,null,null,null,null,null,"normal Hydrogen"]
[null,null,null,null,null,null,null,null,null,29]
[null,null,null,null,null,null,null,null,null,"Refrigerant-123"]
[null,null,null,null,null,null,null,null,null,13]
[null,null,null,null,null,null,null,null,null,"ortho Hydrogen"]
[null,null,null,null,null,null,null,null,null,30]
[null,null,null,null,null,null,null,null,null,"Refrigerant-124"]
[null,null,null,null,null,null,null,null,null,14]
[null,null,null,null,null,null,null,null,null,"para Hydrogen"]
[null,null,null,null,null,null,null,null,null,31]
[null,null,null,null,null,null,null,null,null,"Refrigerant-125"]
[null,null,null,null,null,null,null,null,null,15]
[null,null,null,null,null,null,null,null,null,"Hydrogen Sulfide"]
[null,null,null,null,null,null,null,null,null,32]
[null,null,null,null,null,null,null,null,null,"Refrigerant-134A"]
[null,null,null,null,null,null,null,null,null,16]
[null,null,null,null,null,null,null,null,null,"Krypton"]
[null,null,null,null,null,null,null,null,null,33]
[null,null,null,null,null,null,null,null,null,"Refrigerant-152A"]

{"sheet":"Property GasPak","index":3,"n_rows":66,"n_cols":7,"rows_kept":66,"cut":false,"hidden":false,"merged":[[1,1,1,7]]}
[]
[null,"FluidProperties(Fluide;Entrée1;Valeur de E1;Entrée2;Valeur de E2;Sortie;Phase;Unités)"]
[null,"Fluide num. ",11,"-"]
[null,"Pression ",1,"Bars"]
[null,"Temperature (2)",77,"K"]
[null,"Pression (1)",{"$f":"C4*100000","v":100000},"Pa"]
[null,"Densité (3)",{"$f":"[2]!FluidProperties($C$3,1,$C$6,2,$C$5,3,0,1)","v":{"$error":"#NAME?"}},"kg/m3",null,16,{"$f":"[2]!FluidProperties($C$3,1,$C$4,2,$C$23-10,F7,0,1)","v":{"$error":"#NAME?"}}]
[null,"Enthalpie (5)",{"$f":"[2]!FluidProperties($C$3,1,$C$6,2,$C$5,5,0,1)/1000","v":{"$error":"#NAME?"}},"kJ/kg"]
[null,"Entropie (4)",{"$f":"[2]!FluidProperties($C$3,1,$C$6,2,$C$5,4,0,1)/1000","v":{"$error":"#NAME?"}},"kJ/kg-K"]
[null,"Energie Interne (6)",{"$f":"[2]!FluidProperties($C$3,1,$C$6,2,$C$5,6,0,1)/1000","v":{"$error":"#NAME?"}},"kJ/kg",null,12,{"$f":"[2]!FConstant(C3,F10)","v":{"$error":"#NAME?"}}]
[null,"Cp (10)",{"$f":"[2]!FluidProperties($C$3,1,$C$6,2,$C$5,10,0,1)/1000","v":{"$error":"#NAME?"}},"kJ/kg-K"]
[null,"Cv (9)",{"$f":"[2]!FluidProperties($C$3,1,$C$6,2,$C$5,9,0,1)/1000","v":{"$error":"#NAME?"}},"kJ/kg-K"]
[null,"g (11)",{"$f":"[2]!FluidProperties($C$3,1,$C$6,2,$C$5,11,0,1)","v":{"$error":"#NAME?"}},"--"]
[null,"Conductivité (22)",{"$f":"[2]!FluidProperties($C$3,1,$C$6,2,$C$5,22,0,1)","v":{"$error":"#NAME?"}},"W/m.K"]
[null,"Viscosité (21) ",{"$f":"[2]!FluidProperties($C$3,1,$C$6,2,$C$5,21,0,1)","v":{"$error":"#NAME?"}},"Pa.s"]
[null,"Vitesse du Son (15)",{"$f":"[2]!FluidProperties($C$3,1,$C$6,2,$C$5,15,0,1)","v":{"$error":"#NAME?"}},"m/s"]
[null,"Prandlt (24)",{"$f":"[2]!FluidProperties($C$3,1,$C$6,2,$C$5,24,0,1)","v":{"$error":"#NAME?"}},"--"]
[null,"Chaleur Latente (29)",{"$f":"[2]!FluidProperties($C$3,1,$C$6,10,$C$5,29,0,1)/1000","v":{"$error":"#NAME?"}},"kJ/kg"]
[null,"Z (20)",{"$f":"[2]!FluidProperties($C$3,1,$C$6,2,$C$5,20,0,1)","v":{"$error":"#NAME?"}},"--"]
[null,"Gas constant R (4)",{"$f":"[2]!FConstant(C3,4)","v":{"$error":"#NAME?"}},"--"]
[null,"Masse Molaire",{"$f":"C19*C7*C20*C5/C4/100000*1000","v":{"$error":"#NAME?"}},"g/mol"]
[null,"Sat P (1)",{"$f":"[2]!FluidProperties(C3,2,C5,10,0,1,2,1)/100000","v":{"$error":"#NAME?"}},"bars"]
[null,"Sat T (2)",{"$f":"[2]!FluidProperties(C3,1,C4*100000,10,0,2,2,1)","v":{"$error":"#NAME?"}},"K"]
[null,"V(dH/dV) à P=cste (17)",{"$f":"[2]!FluidProperties($C$3,1,$C$6,2,$C$5,17,0,1)/1000","v":{"$error":"#NAME?"}},"kJ/kg"]
[]
[]
[]
[]
[null,"Ammonia",1,"Pressure","Pressure upper limit"]
[null,"Argon",2,"Temperature","Temperature upper limit"]
[null,"Butane, Iso",3,"Density","Temperature lower limit"]
[null,"Butane, Normal",4,"Entropy","Gas constant \"R\""]
[null,"Carbon Dioxide",5,"Enthalpy","Critical pressure"]
[null,"Carbon Monoxide",6,"Internal energy","Critical temeprature"]
[null,"Deuterium",7,"dP/dD","Critical density"]
[null,"Ethane",8,"dP/dT","Triple point pressure"]
[null,"Ethylene",9,"Cv","Triple point temperature"]
[null,"Ethylene",10,"Cp","Triple point vapor density"]
[null,"Helium",11,"Gamma","Triple point liquid density"]
[null,"Hydrogen, Equilibrium",12,"Alpha","Molecular weight"]
[null,"Hydrogen, Normal",13,"Gruneisen","Pressure of the standard state"]
[null,"Hydrogen, Ortho",14,"Kt","Accentric factor"]
[null,"Hydrogen, Para",15,"Sound speed"]
[null,"Hydrogen Sulfide",16,"JT coefficient"]
[null,"Krypton",17,"(dH/dV)*V @ const P"]
[null,"Methane",18,"dH/dT @ const density"]
[null,"Methane",19,"dS/dT @ const density"]
[null,"Neon",20,"Z compressibility factor"]
[null,"Nitrogen",21,"Viscosity"]
[null,"Nitrogen",22,"Conductivity"]
[null,"Nitrogen Trifluoride",23,"Thermal diffusivity"]
[null,"Oxygen",24,"Prandtl number"]
[null,"Oxygen",25,"Surface tension"]
[null,"Propane",26,"Dielectric constant"]
[null,"Water",27,"PV/RT"]
[null,"Xenon",28,"dP/dT @ const sat"]
[null,"R-11",29,"Latent heat"]
[null,"R-12",30,"Fugacity / Pressure"]
[null,"R-22",31]
[null,"R-32",32]
[null,"R-123",33]
[null,"R-124",34]
[null,"R-125",35]
[null,"R-134a",36]
[null,"R-134a",37]
[null,"R-152a",38]

{"sheet":"Property HePak","index":4,"n_rows":61,"n_cols":9,"rows_kept":61,"cut":false,"hidden":true,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,6],[4,2,4,3]]}
["HePak Spreadsheet Example"]
["Using HeCalc, HeProperty, HeUnit and HeInput"]
["Try new input values (shown in red)"]
[]
[null,null,"Thermodynamic state definition"]
[null,null,"Input 1","Input 2","Validate"]
[null,"Index",2,44,{"$f":"[3]!heProperty(Input2)","v":{"$error":"#NAME?"}}]
[null,"Name",{"$f":"[3]!heProperty(Input1)","v":{"$error":"#NAME?"}},{"$f":"[3]!heProperty(Input2)","v":{"$error":"#NAME?"}}]
[null,"Value",6,0,"Unit System",1]
[null,"Units",{"$f":"[3]!heunit(Input1,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(Input2,Units)","v":{"$error":"#NAME?"}}]
[]
[null,2,"Error Message"]
[null,3]
[]
[null,"Property","Property",null,"Property"]
[null,"Index","Name","Value","Units"]
[null,0,{"$f":"[3]!heProperty(B17)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B17,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B17,Units)","v":{"$error":"#NAME?"}},null,null,{"$f":"D17","v":{"$error":"#NAME?"}}]
[null,1,{"$f":"[3]!heProperty(B18)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B18,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B18,Units)","v":{"$error":"#NAME?"}}]
[null,2,{"$f":"[3]!heProperty(B19)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B19,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B19,Units)","v":{"$error":"#NAME?"}}]
[null,3,{"$f":"[3]!heProperty(B20)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B20,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B20,Units)","v":{"$error":"#NAME?"}}]
[null,4,{"$f":"[3]!heProperty(B21)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B21,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B21,Units)","v":{"$error":"#NAME?"}}]
[null,5,{"$f":"[3]!heProperty(B22)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B22,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B22,Units)","v":{"$error":"#NAME?"}}]
[null,6,{"$f":"[3]!heProperty(B23)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B23,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B23,Units)","v":{"$error":"#NAME?"}}]
[null,7,{"$f":"[3]!heProperty(B24)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B24,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B24,Units)","v":{"$error":"#NAME?"}}]
[null,8,{"$f":"[3]!heProperty(B25)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B25,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B25,Units)","v":{"$error":"#NAME?"}}]
[null,9,{"$f":"[3]!heProperty(B26)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B26,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B26,Units)","v":{"$error":"#NAME?"}},null,null,null,9407.9237518543996]
[null,10,{"$f":"[3]!heProperty(B27)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B27,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B27,Units)","v":{"$error":"#NAME?"}}]
[null,11,{"$f":"[3]!heProperty(B28)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B28,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B28,Units)","v":{"$error":"#NAME?"}}]
[null,12,{"$f":"[3]!heProperty(B29)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B29,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B29,Units)","v":{"$error":"#NAME?"}}]
[null,13,{"$f":"[3]!heProperty(B30)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B30,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}}]
[null,14,{"$f":"[3]!heProperty(B31)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B31,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B31,Units)","v":{"$error":"#NAME?"}}]
[null,15,{"$f":"[3]!heProperty(B32)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B32,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B32,Units)","v":{"$error":"#NAME?"}}]
[null,16,{"$f":"[3]!heProperty(B33)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B33,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B33,Units)","v":{"$error":"#NAME?"}}]
[null,17,{"$f":"[3]!heProperty(B34)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B34,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B34,Units)","v":{"$error":"#NAME?"}}]
[null,18,{"$f":"[3]!heProperty(B35)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B35,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B35,Units)","v":{"$error":"#NAME?"}}]
[null,19,{"$f":"[3]!heProperty(B36)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B36,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B36,Units)","v":{"$error":"#NAME?"}},null,null,null,{"$f":"[3]!hecalc(19,0,1,Value1,2,Value2,1)","v":{"$error":"#NAME?"}}]
[null,20,{"$f":"[3]!heProperty(B37)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B37,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B37,Units)","v":{"$error":"#NAME?"}},null,null,null,{"$f":"[3]!hecalc(20,0,1,P,2,T,1)","v":{"$error":"#NAME?"}}]
[null,21,{"$f":"[3]!heProperty(B38)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B38,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B38,Units)","v":{"$error":"#NAME?"}}]
[null,22,{"$f":"[3]!heProperty(B39)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B39,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B39,Units)","v":{"$error":"#NAME?"}}]
[null,23,{"$f":"[3]!heProperty(B40)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B40,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B40,Units)","v":{"$error":"#NAME?"}}]
[null,24,{"$f":"[3]!heProperty(B41)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B41,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B41,Units)","v":{"$error":"#NAME?"}}]
[null,25,{"$f":"[3]!heProperty(B42)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B42,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B42,Units)","v":{"$error":"#NAME?"}}]
[null,26,{"$f":"[3]!heProperty(B43)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B43,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B43,Units)","v":{"$error":"#NAME?"}}]
[null,27,{"$f":"[3]!heProperty(B44)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B44,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B44,Units)","v":{"$error":"#NAME?"}}]
[null,28,{"$f":"[3]!heProperty(B45)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B45,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B45,Units)","v":{"$error":"#NAME?"}}]
[null,29,{"$f":"[3]!heProperty(B46)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B46,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B46,Units)","v":{"$error":"#NAME?"}}]
[null,30,{"$f":"[3]!heProperty(B47)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B47,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B47,Units)","v":{"$error":"#NAME?"}}]
[null,31,{"$f":"[3]!heProperty(B48)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B48,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B48,Units)","v":{"$error":"#NAME?"}}]
[null,32,{"$f":"[3]!heProperty(B49)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B49,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B49,Units)","v":{"$error":"#NAME?"}}]
[null,33,{"$f":"[3]!heProperty(B50)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B50,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B50,Units)","v":{"$error":"#NAME?"}}]
[null,34,{"$f":"[3]!heProperty(B51)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B51,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B51,Units)","v":{"$error":"#NAME?"}}]
[null,35,{"$f":"[3]!heProperty(B52)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B52,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B52,Units)","v":{"$error":"#NAME?"}}]
[null,36,{"$f":"[3]!heProperty(B53)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B53,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B53,Units)","v":{"$error":"#NAME?"}}]
[null,37,{"$f":"[3]!heProperty(B54)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B54,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B54,Units)","v":{"$error":"#NAME?"}}]
[null,38,{"$f":"[3]!heProperty(B55)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B55,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B55,Units)","v":{"$error":"#NAME?"}}]
[null,39,{"$f":"[3]!heProperty(B56)","v":{"$error":"#NAME?"}},{"$f":"[3]!hecalc(B56,0,Input1,Value1,Input2,Value2,Units)","v":{"$error":"#NAME?"}},{"$f":"[3]!heunit(B56,Units)","v":{"$error":"#NAME?"}}]
[null,40," reserved"]
[null,41,{"$f":"[3]!heProperty(B58)","v":{"$error":"#NAME?"}},"Input only"," N/A"]
[null,42,{"$f":"[3]!heProperty(B59)","v":{"$error":"#NAME?"}},"Input only"," N/A"]
[null,43,{"$f":"[3]!heProperty(B60)","v":{"$error":"#NAME?"}},"Input only"," N/A"]
[null,44,{"$f":"[3]!heProperty(B61)","v":{"$error":"#NAME?"}},"Input only"," N/A"]

{"sheet":"Dump_Case_A","index":5,"n_rows":191,"n_cols":9,"rows_kept":191,"cut":false,"hidden":true,"merged":[]}
[null,"Case:","03-1800s\\(03)-JT60-CALCULA-Case_A-RETOUR FIVE.HSC"]
[null,"Flowsheet:","Case (Main)"]
[null,"Current Flowsheet Environment:","Case (Main)"]
[]
[null,"Name","Vapour Fraction","Temperature","Pressure","Molar Flow","Mass Flow","Liquid Volume Flow","Heat Flow"]
[1,null,"<none>","K","bar","Nm3/h(gas)","g/s","m3/h","W*"]
[]
[null,"HP1-2",1,306.03542159212702,15.43,12848.126284745576,637.3843175785953,18.4951596592811,1016046.3966283227]
[null,"LP2",1,78.184679465655961,1.2650000000000001,11867.086467006613,588.71578950774438,17.082931318815856,239188.18604186684]
[null,"HP3-2",1,40.047038661081586,13.41,8458.7750195132503,419.63243696978395,12.176592215908018,87414.458274469871]
[null,"LP3",1,37.17595899892865,1.28,11867.086467006613,588.71578950774438,17.082931318815856,113626.12494126637]
[null,"T1Inlet",1,40.048499966105226,14.77,3859.2068735841226,191.45188060881134,5.5554129608671445,39894.138560595689]
[null,"MP4",1,31.105560471733043,6.3574972807075403,3853.1595991546756,191.15188060881133,5.5467077766560502,30718.847084303761]
[null,"HP4",1,31.216780198458963,13.39,8458.7750195132503,419.63243696978395,12.176592215908018,67392.470375358709]
[null,"MP5",1,18.206690861326763,6.3074972807075405,3853.1595991546756,191.15188060881133,5.5467077766560502,17318.459678778287]
[null,"LP5",1,17.052574077198301,1.3,11867.086467006613,588.71578950774438,17.082931318815856,51566.207686899477]
[null,"HP6",1,11.64421199456757,13.16,8458.7750195132503,419.63243696978395,12.176592215908018,18561.042432477152]
[null,"LP6",1,11.517741279750169,1.33,8019.974142281385,397.86390889893306,11.5449287263709,23062.891778623496]
[null,"HP7",1,7.2901961314512391,13.15,8458.7750195132503,419.63243696978395,12.176592215908018,5401.8583610406358]
[null,"LP7",1,6.0099043725298884,1.335,8019.974142281385,397.86390889893306,11.5449287263709,10562.960252070212]
[null,"HP7-4",1,6.1198463189917334,4.88,8040.9063406803079,398.90233696978396,11.575061085193328,3065.4507687446835]
[null,"LP8",1,4.7842734195701269,1.34,8019.974142281385,397.86390889893306,11.5449287263709,7017.8639574854187]
[null,"JT2-3",0.18465298228890648,4.29966642777174,1.089,1855.7256880631958,92.060929748454114,2.6713578403496943,-100.22121965492921]
[null,"LHe 3,6K",0,3.6017715941583788,0.53,0,0,0,0]
[null,"HP5",1,18.206690861326763,13.370000000000001,8458.7750195132503,419.63243696978395,12.176592215908018,36433.19976498076]
[null,"GHe 4,3K",1,4.3005872176408388,1.089,8027.9791381393379,398.26102974823527,11.556452093528373,6149.3834057338872]
[null,"LHe 4,3K",0,4.3005872176408388,1.089,0,0,0,0]
[null,"GHe 3,6K",1,3.6017715941583788,0.53,470.50631678953641,23.341407221329757,0.67730416535947757,347.81760490036106]
[null,"HP8-3",0,4.9085733022856743,4.8600000000000003,8040.9063406803052,398.90233696978396,11.575061085193326,-434.26107952146373]
[null,"HP8-5",0,4.9085733022856743,4.8600000000000003,6185.1806526171104,306.84140722132975,8.9037032448436317,-334.03985986653447]
[null,"VLP0",0.16926223137622748,3.6013106108128454,0.53,470.50631678953641,23.341407221329757,0.67730416535947757,-97.914428516176841]
[null,"MP",1,1167.9976906835884,16,13542.722238668552,671.8426158761215,19.495045773550444,4077535.3036996946]
[null,"MP-1",1,306,16,13542.722238668552,671.8426158761215,19.495045773550444,1070975.9404742583]
[null,"TS_inlet",1,79.325619609462962,15,8566.9721083834884,425,12.33234429905032,176636.10745590809]
[null,"TS_outlet",1,99.28787818321868,13.5,8566.9721083834884,425,12.33234429905032,220736.10761227418]
[null,"To Comp LP",1,299.23575242238718,1.05,13542.722238668552,671.8426158761215,19.495045773550444,1044138.4964940305]
[null,"LIN-a",0,78.456658780366723,1.1499999999999999,624.41159674520225,216.77476334869857,0.96777565419156975,-25824.752047636106]
[null,"GAN-b",1,78.083557582674587,1.0999999999999999,663.75237266783768,230.43256124200616,1.0287499303795704,17924.108208211856]
[null,"HP2-5",1,79.325095034324079,15.01,12848.126284745576,637.3843175785953,18.4951596592811,264905.91116159834]
[null,"to_CL-1",1,79.256095211223084,13.41,132.91802613195998,6.5939471252395823,0.19133841467808849,2735.5494622188753]
[null,"CL_inlet",1,49.999999517451386,4,530.1443916482018,26.3,0.76315448250593731,6840.5560942473676]
[null,"CL_outlet",1,300,1.05,530.1443916482018,26.3,0.76315448250593731,40978.289286214262]
[null,"GAN-c",1,298.36423374983542,1.0499999999999998,663.75237266783768,230.43256124200616,1.0287499303795704,71307.415158614458]
[null,"After Comp",1,306.03107160706776,15.5,13542.722238668552,671.8426158761215,19.495045773550444,1070975.9404742583]
[null,"LPbypass",1,306.03107160706776,15.5,406.28166716005654,20.155278476283645,0.58485137320651337,32129.278214227754]
[null,"Paliers",1,306.03107160706776,15.5,241.89097717788673,12,0.3482073684437737,19129.050438296072]
[null,"Recycle",1,307,1.05,268.70056048176917,13.330000000000002,0.3868003517796253,21254.115816195532]
[null,"To recycle",1,277.31156404474967,1.33,268.70056048176917,13.330000000000002,0.3868003517796253,19200.413215522298]
[null,"T1Outlet",1,31.105560471733043,6.3574972807075403,3859.2068735841226,191.45188060881134,5.5554129608671445,30767.058245480621]
[null,"T1Leak",1,31.105560471733043,6.3574972807075403,6.0472744294471683,0.3,8.7051842110943429E-3,48.211161176859093]
[null,"T2Outlet-1",1,11.611000695982284,1.33,3853.1595991546756,191.15188060881133,5.5467077766560502,11177.14369867865]
[null,"T2Leak",1,11.611000695982284,1.33,6.0472744294471674,0.3,8.7051842110943412E-3,17.541774106139908]
[null,"T3Outlet",1,6.1198463189917334,4.88,8055.6213751252953,399.63233696978398,11.59624370010699,3071.0606106879086]
[null,"T3Leak",1,6.1198463189917334,4.88,14.715034444988108,0.73,2.1182614913662898E-2,5.6098419432251321]
[null,"ColdComp_Outlet",1,4.7890911692025497,1.35,8019.974142281385,397.86390889893306,11.5449287263709,7002.8639574854187]
[null,"VLP9-1",1,3.6610712458889907,0.53,470.50631678953641,23.341407221329757,0.67730416535947757,357.81760490036106]
[null,"HP9",0,4.1538860204182129,4.7700000000000005,470.50631678953641,23.341407221329753,0.67730416535947757,-97.914428516176827]
[null,"VLP8",1,4.1006180764131273,0.51,470.50631678953641,23.341407221329757,0.67730416535947757,429.96583626016911]
[null,"HP2-9",1,79.262046622795083,13.43,8856.0013850294927,439.33848984454437,12.748408283735866,182278.77125003026]
[null,"HP2_TS-2",1,79.25467548007893,13.44,8566.9721083834884,425,12.33234429905032,176314.504705826]
[null,"HP8-4",0,4.9085733022856743,4.8600000000000003,1855.7256880631958,92.060929748454114,2.6713578403496943,-100.22121965492926]
[null,"VLP7",1,6.0099118754370693,0.495,470.50631678953641,23.341407221329757,0.67730416535947757,690.92102881500125]
[null,"VLP6",1,11.51780796431575,0.49,470.50631678953641,23.341407221329757,0.67730416535947757,1380.1735736982428]
[null,"VLP5",1,17.052585865976255,0.47500000000000003,470.50631678953641,23.341407221329757,0.67730416535947757,2058.5960187144601]
[null,"VLP4",1,30.895220174119316,0.47000000000000003,470.50631678953641,23.341407221329757,0.67730416535947757,3742.9606464178569]
[null,"VLP3",1,37.175959074112399,0.46500000000000002,470.50631678953641,23.341407221329757,0.67730416535947757,4505.4990102372558]
[null,"LP",1,550.29478168872504,1.18,568.63253578710703,28.209363197649214,0.81855901037733925,80616.732262080885]
[null,"CryoPumps_Inlet",0,3.6999999999999886,4.7,5714.6743358275735,283.5,8.2263990794841533,-1619.9808315339767]
[null,"CryoPumps_Outlet",0,3.8727213200608617,4.2,5714.6743358275735,283.5,8.2263990794841533,-1538.0808315339766]
[null,"LP9-2",0,4.1006253736028384,4.1950000000000003,5714.6743358275735,283.5,8.2263990794841533,-1317.7818185719507]
[null,"HP9-1",0,4.1538860204182129,4.7700000000000005,5714.6743358275735,283.5,8.2263990794841533,-1189.2487981174388]
[null,"HP1",1,306.03107160706776,15.5,12848.126284745576,637.3843175785953,18.4951596592811,1016046.3966283227]
[null,"LP-4",1,298.78047892230057,1.05,12337.59278379615,612.05719672907412,17.760235484175332,949776.58893588337]
[null,"To Comp VLP",1,299.93614087247914,0.35000000000000003,568.63253578710703,28.209363197649214,0.81855901037733925,43937.554366675395]
[null,"to_TS",1,79.325619609462962,15,8566.9721083834884,425,12.33234429905032,176636.10745590809]
[null,"to_CL-2",1,79.25467548007893,13.44,132.91802613195998,6.5939471252395823,0.19133841467808849,2735.5494622188753]
[null,"HP2-7",1,79.326988414522475,14.97,4281.1541763620871,212.3843175785953,6.1628153602307814,88269.917556693661]
[null,"HP2-8",1,79.326988414522475,14.97,3859.2068735841226,191.45188060881134,5.5554129608671445,79570.101550270527]
[null,"HP5-1",1,18.23210103507472,13.19,8458.7750195132503,419.63243696978395,12.176592215908018,36533.199764980767]
[null,"Piston",1,4.3005872176408388,1.089,-8.0049958579525526,-0.39712084930223795,-1.1523367157474059E-2,-6.1317783522879337]
[null,"To Buffer",1,306.03107160706776,15.5,46.423309585034367,2.3030198212425912,6.6827372619061076E-2,3671.2151934120943]
[null,"VLP8-1",1,4.1928491362572231,0.5,470.50631678953641,23.341407221329757,0.67730416535947757,444.96583626016906]
[null,"HP2-4",1,79.25467548007893,15.23,12848.126284745576,637.3843175785953,18.4951596592811,264705.91116159834]
[null,"CP1_Inlet",0,4.4005872176408616,4.4400000000000004,12753.70177170408,632.70000000000016,18.359233501197973,-2162.4171539180679]
[null,"CP1_Outlet",0,4.5925162644143711,5.3639999999999999,12753.70177170408,632.70000000000005,18.359233501197973,-1447.0391818103953]
[null,"TF_Inlet",0,4.4005872176408616,5.3269999999999991,12955.277586018985,642.70000000000016,18.64940630823445,-1957.8661113953472]
[null,"TF_Outlet",0,5.1272391579178134,4.4770000000000003,12955.277586018985,642.70000000000016,18.64940630823445,-30.986111395346903]
[null,"HP9-0",0,4.1538860204182129,4.7700000000000005,6185.1806526171104,306.84140722132975,8.9037032448436317,-1287.1632266336157]
[null,"CP2_Inlet",0,4.4005872176408616,4.5559999999999992,19351.278174230942,960,27.856589475501899,-3235.9260492024214]
[null,"CP2_outlet",0,4.5598665766777344,5.4989999999999988,19351.278174230942,960,27.856589475501899,-2267.9763699260179]
[null,"PF_Inlet",0,4.4005872176408616,5.4289999999999985,19552.853988545845,970,28.146762282538372,-2911.9747366754946]
[null,"PF_Outlet",0,5.1304973513720711,4.6289999999999996,19552.853988545845,970,28.146762282538372,-15.544736675495052]
[null,"HP8-6",0,4.4005872176408616,4.79,6185.1806526171104,306.84140722132975,8.9037032448436317,-1004.7159823117819]
[null,"MP6",1,11.611000695982284,1.33,3847.1123247252285,190.85188060881134,5.5380025924449559,11159.601924572509]
[null,"LP9-3",9.6861101662670031E-3,4.2970891312015169,1.0889999999999997,5714.6743358275735,283.5,8.2263990794841533,-1317.7818185719505]
[null,"HP3-3",1,40.047038661081586,14.950000000000001,3859.2068735841226,191.45188060881134,5.5554129608671445,39894.138560595689]
[null,"GHe1-3",0.99807902472180998,4.2834637322512208,1.069,8019.974142281385,397.86390889893306,11.5449287263709,6143.2516273815991]
[null,"T3Inlet",1,7.2915401710176297,13.07,8055.6213751252953,399.63233696978398,11.59624370010699,5144.4004100137754]
[null,"LP-1",1,307,1.1300000000000001,568.63253578710703,28.209363197649214,0.81855901037733925,44979.352853074466]
[null,"VLP1-1",1,298.45283863110609,0.35000000000000003,470.50631678953641,23.341407221329757,0.67730416535947757,36175.680835607804]
[null,"VLPbypass",1,307,1.1300000000000001,98.126218997570589,4.8679559763194566,0.14125484501786162,7761.8735310675838]
[null,"VLP-2",1,307.04844129479807,0.35000000000000003,98.126218997570589,4.8679559763194566,0.14125484501786162,7761.8735310675838]
[null,"Conso.liq",0,4.2993665145158388,1.089,54.425469860611628,2.6999999997810806,7.8346657893496638E-2,-13.045642021938287]
[null,"HP2-6",1,79.325095034324079,15.01,4281.1541763620871,212.3843175785953,6.1628153602307814,88269.917556693661]
[null,"From_Buffer",1,307,1.05,0,0,0,0]
[null,"LPbypass-2",1,306.03107160706776,15.5,406.28450274243113,20.155419147047358,0.58485545508955084,32129.502455737387]
[null,"LPbypass-3",1,306.928788694204,1.05,406.28450274243113,20.155419147047358,0.58485545508955084,32129.502455737387]
[null,"GHe",1,4.3005870925301792,1.089,8019.974142281385,397.86390889893306,11.5449287263709,6143.2516273815991]
[null,"LP6-2",1,11.547967087580048,1.33,11867.086467006613,588.71578950774438,17.082931318815856,34222.493703196007]
[null,"LP4",1,30.895210157347776,1.29,11867.086467006613,588.71578950774438,17.082931318815856,94336.675405974616]
[null,"HP3-4",1,40.047038661081586,13.41,397.2263655162418,19.70605287476042,0.57181606782784888,4105.0066320284923]
[null,"HP2_TS-3",1,79.25467548007893,13.44,8434.0540822515286,418.40605287476041,12.14100588437223,173578.95524360711]
[null,"HP3-1",1,40.047038661081586,13.41,8856.0013850294927,439.33848984454437,12.748408283735866,91519.464906498353]
[null,"bypass",1,79.399926781546299,13.43,421.94730277796401,20.932436969783975,0.60740239936363649,8699.8160064231361]
[null,"bypass-2",1,79.326988414522475,14.97,421.94730277796401,20.932436969783975,0.60740239936363649,8699.8160064231361]
[null,"T2Outlet",1,11.616052328242404,1.35,3853.1595991546756,191.15188060881133,5.5467077766560502,11177.14369867865]
[null,"HP8",0,4.8999999999999773,4.87,8040.9063406803079,398.90233696978396,11.575061085193328,-449.26107952146361]
[null,"LP-3",1,298.77550072547831,1.1300000000000001,12337.59278379615,612.05719672907412,17.760235484175332,949776.58893588337]
[null,"HP8-1",0,4.8999999999999773,8.1449999999999996,403.15364438795439,20.0001,0.58034851580102653,1.1183121533825173]
[null,"HP7-2",1,7.117430731773311,8.15,403.15364438795439,20.0001,0.58034851580102653,257.45795102686066]
[null,"HP7-3",1,7.2901961314512391,13.15,8055.6213751252953,399.63233696978398,11.59624370010699,5144.4004100137754]
[null,"to_damper",0.2465130159501667,4.2983202188397627,1.089,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,1.5591482809498592E-5]
[null,22,"<empty>","<empty>","<empty>","<empty>","<empty>","<empty>","<empty>"]
[null,"WaterInlet","<empty>",303,"<empty>","<empty>","<empty>","<empty>","<empty>"]
[null,"LP-2",1,307,1.1300000000000001,470.50631678953641,23.341407221329757,0.67730416535947757,37217.479322006882]
[null,"HP_BP1-b",1,306.03542159212702,15.43,910.35312248247158,45.161822889143863,1.3104732918627138,71991.898994318908]
[null,"HP_BP1-a",1,306.04163583935258,15.33,910.3531224824718,45.161822889143856,1.3104732918627138,71991.898994318908]
[null,"HP_BP1",1,306.04163583935258,15.33,910.3531224824718,45.16182288914387,1.3104732918627142,71991.898994318908]
[null,"HP2_MEF",1,87.303262700252361,15.345000000000001,0,0,0,0]
[null,"HP2_MEF-2",1,87.304020830941596,15.33,0,0,0,0]
[null,"HP2-1",1,87.303262700252361,15.345000000000001,11937.773162263104,592.22249468945142,17.184686367418387,270872.3471836485]
[null,"HP2-2",1,87.3065479989925,15.280000000000001,11937.773162263104,592.22249468945142,17.184686367418387,270872.3471836485]
[null,"HP_BP2",1,78.713557687592242,15.280000000000001,910.3531224824718,45.16182288914387,1.3104732918627142,18628.478192913008]
[null,"HP2-3",1,86.697229599499025,15.280000000000001,12848.126284745576,637.3843175785953,18.4951596592811,289500.82537656149]
[null,"to_TS-3",1,79.325568374155807,15,8566.9700926253445,424.99989999999997,12.332341397322249,176635.95204349441]
[null,"HP_CD2-1",1,79.325095034324079,15.01,2.0157581431490558E-3,1E-4,2.9017280703647807E-6,4.1561410259977574E-2]
[null,"HP_CD2",1,79.325568374155807,15,2.0157581431490563E-3,9.9999999999999978E-5,2.9017280703647803E-6,4.1561410259977574E-2]
[null,"HP_CD1",1,298.36421852439736,15,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,0.15541241363548391]
[null,"to_TS-2",1,79.325619609462962,15,8566.9721083834884,425,12.33234429905032,176636.10745590809]
[null,"bypass_TS",1,79.325619609462962,15,0,0,0,0]
[null,"bypass_TS-1",1,79.396660806178204,13.5,0,0,0,0]
[null,"to_TS-4",1,79.325095034324079,15.01,8566.9700926253445,424.99989999999997,12.332341397322249,176635.95204349441]
[null,"bypass_HP_BP-2",1,87.924167462429239,1.2650000000000001,0,0,0,0]
[null,"HP2_TS",1,87.303262123331024,13.47,8566.9721083834884,425,12.33234429905032,194177.36130086574]
[null,"bypass_HP_BP",1,87.303262123331024,13.47,0,0,0,0]
[null,"LIN",5.9270260329935869E-2,78.456658780366723,1.1499999999999999,663.75237266783768,230.43256124200616,1.0287499303795704,-24758.662601791089]
[null,"GAN-a",1,78.068329195532272,1.0999999999999999,624.41159674520225,216.77476334869857,0.96777565419156975,16858.018762366839]
[null,"GAN",1,78.456658780366723,1.1499999999999999,39.340775922635352,13.657797893307597,6.0974276188000547E-2,1066.0894458450171]
[null,"N2-a",5.1478539579731504E-3,83.591521847287027,1.99,663.75237266783768,230.43256124200616,1.0287499303795704,-24758.662601791089]
[null,"N2",0,83.644048867120603,2,663.75237266783768,230.43256124200616,1.0287499303795704,-24958.662601791086]
[null,"to_TS-1",1,79.325619609462962,15,8566.9721083834884,425,12.33234429905032,176636.10745590809]
[null,"HP_CD2-2",1,79.325619609462962,15,0,0,0,0]
[null,"HP2_TS-4",1,79.255148717964175,13.43,8434.0540822515286,418.40605287476041,12.14100588437223,173578.95524360711]
[null,"HP_CD2-3",1,79.399978053521124,13.43,0,0,0,0]
[null,"HP2-10",1,79.255148717964175,13.43,8434.0540822515286,418.40605287476041,12.14100588437223,173578.95524360711]
[null,"supply_loop",0,4.9268380325488579,8.1349999999999998,403.15162862981123,20,0.58034561407295615,3.1182965618997076]
[null,"supply_loop1-1",0,5.1406783912854621,5.3639999999999999,201.57581431490732,10.000000000000085,0.29017280703648057,1.5591482809498671]
[null,"CP1_outlet-2",0,4.6019944153052279,5.3639999999999999,12955.277586018985,642.70000000000016,18.64940630823445,-1445.4800335294456]
[null,"supply_loop2",0,4.9268380325488579,8.1349999999999998,201.57581431490394,9.9999999999999165,0.29017280703647563,1.5591482809498409]
[null,2,0,4.5664677151130491,5.4989999999999988,19552.853988545845,970,28.146762282538372,-2266.4172216450679]
[null,"HP8-2",0,4.9268380325488579,8.1349999999999998,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,1.5591482809498541E-5]
[null,"supply_loop1",0,4.9268380325488579,8.1349999999999998,201.57581431490732,10.000000000000085,0.29017280703648057,1.5591482809498671]
[null,"supply_loop2-2",0,5.1347590053908334,5.4989999999999988,201.57581431490394,10.000000000000028,0.29017280703647563,1.5591482809498409]
[null,"return-1",0,4.4005872176408616,4.4400000000000004,201.57581431490803,10.000000000000121,0.29017280703648152,-34.177606352427595]
[null,"return-2",0,4.4005872176408616,4.5559999999999992,201.57581431490561,10,0.29017280703647808,-33.70756301252522]
[null,"return-3",0,4.4065469298216158,4.4400000000000004,403.15162862981362,20.000000000000117,0.58034561407295959,-67.885169364952816]
[null,"CD_return",0,4.4065469298216158,4.4400000000000004,0,0,0,0]
[null,"baking_return",0,4.4065469298216158,4.4400000000000004,0,0,0,0]
[null,"LP5-1",1,17.052574077198301,1.3,11867.086467006613,588.71578950774438,17.082931318815856,51566.207686899477]
[null,"baking_return-1",1.3322776910864965E-2,4.4975304797696367,1.3,0,0,0,0]
[null,"LP2-1",1,78.184679465655961,1.2650000000000001,11867.086467006613,588.71578950774438,17.082931318815856,239188.18604186684]
[null,"CD_return-2",2.3384523911381492E-2,4.4666663212527169,1.2650000000000001,0,0,0,0]
[null,"CL_inlet-2",1,49.781374749308782,13.41,530.1443916482018,26.3,0.76315448250593731,6840.5560942473676]
[null,"return_4",0,4.4065469298216158,4.4400000000000004,0,0,0,0]
[null,"return_damper",0,4.4065469298216158,4.4400000000000004,403.15162862981362,20.000000000000117,0.58034561407295959,-67.885169364952816]
[null,"HP7-5",1,7.2901961314512391,13.15,403.15364438795439,20.0001,0.58034851580102653,257.45795102686066]
[null,"return_damper-1",7.0991777045512308E-2,4.2992171375507837,1.0889999999999997,403.15162862981362,20.000000000000117,0.58034561407295959,-67.88516936495283]
[null,1,0,4.9268380325488579,8.1349999999999998,403.15364438795439,20.0001,0.58034851580102653,3.1183121533825173]
[null,"CP1_inlet-1",0,4.4005872176408616,4.4400000000000004,12955.277586018985,642.70000000000016,18.64940630823445,-2196.594760270495]
[null,"CP2_Inlet-1",0,4.4005872176408616,4.5559999999999992,19552.853988545845,970,28.146762282538372,-3269.6336122149464]
[null,"HP1-3",1,306.03542159212702,15.43,11937.773162263104,592.22249468945142,17.184686367418387,944054.49763400375]
[null,"LP2-2",1,78.184679465655961,1.2650000000000001,11867.086467006613,588.71578950774438,17.082931318815856,239188.18604186684]
[null,"VLP2",1,78.184679321568581,0.45500000000000002,470.50631678953641,23.341407221329757,0.67730416535947757,9478.7072428435149]
[null,"HP1_TS",1,99.287878180816193,13.5,8566.9721083834884,425,12.33234429905032,220736.10761227418]
[null,"HP2",1,87.303262700252361,15.345000000000001,11937.773162263104,592.22249468945142,17.184686367418387,270872.3471836485]
[null,"LP1",1,298.44941584058631,1.1300000000000001,11867.086467006613,588.71578950774438,17.082931318815856,912559.10961387656]
[null,"VLP1",1,298.44941591898913,0.40500000000000003,470.50631678953641,23.341407221329757,0.67730416535947757,36175.680835607804]
[null,"HP2_TS-1",1,87.303262123331024,13.47,8566.9721083834884,425,12.33234429905032,194177.36130086574]
[null,"LP1a",1,98.29000000000002,1.1300000000000001,11867.086467006613,588.71578950774438,17.082931318815856,300654.74334887642]
[null,"VLP1a",1,98.29000000000002,0.40500000000000003,470.50631678953641,23.341407221329757,0.67730416535947757,11915.582185663225]
[null,"HP1a",1,99.29000000000002,15.43,11937.773162263104,592.22249468945142,17.184686367418387,307917.12961658172]

{"sheet":"Dump_Case_B","index":6,"n_rows":196,"n_cols":9,"rows_kept":196,"cut":false,"hidden":true,"merged":[]}
[]
[]
[]
[null,"Case:","1800s\\(03)-JT60-CALCULB-1800S-OFFCase_A.HSC"]
[null,"Flowsheet:","Case (Main)"]
[null,"Current Flowsheet Environment:","Case (Main)"]
[]
[null,"Name","Vapour Fraction","Temperature","Pressure","Molar Flow","Mass Flow","Liquid Volume Flow","Heat Flow"]
[null,null,"<none>","K","bar","Nm3/h(gas)","g/s","m3/h","W*"]
[]
[null,"HP1-2",1,306.03542159212702,15.43,12859.364394922464,637.9418304039848,18.511337165431314,1016935.1208747287]
[null,"LP2",1,78.223942316800446,1.2650000000000001,11851.177669938003,587.92656798716257,17.060030256415775,238987.47292800268]
[null,"HP3-2",1,40.574857394438254,13.41,8495.865065662274,421.47244174789097,12.229984151050401,88988.32787670166]
[null,"LP3",1,37.693268503161903,1.28,11851.177669938003,587.92656798716257,17.060030256415775,115058.92938827998]
[null,"T1Inlet",1,40.576507807476162,14.77,3833.35493761199,190.1693886560939,5.5181985318749733,40165.743189295616]
[null,"MP4",1,31.52847039955779,6.3644245502282208,3827.3076631825429,189.86938865609389,5.5094933476638799,30940.525213368095]
[null,"HP4",1,31.780008951075501,13.39,8495.865065662274,421.47244174789097,12.229984151050401,68984.43673534182]
[null,"MP5",1,18.468845735746243,6.314424550228221,3827.3076631825429,189.86938865609389,5.5094933476638799,17480.848609270728]
[null,"LP5",1,17.297258737955303,1.3,11851.177669938003,587.92656798716257,17.060030256415775,52258.55671712097]
[null,"HP6",1,11.80606993757084,13.16,8495.865065662274,421.47244174789097,12.229984151050401,19134.349105526548]
[null,"LP6",1,11.671811147563176,1.33,8029.9172811849066,398.35717933106872,11.559242092962991,23424.276112807464]
[null,"HP7",1,7.2195731480463792,13.15,8495.865065662274,421.47244174789097,12.229984151050401,5257.0396852421718]
[null,"LP7",1,5.8844286884979056,1.335,8029.9172811849066,398.35717933106872,11.559242092962991,10252.926751321253]
[null,"HP7-4",1,6.0906044208006165,4.88,8077.9963868293371,400.74234174789115,11.628453020335717,2940.8839276267367]
[null,"LP8",1,4.6321909715632046,1.34,8029.9172811849066,398.35717933106872,11.559242092962991,6452.6077499938692]
[null,"JT2-3",8.8338852450732988E-2,4.5100597024934928,1.3134999999999999,1885.3687908933953,93.531498176067686,2.7140297372076794,-178.53328742286783]
[null,"LHe 3,6K",0,3.6017715941583788,0.53,0,0,0,0]
[null,"HP5",1,18.468845735746243,13.370000000000001,8495.865065662274,421.47244174789097,12.229984151050401,37257.403367046041]
[null,"GHe 4,3K",1,4.5104401840179094,1.3134999999999999,8036.1065393242843,398.66422301884512,11.56815166583948,6051.978905552508]
[null,"LHe 4,3K",0,4.5104401840179094,1.3134999999999999,0,0,0,0]
[null,"GHe 3,6K",1,3.6017715941583788,0.53,477.95326010837084,23.710843571823705,0.68802420364389161,353.32269143492579]
[null,"HP8-3",0,4.7273832222070951,4.8600000000000003,8077.9963868293398,400.74234174789126,11.628453020335721,-764.93854024564462]
[null,"HP8-5",0,4.7273832222070951,4.8600000000000003,6192.6275959359436,307.21084357182366,8.9144232831280448,-586.4052528227769]
[null,"VLP0",0.17024809307344591,3.6013829126205792,0.53,477.95326010837084,23.710843571823705,0.68802420364389161,-98.919671321231661]
[null,"MP",1,1163.8683834077385,16,13533.996254880778,671.40972744566022,19.482484528450389,4060513.6138515058]
[null,"MP-1",1,306,16,13533.996254880778,671.40972744566022,19.482484528450389,1070285.8784225543]
[null,"TS_inlet",1,79.325568839981031,15,8566.9721083834884,425,12.33234429905032,176635.99464002429]
[null,"TS_outlet",1,99.2878271514044,13.5,8566.9721083834884,425,12.33234429905032,220735.99461334318]
[null,"To Comp LP",1,298.17774337280605,1.05,13533.996254880778,671.40972744566022,19.482484528450389,1039777.1995343617]
[null,"LIN-a",0,78.456627644318417,1.1499999999999999,645.97568840555164,224.26109270399618,1.0011978440138345,-26716.625823532398]
[null,"GAN-b",1,78.083518235379557,1.0999999999999999,686.56857857456919,238.35358266718188,1.06411277231373,18540.231238815446]
[null,"HP2-5",1,79.325042587181144,15.01,12859.364394922464,637.9418304039848,18.511337165431314,265137.4464164814]
[null,"to_CL-1",1,79.256095211223084,13.41,127.4024609682124,6.3203247572737977,0.1833986376200285,2622.0351274322338]
[null,"CL_inlet",1,49.999439213672701,4,530.1443916482018,26.3,0.76315448250593731,6840.4791234295944]
[null,"CL_outlet",1,300,1.05,530.1443916482018,26.3,0.76315448250593731,40978.289286214262]
[null,"GAN-c",1,305.54610271176699,1.0499999999999998,686.56857857456919,238.35358266718188,1.06411277231373,75540.05678711072]
[null,"After Comp",1,306.03107160706776,15.5,13533.996254880778,671.40972744566022,19.482484528450389,1070285.8784225543]
[null,"LPbypass",1,306.03107160706776,15.5,406.01988764642334,20.142291823369806,0.58447453585351172,32108.576352676628]
[null,"Paliers",1,306.03107160706776,15.5,241.8909771778867,12,0.3482073684437737,19129.050438296068]
[null,"Recycle",1,307,1.05,268.70056048176917,13.330000000000002,0.3868003517796253,21254.115816195532]
[null,"To recycle",1,277.3217219691283,1.33,268.70056048176917,13.329999999999998,0.38680035177962524,19201.116304837473]
[null,"T1Outlet",1,31.52847039955779,6.3644245502282208,3833.35493761199,190.1693886560939,5.5181985318749733,30989.4122805763]
[null,"T1Leak",1,31.52847039955779,6.3644245502282208,6.0472744294471683,0.3,8.7051842110943429E-3,48.887067208200619]
[null,"T2Outlet-1",1,11.783173096772089,1.33,3827.3076631825429,189.86938865609389,5.5094933476638799,11279.272230484112]
[null,"T2Leak",1,11.783173096772089,1.33,6.0472744294471674,0.3,8.7051842110943412E-3,17.821628294565162]
[null,"T3Outlet",1,6.0906044208006165,4.88,8092.7114212743254,401.47234174789116,11.64963563524938,2946.241098665374]
[null,"T3Leak",1,6.0906044208006165,4.88,14.715034444988108,0.73,2.1182614913662894E-2,5.3571710386373583]
[null,"ColdComp_Outlet",1,4.6381976389737929,1.35,8029.9172811849066,398.35717933106872,11.559242092962991,6437.6077499938701]
[null,"VLP9-1",1,3.6601359061009475,0.53,477.95326010837084,23.710843571823705,0.68802420364389161,363.32269143492579]
[null,"HP9",0,4.1603688997793142,4.7700000000000005,477.95326010837084,23.710843571823705,0.68802420364389172,-98.919671321231633]
[null,"VLP8",1,4.3095735949195273,0.51,477.95326010837084,23.710843571823705,0.68802420364389161,467.76364396435713]
[null,"HP2-9",1,79.262614326497157,13.43,8898.6069963422633,441.45211699061713,12.80973999593631,183157.01127474301]
[null,"HP2_TS-2",1,79.25467548007893,13.44,8566.9721083834884,425,12.33234429905032,176314.504705826]
[null,"HP8-4",0,4.7273832222070951,4.8600000000000003,1885.3687908933953,93.531498176067686,2.7140297372076794,-178.5332874228678]
[null,"VLP7",1,5.8843361190763517,0.495,477.95326010837084,23.710843571823705,0.68802420364389161,685.33165863450427]
[null,"VLP6",1,11.671897330608374,0.49,477.95326010837084,23.710843571823705,0.68802420364389161,1421.2917174326753]
[null,"VLP5",1,17.297261160886023,0.47500000000000003,477.95326010837084,23.710843571823705,0.68802420364389161,2121.5165494321641]
[null,"VLP4",1,31.412928340276352,0.47000000000000003,477.95326010837084,23.710843571823705,0.68802420364389161,3866.0732246356611]
[null,"VLP3",1,37.693268979664651,0.46500000000000002,477.95326010837084,23.710843571823705,0.68802420364389161,4640.5874419200718]
[null,"LP",1,548.27179383594478,1.18,570.73031408777081,28.313432145989744,0.82157880826386975,80616.727131865206]
[null,"CryoPumps_Inlet",0,3.6999999999999886,4.7,5714.6743358275735,283.5,8.2263990794841533,-1619.9808315339767]
[null,"CryoPumps_Outlet",0,3.8727213200608617,4.2,5714.6743358275735,283.5,8.2263990794841533,-1538.0808315339766]
[null,"LP9-2",0,4.3095325824839392,4.1950000000000003,5714.6743358275735,283.5,8.2263990794841533,-1097.9976503219907]
[null,"HP9-1",0,4.1603688997793142,4.7700000000000005,5714.6743358275735,283.5,8.2263990794841533,-1182.7384687778192]
[null,"HP1",1,306.03107160706776,15.5,12859.364394922464,637.9418304039848,18.511337165431314,1016935.1208747287]
[null,"LP-4",1,297.61892824104081,1.05,12329.130930046373,611.63741155898629,17.748054460059667,945436.17972026381]
[null,"To Comp VLP",1,298.833471126929,0.35000000000000003,570.73031408777081,28.313432145989744,0.82157880826386975,43937.533985302704]
[null,"to_TS",1,79.325568839981031,15,8566.9721083834884,425,12.33234429905032,176635.99464002429]
[null,"to_CL-2",1,79.25467548007893,13.44,127.4024609682124,6.3203247572737977,0.1833986376200285,2622.0351274322338]
[null,"HP2-7",1,79.326935966425054,14.97,4292.3922865389768,212.94183040398485,6.1789928663809937,88501.569355956352]
[null,"HP2-8",1,79.326935966425054,14.97,3833.35493761199,190.1693886560939,5.5181985318749733,79037.027659607091]
[null,"HP5-1",1,18.494561897014648,13.19,8495.865065662274,421.47244174789097,12.229984151050401,37357.403367046041]
[null,"Piston",1,4.5104401840179094,1.3134999999999999,-6.1892581393774613,-0.30704368777637597,-8.909572876490298E-3,-4.6611203469287457]
[null,"To Buffer",1,306.03107160706776,15.5,26.720995134004021,1.3256052183056033,3.8465458721794021E-2,2113.1307568530301]
[null,"VLP8-1",1,4.4037775428209898,0.5,477.95326010837084,23.710843571823705,0.68802420364389161,482.76364396435713]
[null,"HP2-4",1,79.25467548007893,15.23,12859.364394922464,637.9418304039848,18.511337165431314,264937.4464164814]
[null,"CP1_Inlet",0,4.6104401840179321,6.1639999999999997,8949.9661555818093,444,12.883672632419628,-839.76059223039522]
[null,"CP1_Outlet",0,4.7478888063139379,6.7019999999999991,8949.9661555818093,444,12.883672632419628,-503.31979695129104]
[null,"TF_Inlet",0,4.6104401840179321,6.6829999999999998,9151.5419698967162,454.00000000000006,13.173845439456107,-758.67062793341813]
[null,"TF_Outlet",1,5.7794851490563701,6.1829999999999998,9151.5419698967162,454.00000000000006,13.173845439456107,1717.1693720665821]
[null,"HP9-0",0,4.1603688997793142,4.7700000000000005,6192.6275959359436,307.21084357182366,8.9144232831280448,-1281.6581400990508]
[null,"CP2_Inlet",0,4.6104401840179321,5.5080000000000009,19351.278174230942,960,27.856589475501899,-2072.1330989101539]
[null,"CP2_outlet",0,4.7688295743375875,6.4510000000000005,19351.278174230942,960,27.856589475501899,-1105.2015980381834]
[null,"PF_Inlet",0,4.6104401840179321,6.3810000000000002,19552.853988545845,970,28.146762282538372,-1746.1054639876781]
[null,"PF_Outlet",1,5.3537963346590232,5.5810000000000004,19552.853988545845,970,28.146762282538372,1258.8945360123219]
[null,"HP8-6",0,4.6104401840179321,4.79,6192.6275959359436,307.21084357182366,8.9144232831280448,-747.13400635763344]
[null,"MP6",1,11.783173096772089,1.33,3821.2603887530959,189.56938865609391,5.5007881634527855,11261.450602189549]
[null,"LP9-3",0,4.4631187865177822,1.3135000000000003,5714.6743358275735,283.5,8.2263990794841533,-1097.9976503219907]
[null,"HP3-3",1,40.574857394438254,14.950000000000001,3833.35493761199,190.1693886560939,5.5181985318749733,40165.743189295616]
[null,"GHe1-3",0.99350798967310494,4.4561961797488152,1.25,8029.9172811849066,398.35717933106872,11.559242092962991,6047.3177852055796]
[null,"T3Inlet",1,7.2212356699511133,13.07,8092.7114212743227,401.47234174789105,11.649635635249377,5007.5777774296948]
[null,"LP-1",1,307,1.1300000000000001,570.73031408777081,28.313432145989744,0.82157880826386975,45145.28903233735]
[null,"VLP1-1",1,297.23883688133611,0.35000000000000003,477.95326010837084,23.710843571823705,0.68802420364389161,36598.784292002463]
[null,"VLPbypass",1,307,1.1300000000000001,92.77705397939998,4.6025885741660399,0.13355460461997809,7338.7496933002376]
[null,"VLP-2",1,307.04844129479807,0.35000000000000003,92.77705397939998,4.6025885741660399,0.13355460461997809,7338.7496933002376]
[null,"Conso.liq",0,4.5092194808929094,1.3134999999999999,32.909768215359307,1.6326248427773702,4.7374333346619821E-2,-5.8285660758903743]
[null,"HP2-6",1,79.325042587181144,15.01,4292.3922865389768,212.94183040398485,6.1789928663809937,88501.569355956352]
[null,"From_Buffer",1,307,1.05,0,0,0,0]
[null,"LPbypass-2",1,306.03107160706776,15.5,406.02037270443418,20.142315886673853,0.58447523410515989,32108.614711688148]
[null,"LPbypass-3",1,306.928788694204,1.05,406.02037270443418,20.142315886673853,0.58447523410515989,32108.614711688148]
[null,"GHe",1,4.5104397521046167,1.3134999999999999,8029.9172811849066,398.35717933106872,11.559242092962991,6047.3177852055796]
[null,"LP6-2",1,11.707708395208158,1.33,11851.177669938003,587.92656798716257,17.060030256415775,34685.726714997007]
[null,"LP4",1,31.41292642667716,1.29,11851.177669938003,587.92656798716257,17.060030256415775,95799.552464204549]
[null,"HP3-4",1,40.574857394438254,13.41,402.74193067998937,19.979675242726202,0.57975584488590892,4218.4439959973606]
[null,"HP2_TS-3",1,79.25467548007893,13.44,8439.5696474152774,418.6796752427262,12.148945661430291,173692.46957839376]
[null,"HP3-1",1,40.574857394438254,13.41,8898.6069963422633,441.45211699061713,12.80973999593631,93206.771872699028]
[null,"bypass",1,79.399874296629605,13.43,459.03734892698702,22.772441747890948,0.66079433450601976,9464.5416963492553]
[null,"bypass-2",1,79.326935966425054,14.97,459.03734892698702,22.772441747890948,0.66079433450601976,9464.5416963492553]
[null,"T2Outlet",1,11.788119499088168,1.35,3827.3076631825429,189.86938865609389,5.5094933476638799,11279.272230484112]
[null,"HP8",0,4.7180000000000177,4.87,8077.9963868293371,400.74234174789115,11.628453020335717,-779.93854024564484]
[null,"LP-3",1,297.61394869545461,1.1300000000000001,12329.130930046373,611.63741155898629,17.748054460059667,945436.17972026381]
[null,"HP8-1",0,4.7180000000000177,8.1449999999999996,403.15364438795439,20.0001,0.58034851580102653,-12.602640312675387]
[null,"HP7-2",1,7.07015857373176,8.15,403.15364438795439,20.0001,0.58034851580102653,249.46190781247702]
[null,"HP7-3",1,7.2195731480463792,13.15,8092.7114212743209,401.47234174789094,11.649635635249373,5007.5777774296948]
[null,"to_damper",0.16257190498883456,4.5084021139440438,1.3134999999999999,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,-5.3012936498694436E-5]
[null,22,"<empty>","<empty>","<empty>","<empty>","<empty>","<empty>","<empty>"]
[null,"WaterInlet","<empty>",303,"<empty>","<empty>","<empty>","<empty>","<empty>"]
[null,"LP-2",1,307,1.1300000000000001,477.95326010837084,23.710843571823705,0.68802420364389161,37806.539339037117]
[null,"HP_BP1-b",1,306.03542159212702,15.43,1017.3531348473286,50.47,1.4645021571131049,80453.597968400238]
[null,"HP_BP1-a",1,306.04163583935269,15.33,1017.3531348473286,50.47,1.4645021571131049,80453.597968400238]
[null,"HP_BP1",1,306.04163583935269,15.33,1017.3531348473286,50.47,1.4645021571131049,80453.597968400238]
[null,"HP2_MEF",1,87.120658313991157,15.345000000000001,0,0,0,0]
[null,"HP2_MEF-2",1,87.121415465472182,15.33,0,0,0,0]
[null,"HP2-1",1,87.120658313991157,15.345000000000001,11842.011260075134,587.47183040398477,17.046835008318205,268139.37810028618]
[null,"HP2-2",1,87.12393937684709,15.280000000000001,11842.011260075134,587.47183040398477,17.046835008318205,268139.37810028618]
[null,"HP_BP2",1,88.781392757884589,15.280000000000001,1017.3531348473286,50.47,1.4645021571131049,23472.681914289409]
[null,"HP2-3",1,87.255050163604039,15.280000000000001,12859.364394922464,637.9418304039848,18.511337165431314,291612.0600145756]
[null,"to_TS-3",1,79.325515926774244,15,8566.9700926253445,424.99989999999997,12.332341397322249,176635.83549914221]
[null,"HP_CD2-1",1,79.325042587181144,15.01,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,4.1561382837770611E-2]
[null,"HP_CD2",1,79.325515926774244,15,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,4.1561382837770604E-2]
[null,"HP_CD1",1,305.54615477145393,15,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,0.15914088206109941]
[null,"to_TS-2",1,79.325568839981031,15,8566.9721083834884,425,12.33234429905032,176635.99464002429]
[null,"bypass_TS",1,79.325568839981031,15,0,0,0,0]
[null,"bypass_TS-1",1,79.396610001984925,13.5,0,0,0,0]
[null,"to_TS-4",1,79.325042587181144,15.01,8566.9700926253445,424.99989999999997,12.332341397322249,176635.83549914221]
[null,"bypass_HP_BP-2",1,87.740762412366507,1.2650000000000001,0,0,0,0]
[null,"HP2_TS",1,87.120658313991157,13.47,8566.9721083834884,425,12.33234429905032,193772.43176562918]
[null,"bypass_HP_BP",1,87.120658313991157,13.47,0,0,0,0]
[null,"LIN",5.9124305183460714E-2,78.456627644318417,1.1499999999999999,686.56857857456919,238.35358266718188,1.06411277231373,-25616.606028479338]
[null,"GAN-a",1,78.068329195532272,1.0999999999999999,645.97568840555164,224.26109270399618,1.0011978440138345,17440.211443762386]
[null,"GAN",1,78.456627644318417,1.1499999999999999,40.592890169017643,14.092489963185688,6.2914928299895395E-2,1100.0197950530587]
[null,"N2-a",5.0050966404227943E-3,83.590696744165257,1.99,686.56857857456919,238.35358266718188,1.06411277231373,-25616.606028479338]
[null,"N2",0,83.644048867120603,2,686.56857857456919,238.35358266718191,1.06411277231373,-25816.606028479342]
[null,"to_TS-1",1,79.325568839981031,15,8566.9721083834884,425,12.33234429905032,176635.99464002429]
[null,"HP_CD2-2",1,79.325568839981031,15,0,0,0,0]
[null,"HP2_TS-4",1,79.255148717964175,13.43,8439.5696474152774,418.6796752427262,12.148945661430291,173692.46957839376]
[null,"HP_CD2-3",1,79.399927247704909,13.43,0,0,0,0]
[null,"HP2-10",1,79.255148717964175,13.43,8439.5696474152774,418.6796752427262,12.148945661430291,173692.46957839376]
[null,"supply_loop",0,4.7462969827008124,8.1349999999999998,403.15162862981123,20,0.58034561407295615,-10.602587299738888]
[null,"supply_loop1-1",0,4.8976720550753612,6.7019999999999991,201.57581431490732,10.000000000000085,0.29017280703648057,-5.3012936498694891]
[null,"CP1_outlet-2",0,4.7512660689832273,6.7019999999999991,9151.5419698967162,454.00000000000006,13.173845439456107,-508.62109060116057]
[null,"supply_loop2",0,4.7462969827008124,8.1349999999999998,201.57581431490394,9.9999999999999165,0.29017280703647563,-5.3012936498694003]
[null,"CP2_outlet-2",0,4.7704262835385975,6.4510000000000005,19552.853988545845,970,28.146762282538372,-1110.5028916880528]
[null,"HP8-2",0,4.7462969827008124,8.1349999999999998,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,-5.3012936498694443E-5]
[null,"supply_loop1",0,4.7462969827008124,8.1349999999999998,201.57581431490732,10.000000000000085,0.29017280703648057,-5.3012936498694891]
[null,"supply_loop2-2",0,4.9199222119801789,6.4510000000000005,201.57581431490394,10.000000000000028,0.29017280703647563,-5.3012936498694003]
[null,"return-1",0,4.6104401840179321,6.1639999999999997,201.57581431490689,10.000000000000064,0.29017280703647991,-18.91352685203605]
[null,"return-2",0,4.6104401840179321,5.5080000000000009,201.57581431490561,10,0.29017280703647808,-21.584719780314099]
[null,"return-3",0,4.6436646225379832,5.5080000000000009,403.15162862981248,20.000000000000064,0.58034561407295804,-40.498246632350146]
[null,"CD_return",0,4.6436646225379832,5.5080000000000009,0,0,0,0]
[null,"baking_return",0,4.6436646225379832,5.5080000000000009,0,0,0,0]
[null,"LP5-1",1,17.297258737955303,1.3,11851.177669938003,587.92656798716257,17.060030256415775,52258.55671712097]
[null,"baking_return-1",8.5660074276668968E-2,4.4984756127961418,1.3,0,0,0,0]
[null,"LP2-1",1,78.223942316800446,1.2650000000000001,11851.177669938003,587.92656798716257,17.060030256415775,238987.47292800268]
[null,"CD_return-2",9.6339225979878401E-2,4.463275069898998,1.2650000000000001,0,0,0,0]
[null,"CL_inlet-2",1,49.780821748681291,13.41,530.1443916482018,26.3,0.76315448250593731,6840.4791234295944]
[null,"return_4",0,4.6436646225379832,5.5080000000000009,0,0,0,0]
[null,"return_damper",0,4.6436646225379832,5.5080000000000009,403.15162862981248,20.000000000000064,0.58034561407295804,-40.498246632350146]
[null,"HP7-5",1,7.2195731480463792,13.15,403.15364438795439,20.0001,0.58034851580102653,249.46190781247702]
[null,"return_damper-1",8.2352926634343515E-2,4.5095130314038556,1.3135000000000003,403.15162862981248,20.000000000000064,0.58034561407295804,-40.498246632350138]
[null,1,0,4.7462969827008124,8.1349999999999998,403.15364438795439,20.0001,0.58034851580102653,-10.602640312675387]
[null,"CP1_inlet-1",0,4.6104401840179321,6.1639999999999997,9151.5419698967162,454.00000000000006,13.173845439456107,-858.67411908243128]
[null,"CP2_Inlet-1",0,4.6104401840179321,5.5080000000000009,19552.853988545845,970,28.146762282538372,-2093.717818690468]
[null,"HP1-3",1,306.03542159212702,15.43,11842.011260075134,587.47183040398477,17.046835008318205,936481.52290632832]
[null,"LP2-2",1,78.223942316800446,1.2650000000000001,11851.177669938003,587.92656798716257,17.060030256415775,238987.47292800268]
[null,"VLP2",1,78.223950819591408,0.45500000000000002,477.95326010837084,23.710843571823705,0.68802420364389161,9633.567774552861]
[null,"HP1_TS",1,99.287827149001885,13.5,8566.9721083834884,425,12.33234429905032,220735.99461334318]
[null,"HP2",1,87.120658313991157,15.345000000000001,11842.011260075134,587.47183040398477,17.046835008318205,268139.37810028618]
[null,"LP1",1,297.23541314855333,1.1300000000000001,11851.177669938003,587.92656798716257,17.060030256415775,907629.64038122667]
[null,"VLP1",1,297.23541319850835,0.40500000000000003,477.95326010837084,23.710843571823705,0.68802420364389161,36598.784292002463]
[null,"HP2_TS-1",1,87.120658313991157,13.47,8566.9721083834884,425,12.33234429905032,193772.43176562918]
[null,"LP1a",1,97.979258632190749,1.1300000000000001,11851.177669938003,587.92656798716257,17.060030256415775,299302.76458009367]
[null,"VLP1a",1,97.979243102475948,0.40500000000000003,477.95326010837084,23.710843571823705,0.68802420364389161,12065.911661901326]
[null,"HP1a",1,98.696221747400415,15.43,11842.011260075134,587.47183040398477,17.046835008318205,303628.74992950168]
[null,3,"<empty>","<empty>","<empty>",403.15162862981123,20,0.58034561407295615,"<empty>"]
[null,4,"<empty>","<empty>","<empty>",403.15162862981123,20,0.58034561407295615,"<empty>"]

{"sheet":"Dump_Case_C","index":7,"n_rows":194,"n_cols":9,"rows_kept":194,"cut":false,"hidden":true,"merged":[]}
[]
[]
[]
[null,"Case:","03-1800s\\(03)-JT60-CALCULC-OFFCase_A.HSC"]
[null,"Flowsheet:","Case (Main)"]
[null,"Current Flowsheet Environment:","Case (Main)"]
[]
[null,"Name","Vapour Fraction","Temperature","Pressure","Molar Flow","Mass Flow","Liquid Volume Flow","Heat Flow"]
[null,null,"<none>","K","bar","Nm3/h(gas)","g/s","m3/h","W*"]
[]
[null,"HP1-2",1,306.03542159212702,15.43,12206.794837279933,605.56842490092799,17.571948970616095,965329.07864744659]
[null,"LP2",1,78.59573863471627,1.2650000000000001,10860.013685828664,538.75578886973722,15.633227956348378,220040.69518194819]
[null,"HP3-2",1,45.043475648905087,13.41,7896.4348604958468,391.73523308505082,11.367091219937821,92044.595657805476]
[null,"LP3",1,41.90362579048508,1.28,10860.013685828664,538.75578886973722,15.633227956348378,117252.90429788877]
[null,"T1Inlet",1,45.0465561671991,14.77,3639.8227288964445,180.56842490092799,5.2396046715657771,42452.588146629751]
[null,"MP4",1,35.02753635920439,6.3669324941690775,3633.7754544669974,180.26842490092801,5.2308994873546828,32727.224654684498]
[null,"HP4",1,36.070937661824672,13.39,7896.4348604958468,391.73523308505082,11.367091219937821,73233.696967246637]
[null,"MP5",1,20.343059215737924,6.3169324941690776,3633.7754544669974,180.26842490092801,5.2308994873546828,18477.155396197286]
[null,"LP5",1,18.951195869891933,1.3,10860.013685828664,538.75578886973722,15.633227956348378,52595.546666192764]
[null,"HP6",1,13.06446348302012,13.16,7896.4348604958468,391.73523308505082,11.367091219937821,21239.241553307267]
[null,"LP6",1,12.931857404894913,1.33,7232.2855057911138,358.78736396880925,10.41103365320479,23537.086079488527]
[null,"HP7",1,8.3310445500848118,13.15,7896.4348604958468,391.73523308505082,11.367091219937821,7638.5085287107759]
[null,"LP7",1,6.5339382780915116,1.335,7232.2855057911138,358.78736396880925,10.41103365320479,10702.117049948312]
[null,"HP7-4",1,6.539297091796584,4.88,7478.5661816629045,371.00513308505077,10.765560089223133,4935.82664296444]
[null,"LP8",1,4.7847335581524248,1.34,7232.2855057911138,358.78736396880925,10.41103365320479,6330.0716698372917]
[null,"JT2-3",0.32236372531207524,4.2995557455670905,1.089,1293.3855290457934,64.163725863721012,1.8618568443794998,109.1340775005343]
[null,"LHe 3,6K",0,3.6017715941583788,0.53,0,0,0,0]
[null,"HP5",1,20.343059215737924,13.370000000000001,7896.4348604958468,391.73523308505082,11.367091219937821,38978.316342316124]
[null,"GHe 4,3K",1,4.3005872176408388,1.089,7201.430199863632,357.25665920482999,10.366616763393994,5516.2519242490416]
[null,"LHe 4,3K",0,4.3005872176408388,1.089,0,0,0,0]
[null,"GHe 3,6K",1,3.6017715941583788,0.53,470.50631678953641,23.341407221329757,0.67730416535947757,347.81760490036106]
[null,"HP8-3",1,5.4252927455846134,4.8600000000000003,7478.5661816629045,371.00513308505077,10.765560089223133,631.0310444439624]
[null,"HP8-5",1,5.4252927455846134,4.8600000000000003,6185.1806526171104,306.84140722132975,8.9037032448436317,521.89696694342808]
[null,"VLP0",0.16926223137622748,3.6013106108128454,0.53,470.50631678953641,23.341407221329757,0.67730416535947757,-97.914428516176841]
[null,"MP",1,1169.6866103573188,16,12833.697191390766,636.66850286620775,18.474388662839953,3869639.9937386736]
[null,"MP-1",1,306,16,12833.697191390766,636.66850286620775,18.474388662839953,1014905.3253168447]
[null,"TS_inlet",1,79.328774337133439,15,8566.9721083834884,425,12.33234429905032,176643.11763698576]
[null,"TS_outlet",1,99.291044028561402,13.5,8566.9721083834884,425,12.33234429905032,220743.11769192221]
[null,"To Comp LP",1,299.66848657867644,1.05,12833.697191390766,636.66850286620775,18.474388662839953,990903.5219449494]
[null,"LIN-a",0,78.456570365576738,1.1499999999999999,689.79007157384319,239.47197698622918,1.069105764934458,-28528.754064201592]
[null,"GAN-b",1,78.083445858788878,1.0999999999999999,732.9270342611793,254.44768359845716,1.1359637517210317,19792.083211465331]
[null,"HP2-5",1,79.328248071566662,15.01,12206.794837279933,605.56842490092799,17.571948970616095,251692.76074607516]
[null,"to_CL-1",1,79.256095211223084,13.41,74.061186977358361,3.6741107671607147,0.10661270346699725,1524.2329885794911]
[null,"CL_inlet",1,49.999994962515302,4,530.1443916482018,26.3,0.76315448250593731,6840.5554685205016]
[null,"CL_outlet",1,300,1.05,530.1443916482018,26.3,0.76315448250593731,40978.289286214262]
[null,"GAN-c",1,305.54143732955237,1.0499999999999998,732.9270342611793,254.44768359845716,1.1359637517210317,80639.434021732508]
[null,"After Comp",1,306.03107160706776,15.5,12833.697191390766,636.66850286620775,18.474388662839953,1014905.3253168447]
[null,"LPbypass",1,306.03107160706776,15.5,385.0109157417229,19.100055085986234,0.55423165988519851,30447.159759505335]
[null,"Paliers",1,306.03107160706776,15.5,241.89097717788673,12,0.3482073684437737,19129.050438296072]
[null,"Recycle",1,307,1.05,268.70056048176917,13.330000000000002,0.3868003517796253,21254.115816195532]
[null,"To recycle",1,277.49446030863908,1.33,268.70056048176917,13.330000000000002,0.3868003517796253,19213.072534729366]
[null,"T1Outlet",1,35.02753635920439,6.3669324941690775,3639.8227288964445,180.56842490092799,5.2396046715657771,32781.688809468127]
[null,"T1Leak",1,35.02753635920439,6.3669324941690775,6.0472744294471683,0.3,8.7051842110943429E-3,54.46415478363015]
[null,"T2Outlet-1",1,13.034530227763923,1.33,3633.7754544669974,180.26842490092801,5.2308994873546828,11925.400535226097]
[null,"T2Leak",1,13.034530227763923,1.33,6.0472744294471683,0.3,8.7051842110943429E-3,19.846072114592552]
[null,"T3Outlet",1,6.539297091796584,4.88,7493.2812161078928,371.73513308505079,10.786742704136795,4945.5385124995128]
[null,"T3Leak",1,6.539297091796584,4.88,14.715034444988106,0.73,2.1182614913662894E-2,9.7118695350720081]
[null,"ColdComp_Outlet",1,4.7890911692025497,1.35,7232.2855057911138,358.78736396880925,10.41103365320479,6315.0716698372926]
[null,"VLP9-1",1,3.6610712458892181,0.53,470.50631678953641,23.341407221329757,0.67730416535947757,357.81760490036106]
[null,"HP9",0,4.1538860204182129,4.7700000000000005,470.50631678953641,23.341407221329753,0.67730416535947757,-97.914428516176827]
[null,"VLP8",1,4.1006180779543797,0.51,470.50631678953641,23.341407221329757,0.67730416535947757,429.96583626016911]
[null,"HP2-9",1,79.255148717964175,13.43,8352.5180651666888,414.36112231788991,12.023632998976757,171900.88482547982]
[null,"HP2_TS-2",1,79.25467548007893,13.44,8426.5792521440453,418.03523308505066,12.130245702443755,173425.11781405931]
[null,"HP8-4",1,5.4252927455846134,4.8600000000000003,1293.3855290457934,64.163725863721012,1.8618568443794998,109.13407750053425]
[null,"VLP7",1,6.5339565381873967,0.495,470.50631678953641,23.341407221329757,0.67730416535947757,758.26782581780492]
[null,"VLP6",1,12.931923586035339,0.49,470.50631678953641,23.341407221329757,0.67730416535947757,1554.0318208740871]
[null,"VLP5",1,18.951194061221656,0.47500000000000003,470.50631678953641,23.341407221329757,0.67730416535947757,2290.2000501121838]
[null,"VLP4",1,35.470323453567715,0.47000000000000003,470.50631678953641,23.341407221329757,0.67730416535947757,4298.4670511263812]
[null,"VLP3",1,41.903626113611239,0.46500000000000002,470.50631678953641,23.341407221329757,0.67730416535947757,5079.1909923927014]
[null,"LP",1,550.78735854784463,1.18,568.12408070423646,28.18413918530435,0.81782707813065592,80616.733504577016]
[null,"CryoPumps_Inlet",0,3.6999999999999886,4.7,5714.6743358275735,283.5,8.2263990794841533,-1619.9808315339767]
[null,"CryoPumps_Outlet",0,3.8727213200608617,4.2,5714.6743358275735,283.5,8.2263990794841533,-1538.0808315339766]
[null,"LP9-2",0,4.1006253736028384,4.1950000000000003,5714.6743358275735,283.5,8.2263990794841533,-1317.7818185719507]
[null,"HP9-1",0,4.1538860204182129,4.7700000000000005,5714.6743358275735,283.5,8.2263990794841533,-1189.2487981174388]
[null,"HP1",1,306.03107160706776,15.5,12206.794837279933,605.56842490092799,17.571948970616095,965329.07864744659]
[null,"LP-4",1,299.1233824483802,1.05,11470.912858857642,569.0619630060163,16.512630718314419,884070.78113167372]
[null,"To Comp VLP",1,300.20462968887642,0.35000000000000003,568.12408070423646,28.18413918530435,0.81782707813065592,43937.559305469076]
[null,"to_TS",1,79.328774337133439,15,8566.9721083834884,425,12.33234429905032,176643.11763698576]
[null,"to_CL-2",1,79.25467548007893,13.44,74.061186977358361,3.6741107671607147,0.10661270346699725,1524.2329885794911]
[null,"HP2-7",1,79.330141509144482,14.97,3639.8227288964445,180.56842490092799,5.2396046715657771,75049.76068446807]
[null,"HP2-8",1,79.330141509144482,14.97,3639.8227288964445,180.56842490092799,5.2396046715657771,75049.76068446807]
[null,"HP5-1",1,20.37501888473551,13.19,7896.4348604958468,391.73523308505082,11.367091219937821,39078.316342316131]
[null,"Piston",1,4.3005872176408388,1.089,30.855305927481655,1.5307047639792195,4.4416889810795973E-2,23.634977493635446]
[null,"To Buffer",1,306.03107160706776,15.5,4.6119122324858055E-4,2.2879293570809978E-5,6.638948838453577E-7,3.6471596725717259E-2]
[null,"VLP8-1",1,4.1928491279184072,0.5,470.50631678953641,23.341407221329757,0.67730416535947757,444.96583626016906]
[null,"HP2-4",1,79.25467548007893,15.23,12206.794837279933,605.56842490092799,17.571948970616095,251492.76074607522]
[null,"CP1_Inlet",0,4.4005872176408616,3.93,17658.04133398573,876,25.41913789639548,-3168.890943038145]
[null,"CP1_Outlet",0,4.6473540957409796,5.37,17658.04133398573,876,25.41913789639548,-1807.251964908804]
[null,"TF_Inlet",0,4.4005872176408616,5.3,17859.61714830064,886.00000000000011,25.70931070343196,-2709.3767273327167]
[null,"TF_Outlet",0,4.8958879854714041,4,17859.61714830064,886.00000000000011,25.70931070343196,-1186.8767273327167]
[null,"HP9-0",0,4.1538860204182129,4.7700000000000005,6185.1806526171104,306.84140722132975,8.9037032448436317,-1287.1632266336157]
[null,"CP2_Inlet",0,4.4005872176408616,3.93,19351.278174230942,960,27.856589475501899,-3472.7571978500227]
[null,"CP2_outlet",0,4.5626832753798681,4.87,19351.278174230942,960,27.856589475501899,-2495.3273739790552]
[null,"PF_Inlet",0,4.4005872176408616,4.8,19552.853988545845,970,28.146762282538372,-3172.1130099044599]
[null,"PF_Outlet",0,4.6762262886298345,4,19552.853988545845,970,28.146762282538372,-2332.1130099044599]
[null,"HP8-6",0,4.4005872176408616,4.79,6185.1806526171104,306.84140722132975,8.9037032448436317,-1004.7159823117819]
[null,"MP6",1,13.034530227763923,1.33,3627.7281800375499,179.96842490092803,5.2221943031435893,11905.554463111504]
[null,"LP9-3",9.6707030242842371E-3,4.2971447652554957,1.0889999999999997,5714.6743358275735,283.5,8.2263990794841533,-1317.7818185719507]
[null,"HP3-3",1,45.043475648905087,14.950000000000001,3639.8227288964445,180.56842490092799,5.2396046715657771,42452.588146629751]
[null,"GHe1-3",0.99807902472181076,4.2834637322512208,1.069,7232.2855057911138,358.78736396880925,10.41103365320479,5539.8869017426769]
[null,"T3Inlet",1,8.3277757468866866,13.07,7493.2812161078928,371.73513308505079,10.786742704136795,7248.523351166381]
[null,"LP-1",1,307,1.1300000000000001,568.12408070423646,28.18413918530435,0.81782707813065592,44939.133591700833]
[null,"VLP1-1",1,298.78471779089165,0.35000000000000003,470.50631678953641,23.341407221329757,0.67730416535947757,36215.905035775133]
[null,"VLPbypass",1,307,1.1300000000000001,97.617763914700006,4.8427319639745896,0.14052291277117832,7721.6542696939478]
[null,"VLP-2",1,307.04844129479807,0.35000000000000003,97.617763914700006,4.8427319639745896,0.14052291277117832,7721.6542696939478]
[null,"Conso.liq",0,4.2993665145158388,1.089,-209.78330939769208,-10.407166658891159,-0.30198767627068923,50.284507668723649]
[null,"HP2-6",1,79.328248071566691,15.01,3639.8227288964445,180.56842490092799,5.2396046715657771,75049.76068446807]
[null,"From_Buffer",1,307,1.05,178.92846466142919,8.8764847742052879,0.25757145035477064,14153.175951361996]
[null,"LPbypass-2",1,306.03107160706776,15.5,385.01091574172301,19.100055085986238,0.55423165988519862,30447.159759503873]
[null,"LPbypass-3",1,306.928788694204,1.05,385.01091574172301,19.100055085986238,0.55423165988519862,30447.159759503873]
[null,"GHe",1,4.3005870925301792,1.089,7232.2855057911138,358.78736396880925,10.41103365320479,5539.8869017426769]
[null,"LP6-2",1,12.966148435236164,1.33,10860.013685828664,538.75578886973722,15.633227956348378,35442.640542600035]
[null,"LP4",1,35.47032197407799,1.29,10860.013685828664,538.75578886973722,15.633227956348378,99192.729548596282]
[null,"HP3-4",1,45.043475648905087,13.41,456.08320467084343,22.625889232839285,0.65654177903894018,5316.3224799410091]
[null,"HP2_TS-3",1,79.25467548007893,13.44,8352.5180651666869,414.36112231788991,12.023632998976757,171900.88482547985]
[null,"HP3-1",1,45.043475648905087,13.41,8352.5180651666906,414.36112231789002,12.02363299897676,97360.918137746485]
[null,"bypass",1,79.403082089572251,13.43,0,0,0,0]
[null,"bypass-2",1,79.330141509144482,14.97,0,0,0,0]
[null,"T2Outlet",1,13.038795438384682,1.35,3633.7754544669974,180.26842490092801,5.2308994873546828,11925.400535226097]
[null,"HP8",1,5.4189999999999827,4.87,7478.5661816629045,371.00513308505077,10.765560089223133,616.0310444439624]
[null,"LP-3",1,299.11840465130558,1.1300000000000001,11470.912858857642,569.0619630060163,16.512630718314419,884070.78113167372]
[null,"HP8-1",1,5.4189999999999827,8.1449999999999996,403.15364438795439,20.0001,0.58034851580102653,44.433406396215496]
[null,"HP7-2",1,7.8463092739419835,8.15,403.15364438795439,20.0001,0.58034851580102653,389.98517754439473]
[null,"HP7-3",1,8.3310445500848118,13.15,7493.2812161078928,371.73513308505079,10.786742704136795,7248.523351166381]
[null,"to_damper",0.35310088835396053,4.2992716542823928,1.089,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,2.3216587115172169E-4]
[null,22,"<empty>","<empty>","<empty>","<empty>","<empty>","<empty>","<empty>"]
[null,"WaterInlet","<empty>",303,"<empty>","<empty>","<empty>","<empty>","<empty>"]
[null,"LP-2",1,307,1.1300000000000001,470.50631678953641,23.341407221329757,0.67730416535947757,37217.479322006882]
[null,"HP_BP1-b",1,306.03542159212702,15.43,1088.5093973004903,54,1.5669331579969816,86080.726972332312]
[null,"HP_BP1-a",1,306.04163583935269,15.33,1088.5093973004903,54,1.5669331579969816,86080.726972332312]
[null,"HP_BP1",1,306.04163583935269,15.33,1088.5093973004903,54,1.5669331579969816,86080.726972332312]
[null,"HP2_MEF",1,87.998922503771496,15.345000000000001,0,0,0,0]
[null,"HP2_MEF-2",1,87.999684305576295,15.33,0,0,0,0]
[null,"HP2-1",1,87.998922503771496,15.345000000000001,11118.285439979441,551.56842490092799,16.005015812619114,254281.10057002166]
[null,"HP2-2",1,88.002223718560316,15.280000000000001,11118.285439979441,551.56842490092799,16.005015812619114,254281.10057002166]
[null,"HP_BP2",1,89.269713798201622,15.280000000000001,1088.5093973004903,54,1.5669331579969816,25252.054826994681]
[null,"HP2-3",1,88.115238315613567,15.280000000000001,12206.794837279933,605.56842490092799,17.571948970616095,279533.15539701632]
[null,"to_TS-3",1,79.328721425742685,15,8566.9700926253445,424.99989999999997,12.332341397322249,176642.95849854831]
[null,"HP_CD2-1",1,79.328248071566691,15.01,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,4.1563058838025212E-2]
[null,"HP_CD2",1,79.328721425742685,15,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,4.1563058838025205E-2]
[null,"HP_CD1",1,305.54144585004047,15,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,0.15913843745626555]
[null,"to_TS-2",1,79.328774337133439,15,8566.9721083834884,425,12.33234429905032,176643.11763698576]
[null,"bypass_TS",1,79.328774337133439,15,0,0,0,0]
[null,"bypass_TS-1",1,79.39981769064326,13.5,0,0,0,0]
[null,"to_TS-4",1,79.328248071566691,15.01,8566.9700926253445,424.99989999999997,12.332341397322249,176642.95849854831]
[null,"bypass_HP_BP-2",1,88.622838980307108,1.2650000000000001,140.39285623944281,6.9647669149493501,0.20209859660656446,3207.396573327705]
[null,"HP2_TS",1,87.998922503771496,13.47,8426.5792521440453,418.03523308505066,12.130245702443755,192512.51197643139]
[null,"bypass_HP_BP",1,87.998922503771496,13.47,140.39285623944281,6.9647669149493501,0.20209859660656446,3207.396573327705]
[null,"LIN",5.8855739617818738E-2,78.456570365576738,1.1499999999999999,732.9270342611793,254.44768359845716,1.1359637517210317,-27359.793852534331]
[null,"GAN-a",1,78.068329195532272,1.0999999999999999,689.79007157384319,239.47197698622918,1.069105764934458,18623.122999798066]
[null,"GAN",1,78.456570365576738,1.1499999999999999,43.13696268733613,14.975706612227937,6.6857986786573606E-2,1168.960211667265]
[null,"N2-a",4.6852276315149403E-3,83.594396814769027,1.99,732.9270342611793,254.44768359845716,1.1359637517210317,-27359.793852534331]
[null,"N2",0,83.644048867120603,2,732.9270342611793,254.44768359845716,1.1359637517210317,-27559.793852534331]
[null,"to_TS-1",1,79.328774337133439,15,8566.9721083834884,425,12.33234429905032,176643.11763698576]
[null,"HP_CD2-2",1,79.328774337133439,15,0,0,0,0]
[null,"HP2_TS-4",1,79.255148717964175,13.43,8352.5180651666869,414.36112231788991,12.023632998976757,171900.88482547982]
[null,"HP_CD2-3",1,79.403135038826434,13.43,0,0,0,0]
[null,"HP2-10",1,79.255148717964175,13.43,8352.5180651666888,414.36112231788991,12.023632998976757,171900.88482547982]
[null,"supply_loop",1,5.4417815395868274,8.1349999999999998,403.15162862981123,20,0.58034561407295615,46.433174230344342]
[null,"supply_loop1-1",1,5.5328549009391281,5.37,201.57581431490732,10.000000000000085,0.29017280703648057,23.21658711517237]
[null,"CP1_outlet-2",0,4.6594516754739175,5.37,17859.61714830064,886.00000000000011,25.70931070343196,-1784.0353777936316]
[null,"supply_loop2",1,5.4417815395868274,8.1349999999999998,201.57581431490394,9.9999999999999165,0.29017280703647563,23.216587115171976]
[null,2,0,4.5750900177736185,4.87,19552.853988545845,970,28.146762282538372,-2472.1107868638833]
[null,"HP8-2",1,5.4417815395868274,8.1349999999999998,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,2.3216587115172169E-4]
[null,"supply_loop1",1,5.4417815395868274,8.1349999999999998,201.57581431490732,10.000000000000085,0.29017280703648057,23.21658711517237]
[null,"supply_loop2-2",1,5.5212402645545353,4.87,201.57581431490394,10.000000000000028,0.29017280703647563,23.216587115171976]
[null,"return-1",0,4.4005872176408616,3.93,201.57581431490803,10.000000000000121,0.29017280703648152,-36.174554144271504]
[null,"return-2",0,4.4005872176408616,3.93,201.57581431490561,10,0.29017280703647808,-36.174554144271063]
[null,"return-3",0,4.4005872236788832,3.93,403.15162862981362,20.000000000000117,0.58034561407295959,-72.349108288542567]
[null,"CD_return",0,4.4005872236788832,3.93,0,0,0,0]
[null,"baking_return",0,4.4005872236788832,3.93,0,0,0,0]
[null,"LP5-1",1,18.951195869891933,1.3,10860.013685828664,538.75578886973722,15.633227956348378,52595.546666192764]
[null,"baking_return-1",1.4894375759560657E-3,4.4974872515857101,1.3,0,0,0,0]
[null,"LP2-1",1,78.59573863471627,1.2650000000000001,10860.013685828664,538.75578886973722,15.633227956348378,220040.69518194819]
[null,"CD_return-2",1.1640100226630461E-2,4.4668217583389378,1.2650000000000001,0,0,0,0]
[null,"CL_inlet-2",1,49.781370253742267,13.41,530.1443916482018,26.3,0.76315448250593731,6840.5554685205016]
[null,"return_4",0,4.4005872236788832,3.93,0,0,0,0]
[null,"return_damper",0,4.4005872236788832,3.93,403.15162862981362,20.000000000000117,0.58034561407295959,-72.349108288542567]
[null,"HP7-5",1,8.3310445500848118,13.15,403.15364438795439,20.0001,0.58034851580102653,389.98517754439473]
[null,"return_damper-1",6.0148170702049794E-2,4.2986149866002279,1.0889999999999997,403.15162862981362,20.000000000000117,0.58034561407295959,-72.349108288542567]
[null,1,1,5.4417815395868274,8.1349999999999998,403.15364438795439,20.0001,0.58034851580102653,46.433406396215496]
[null,"CP1_inlet-1",0,4.4005872176408616,3.93,17859.61714830064,886.00000000000011,25.70931070343196,-3205.0654971824169]
[null,"CP2_Inlet-1",0,4.4005872176408616,3.93,19552.853988545845,970,28.146762282538372,-3508.9317519942933]
[null,"HP1-3",1,306.03542159212702,15.43,11118.285439979441,551.56842490092799,16.005015812619114,879248.35167511425]
[null,"LP2-2",1,78.723698120571328,1.2650000000000001,11000.406542068107,545.72055578468655,15.835326552954943,223248.09175527591]
[null,"VLP2",1,78.595737106613797,0.45500000000000002,470.50631678953641,23.341407221329757,0.67730416535947757,9528.539333904946]
[null,"TS_outlet-2",1,99.291044026159,13.5,8566.9721083834884,425,12.33234429905032,220743.11769192221]
[null,"HP2",1,87.998922503771496,15.345000000000001,11118.285439979441,551.56842490092799,16.005015812619114,254281.10057002166]
[null,"LP1",1,298.78129536733121,1.1300000000000001,11000.406542068107,545.72055578468655,15.835326552954943,846853.30180966679]
[null,"VLP1",1,298.78129534522259,0.40500000000000003,470.50631678953641,23.341407221329757,0.67730416535947757,36215.905035775133]
[null,"HP2_TS-1",1,87.998922503771496,13.47,8566.9721083834884,425,12.33234429905032,195719.9085497591]
[null,"LP1a",1,98.625209150979913,1.1300000000000001,11000.406542068107,545.72055578468655,15.835326552954943,279647.41056797444]
[null,"VLP1a",1,98.625208433488808,0.40500000000000003,470.50631678953641,23.341407221329757,0.67730416535947757,11956.214352542358]
[null,"HP1a",1,99.640283872288137,15.43,11118.285439979441,551.56842490092799,16.005015812619114,287786.73443238321]

{"sheet":"Dump_Case_D","index":8,"n_rows":194,"n_cols":9,"rows_kept":194,"cut":false,"hidden":true,"merged":[]}
[]
[]
[]
[null,"Case:","03-1800s\\(03)-JT60-CALCULD-OFFCase_A.hsc"]
[null,"Flowsheet:","Case (Main)"]
[null,"Current Flowsheet Environment:","Case (Main)"]
[]
[null,"Name","Vapour Fraction","Temperature","Pressure","Molar Flow","Mass Flow","Liquid Volume Flow","Heat Flow"]
[null,null,"<none>","K","bar","Nm3/h(gas)","g/s","m3/h","W*"]
[]
[null,"HP1-2",1,306.03542159212702,15.43,12096.965157500015,600.11987046233151,17.413846737042235,956643.60592480376]
[null,"LP2",1,78.765470906926453,1.2650000000000001,10343.73144972636,513.14347829284623,14.890028350869727,210032.55169227373]
[null,"HP3-2",1,47.95265865994179,13.41,7599.229689848702,376.99114428366084,10.939257856468377,94402.79584005737]
[null,"LP3",1,44.680396774079469,1.28,10343.73144972636,513.14347829284634,14.890028350869727,119097.35259893761]
[null,"T1Inlet",1,47.956529029344466,14.77,3529.9930491165319,175.11987046233179,5.081502437991924,43882.558047567298]
[null,"MP4",1,37.343775251063789,6.3925093081630973,3523.9457746870848,174.81987046233181,5.0727972537808306,33881.207655665145]
[null,"HP4",1,38.896372197436818,13.39,7599.2296898487029,376.9911442836609,10.93925785646838,76206.746465385309]
[null,"MP5",1,21.73297255752874,6.3425093081630974,3523.9457746870848,174.81987046233181,5.0727972537808306,19255.013170645019]
[null,"LP5",1,20.199182456827799,1.3,10343.73144972636,513.14347829284634,14.890028350869727,53469.981596656144]
[null,"HP6",1,14.041457873583056,13.16,7599.2296898487048,376.99114428366096,10.939257856468382,22916.011403846805]
[null,"LP6",1,13.894978794068493,1.33,6825.8329494687223,338.62360783051452,9.8259362812999935,23963.341944585918]
[null,"HP7",1,8.832961959414547,13.15,7599.2296898487048,376.99114428366096,10.939257856468382,8715.2777643170703]
[null,"LP7",1,6.7839552831377432,1.335,6825.8329494687223,338.62360783051452,9.8259362812999935,10614.631907805631]
[null,"HP7-4",1,6.763902332840189,4.88,7181.3610110157615,356.26104428366102,10.337726725753694,5797.8848592475852]
[null,"LP8",1,4.7850125992403036,1.34,6825.8329494687223,338.62360783051452,9.8259362812999935,5975.166291515432]
[null,"JT2-3",0.41065716303042338,4.298983238307585,1.089,996.18035841031497,49.419637062909885,1.4340234809268531,172.26097564481032]
[null,"LHe 3,6K",0,3.6017715941583788,0.53,0,0,0,0]
[null,"HP5",1,21.73297255752874,13.370000000000001,7599.2296898487039,376.9911442836609,10.939257856468382,40556.150900371045]
[null,"GHe 4,3K",1,4.3005872176408388,1.089,6776.1384375937578,336.15830652222712,9.7543999412183471,5190.4810097391874]
[null,"LHe 4,3K",0,4.3005872176408388,1.089,0,0,0,0]
[null,"GHe 3,6K",1,3.6017715941583788,0.53,470.50631677787362,23.341407220751176,0.67730416534268878,347.81760489173939]
[null,"HP8-3",1,5.682793436068323,4.8600000000000003,7181.3610110157615,356.26104428366102,10.337726725753694,1241.8115291785771]
[null,"HP8-5",1,5.682793436068323,4.8600000000000003,6185.180652605447,306.84140722075114,8.9037032448268398,1069.5505535337668]
[null,"VLP0",0.16926223137468024,3.6013106108127317,0.53,470.50631677787362,23.341407220751176,0.67730416534268878,-97.914428514590199]
[null,"MP",1,1172.8651932390358,16,12720.463505119351,631.0510786401785,18.311386287241785,3845911.79977126]
[null,"MP-1",1,306,16,12720.463505119351,631.0510786401785,18.311386287241785,1005950.6593707596]
[null,"TS_inlet",1,79.329347834827729,15,8566.9721083834884,425,12.33234429905032,176644.39201671409]
[null,"TS_outlet",1,99.291619547763162,13.5,8566.9721083834884,425,12.33234429905032,220744.39205445888]
[null,"To Comp LP",1,300.4829014987115,1.05,12720.463505119351,631.0510786401785,18.311386287241785,984829.24402067519]
[null,"LIN-a",0,78.456539775049492,1.1499999999999999,715.7104634079443,248.47066764961809,1.1092797852359824,-29600.800976594939]
[null,"GAN-b",1,78.083407209171696,1.0999999999999999,760.35248793403468,263.96888125182147,1.1784704676566404,20532.673206382369]
[null,"HP2-5",1,79.328821566825354,15.01,12096.965157500023,600.11987046233173,17.413846737042242,249429.97434326354]
[null,"to_CL-1",1,79.256095211223084,13.41,31.221488834185362,1.5488707779897914,4.4944018138607149E-2,642.56090370493507]
[null,"CL_inlet",1,49.999738834479245,4,530.1443916482018,26.3,0.76315448250593731,6840.5202833507055]
[null,"CL_outlet",1,300,1.05,530.1443916482018,26.3,0.76315448250593731,40978.289286214262]
[null,"GAN-c",1,305.54126977384868,1.0499999999999998,760.35248793403468,263.96888125182147,1.1784704676566404,83656.841242597467]
[null,"After Comp",1,306.03107160706776,15.5,12720.463505119351,631.0510786401785,18.311386287241785,1005950.6593707596]
[null,"LPbypass",1,306.03107160706776,15.5,381.61390515358056,18.931532359205352,0.54934158861725368,30178.519781122792]
[null,"Paliers",1,306.03107160706776,15.5,241.89097717788673,12,0.3482073684437737,19129.050438296072]
[null,"Recycle",1,307,1.05,268.70056048176917,13.330000000000002,0.3868003517796253,21254.115816195532]
[null,"To recycle",1,277.60230498169892,1.33,268.70056048176917,13.330000000000002,0.3868003517796253,19220.537094589963]
[null,"T1Outlet",1,37.343775251063789,6.3925093081630973,3529.9930491165319,175.11987046233179,5.081502437991924,33939.349572083564]
[null,"T1Leak",1,37.343775251063789,6.3925093081630973,6.0472744294471683,0.3,8.7051842110943429E-3,58.141916418417907]
[null,"T2Outlet-1",1,14.041082149880822,1.33,3523.9457746870848,174.81987046233181,5.0727972537808306,12508.087895032108]
[null,"T2Leak",1,14.041082149880822,1.33,6.0472744294471683,0.3,8.7051842110943429E-3,21.464530082226332]
[null,"T3Outlet",1,6.763902332840189,4.88,7196.0760454607498,356.99104428366104,10.358909340667356,5809.7650690408309]
[null,"T3Leak",1,6.763902332840189,4.88,14.715034444988106,0.73,2.1182614913662894E-2,11.880209793245831]
[null,"ColdComp_Outlet",1,4.7890911692025497,1.35,6825.8329494687223,338.62360783051452,9.8259362812999935,5960.166291515432]
[null,"VLP9-1",1,3.661071245890696,0.53,470.50631677787362,23.341407220751176,0.67730416534268878,357.81760489173939]
[null,"HP9",0,4.1538860204080379,4.7700000000000005,470.50631677787368,23.341407220751176,0.67730416534268878,-97.914428514590213]
[null,"VLP8",1,4.1006180676567965,0.51,470.50631677787362,23.341407220751176,0.67730416534268878,429.96583625177357]
[null,"HP2-9",1,79.255148717964175,13.43,8098.1525926627173,401.74227350567105,11.657468320835708,166665.8587589291]
[null,"HP2_TS-2",1,79.25467548007893,13.44,8129.3740814969024,403.29114428366086,11.702412338974316,167308.41966263403]
[null,"HP8-4",1,5.682793436068323,4.8600000000000003,996.18035841031497,49.419637062909885,1.4340234809268531,172.26097564481029]
[null,"VLP7",1,6.7838979427074264,0.495,470.50631677787362,23.341407220751176,0.67730416534268878,790.13732695922783]
[null,"VLP6",1,13.895060632975458,0.49,470.50631677787362,23.341407220751176,0.67730416534268878,1672.1609297086668]
[null,"VLP5",1,20.199183245051017,0.47500000000000003,470.50631677787362,23.341407220751176,0.67730416534268878,2442.2841391125589]
[null,"VLP4",1,38.156629043746563,0.47000000000000003,470.50631677787362,23.341407220751176,0.67730416534268878,4624.515778105495]
[null,"VLP3",1,44.680396715750135,0.46500000000000002,470.50631677787362,23.341407220751176,0.67730416534268878,5416.069826714308]
[null,"LP",1,552.08426236274431,1.18,566.78970963235008,28.117942202475756,0.81590622169818405,80616.736764028989]
[null,"CryoPumps_Inlet",0,3.6999999999999886,4.7,5714.6743358275735,283.5,8.2263990794841533,-1619.9808315339767]
[null,"CryoPumps_Outlet",0,3.8727213200608617,4.2,5714.6743358275735,283.5,8.2263990794841533,-1538.0808315339766]
[null,"LP9-2",0,4.1006253736130134,4.1950000000000003,5714.6743358275735,283.5,8.2263990794841533,-1317.7818185616604]
[null,"HP9-1",0,4.1538860204080379,4.7700000000000005,5714.6743358275735,283.5,8.2263990794841533,-1189.2487981276472]
[null,"HP1",1,306.03107160706776,15.5,12096.965157500015,600.11987046233151,17.413846737042235,956643.60592480376]
[null,"LP-4",1,299.96449685600982,1.05,11251.835793390817,558.19374122993668,16.197264476288417,869624.26841013262]
[null,"To Comp VLP",1,300.91153292684658,0.35000000000000003,566.78970963235008,28.117942202475756,0.81590622169818405,43937.572264666618]
[null,"to_TS",1,79.329347834827729,15,8566.9721083834884,425,12.33234429905032,176644.39201671409]
[null,"to_CL-2",1,79.25467548007893,13.44,31.221488834185362,1.5488707779897914,4.4944018138607149E-2,642.56090370493507]
[null,"HP2-7",1,79.330715014839086,14.97,3529.9930491165319,175.11987046233179,5.081502437991924,72785.699901527856]
[null,"HP2-8",1,79.330715014839086,14.97,3529.9930491165319,175.11987046233179,5.081502437991924,72785.699901527856]
[null,"HP5-1",1,21.768778024677232,13.19,7599.2296898487048,376.99114428366096,10.939257856468382,40656.150900371045]
[null,"Piston",1,4.3005872176408388,1.089,49.694511874964583,2.4653013082874544,7.1536340081647248E-2,38.065695167062948]
[null,"To Buffer",1,306.03107160706776,15.5,-6.5347121287704941E-3,-3.241813583132469E-4,-9.4068614730653155E-6,-0.51677346286078596]
[null,"VLP8-1",1,4.1928491279364835,0.5,470.50631677787362,23.341407220751176,0.67730416534268878,444.96583625177357]
[null,"HP2-4",1,79.25467548007893,15.23,12096.965157500019,600.11987046233162,17.413846737042238,249229.97434326363]
[null,"CP1_Inlet",0,4.4005872176408616,4.6420000000000003,8949.9661555818093,444,12.883672632419628,-1480.9934898377328]
[null,"CP1_Outlet",0,4.5396416125327619,5.1779999999999999,8949.9661555818093,444,12.883672632419628,-1141.8552254362739]
[null,"TF_Inlet",0,4.4005872176408616,5.16,9151.5419698967162,454.00000000000006,13.173845439456107,-1415.6550181471371]
[null,"TF_Outlet",0,5.1881963855285562,4.66,9151.5419698967162,454.00000000000006,13.173845439456107,137.72733479404286]
[null,"HP9-0",0,4.1538860204080379,4.7700000000000005,6185.180652605447,306.84140722075114,8.9037032448268398,-1287.1632266422375]
[null,"CP2_Inlet",0,4.4005872176408616,3.93,19351.278174230942,960,27.856589475501899,-3472.7571978500227]
[null,"CP2_outlet",0,4.5626832753798681,4.87,19351.278174230942,960,27.856589475501899,-2495.3273739790552]
[null,"PF_Inlet",0,4.4005872176408616,4.8,19552.853988545845,970,28.146762282538372,-3172.1130099044599]
[null,"PF_Outlet",0,4.6762262886298345,4,19552.853988545845,970,28.146762282538372,-2332.1130099044599]
[null,"HP8-6",0,4.4005872176408616,4.79,6185.180652605447,306.84140722075114,8.9037032448268398,-1004.7159823098872]
[null,"MP6",1,14.041082149880822,1.33,3517.8985002576378,174.5198704623318,5.0640920695697362,12486.623364949879]
[null,"LP9-3",9.2258467519393851E-3,4.2987502214414235,1.0889999999999997,5714.6743358275735,283.5,8.2263990794841533,-1317.7818185616602]
[null,"HP3-3",1,47.95265865994179,14.950000000000001,3529.9930491165319,175.11987046233179,5.081502437991924,43882.558047567298]
[null,"GHe1-3",0.99807902472180998,4.2834637322512208,1.069,6825.8329494687223,338.62360783051452,9.8259362812999935,5228.5467049062499]
[null,"T3Inlet",1,8.8278263516534707,13.07,7196.0760454607498,356.99104428366104,10.358909340667356,8252.9156386885588]
[null,"LP-1",1,307,1.1300000000000001,566.78970963235008,28.117942202475756,0.81590622169818405,44833.5836213738]
[null,"VLP1-1",1,299.65568941382156,0.35000000000000003,470.50631677787362,23.341407220751176,0.67730416534268878,36321.46796437716]
[null,"VLPbypass",1,307,1.1300000000000001,96.28339285447646,4.7765349817245779,0.13860205635549533,7616.1043002894585]
[null,"VLP-2",1,307.04844129479807,0.35000000000000003,96.28339285447646,4.7765349817245779,0.13860205635549533,7616.1043002894594]
[null,"Conso.liq",0,4.2993665145158388,1.089,-337.86990103208637,-16.761430540682802,-0.48637113499368806,80.986526898911421]
[null,"HP2-6",1,79.328821566825354,15.01,3529.9930491165319,175.11987046233179,5.081502437991924,72785.699901527856]
[null,"From_Buffer",1,307,1.05,288.16865234048186,14.295795024808841,0.41482509711668991,22794.034744327004]
[null,"LPbypass-2",1,306.03107160706776,15.5,381.61410725808025,18.931542385432973,0.5493418795511148,30178.535763805819]
[null,"LPbypass-3",1,306.928788694204,1.05,381.61410725808025,18.931542385432973,0.5493418795511148,30178.535763805819]
[null,"GHe",1,4.3005870925301792,1.089,6825.8329494687223,338.62360783051452,9.8259362812999935,5228.5467049062499]
[null,"LP6-2",1,13.944658257295146,1.33,10343.73144972636,513.14347829284634,14.890028350869727,36449.965309535801]
[null,"LP4",1,38.156683741013836,1.29,10343.73144972636,513.14347829284634,14.890028350869727,101662.85727287436]
[null,"HP3-4",1,47.95265865994179,13.41,498.92290281401642,24.75112922201021,0.71821046436733005,6197.9593796457702]
[null,"HP2_TS-3",1,79.25467548007893,13.44,8098.1525926627173,401.74227350567099,11.657468320835708,166665.85875892907]
[null,"HP3-1",1,47.95265865994179,13.41,8098.1525926627173,401.74227350567105,11.657468320835708,100600.75521970313]
[null,"bypass",1,79.403655997831663,13.43,0,0,0,0]
[null,"bypass-2",1,79.330715014839086,14.97,0,0,0,0]
[null,"T2Outlet",1,14.044886923949662,1.35,3523.9457746870848,174.81987046233181,5.0727972537808306,12508.087895032108]
[null,"HP8",1,5.6779999999999973,4.87,7181.3610110157615,356.26104428366102,10.337726725753694,1226.8115291785773]
[null,"LP-3",1,299.95952004247681,1.1300000000000001,11251.835793390817,558.19374122993668,16.197264476288417,869624.26841013262]
[null,"HP8-1",1,5.6779999999999973,8.1449999999999996,403.15364438795439,20.0001,0.58034851580102653,68.798348699866608]
[null,"HP7-2",1,8.2381730085236313,8.15,403.15364438795439,20.0001,0.58034851580102653,462.36212562851006]
[null,"HP7-3",1,8.832961959414547,13.15,7196.0760454607498,356.99104428366104,10.358909340667356,8252.9156386885588]
[null,"to_damper",0.41318596968491073,4.2993964724463467,1.089,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,3.5398997354946525E-4]
[null,22,"<empty>","<empty>","<empty>","<empty>","<empty>","<empty>","<empty>"]
[null,"WaterInlet","<empty>",303,"<empty>","<empty>","<empty>","<empty>","<empty>"]
[null,"LP-2",1,307,1.1300000000000001,470.50631677787362,23.341407220751176,0.67730416534268878,37217.479321084342]
[null,"HP_BP1-b",1,306.03542159212702,15.43,1131.0418941209352,56.11,1.6281596202816784,89444.251674399376]
[null,"HP_BP1-a",1,306.04163583935264,15.33,1131.0418941209355,56.110000000000007,1.6281596202816782,89444.251674399376]
[null,"HP_BP1",1,306.04163583935264,15.33,1131.0418941209355,56.110000000000007,1.6281596202816786,89444.251674399376]
[null,"HP2_MEF",1,88.5200027980664,15.345000000000001,0,0,0,0]
[null,"HP2_MEF-2",1,88.520767301819177,15.33,0,0,0,0]
[null,"HP2-1",1,88.5200027980664,15.345000000000001,10965.92326337908,544.00987046233149,15.785687116760554,252276.28868542984]
[null,"HP2-2",1,88.523315721573965,15.280000000000001,10965.92326337908,544.00987046233149,15.785687116760554,252276.28868542984]
[null,"HP_BP2",1,89.619144923060162,15.280000000000001,1131.0418941209355,56.110000000000007,1.6281596202816786,26341.084668901374]
[null,"HP2-3",1,88.625765449936694,15.280000000000001,12096.965157500017,600.11987046233151,17.413846737042235,278617.37335433124]
[null,"to_TS-3",1,79.329294923610263,15,8566.9700926253445,424.99989999999997,12.332341397322249,176644.23287837702]
[null,"HP_CD2-1",1,79.328821566825354,15.01,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,4.1563358692173105E-2]
[null,"HP_CD2",1,79.329294923610263,15,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,4.1563358692173105E-2]
[null,"HP_CD1",1,305.54125249486987,15,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,0.15913833707723082]
[null,"to_TS-2",1,79.329347834827729,15,8566.9721083834884,425,12.33234429905032,176644.39201671409]
[null,"bypass_TS",1,79.329347834827729,15,0,0,0,0]
[null,"bypass_TS-1",1,79.400391580397979,13.5,0,0,0,0]
[null,"to_TS-4",1,79.328821566825354,15.01,8566.9700926253445,424.99989999999997,12.332341397322249,176644.23287837702]
[null,"bypass_HP_BP-2",1,89.146132617338878,1.2650000000000001,437.59802688658527,21.708855716339126,0.62993196007600172,10056.320500776927]
[null,"HP2_TS",1,88.5200027980664,13.47,8129.3740814969024,403.2911442836608,11.702412338974316,186818.92104470098]
[null,"bypass_HP_BP",1,88.5200027980664,13.47,437.59802688658527,21.708855716339126,0.62993196007600172,10056.320500776927]
[null,"LIN",5.871227520723693E-2,78.456539775049492,1.1499999999999999,760.35248793403468,263.96888125182147,1.1784704676566404,-28391.055921204024]
[null,"GAN-a",1,78.068329195532272,1.0999999999999999,715.7104634079443,248.47066764961809,1.1092797852359824,19322.928150991447]
[null,"GAN",1,78.456539775049492,1.1499999999999999,44.64202452609041,15.498213602203412,6.9190682420657984E-2,1209.7450553909205]
[null,"N2-a",4.5463563322817556E-3,83.593453507063998,1.99,760.35248793403468,263.96888125182147,1.1784704676566404,-28391.055921204024]
[null,"N2",0,83.644048867120603,2,760.35248793403468,263.96888125182147,1.1784704676566404,-28591.055921204024]
[null,"to_TS-1",1,79.329347834827729,15,8566.9721083834884,425,12.33234429905032,176644.39201671409]
[null,"HP_CD2-2",1,79.329347834827729,15,0,0,0,0]
[null,"HP2_TS-4",1,79.255148717964175,13.43,8098.1525926627173,401.74227350567105,11.657468320835708,166665.8587589291]
[null,"HP_CD2-3",1,79.403708946911735,13.43,0,0,0,0]
[null,"HP2-10",1,79.255148717964175,13.43,8098.1525926627173,401.74227350567105,11.657468320835708,166665.8587589291]
[null,"supply_loop",1,5.6987717047147157,8.1349999999999998,403.15162862981123,20,0.58034561407295615,70.797994709893047]
[null,"supply_loop1-1",1,5.7097717785969166,5.1779999999999999,201.57581431490732,10.000000000000085,0.29017280703648057,35.398997354946822]
[null,"CP1_outlet-2",0,4.5733395946256223,5.1779999999999999,9151.5419698967162,454.00000000000006,13.173845439456107,-1106.456228081327]
[null,"supply_loop2",1,5.6987717047147157,8.1349999999999998,201.57581431490394,9.9999999999999165,0.29017280703647563,35.398997354946225]
[null,2,0,4.5781524209469922,4.87,19552.853988545845,970,28.146762282538372,-2459.9283766241092]
[null,"HP8-2",1,5.6987717047147157,8.1349999999999998,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,3.5398997354946525E-4]
[null,"supply_loop1",1,5.6987717047147157,8.1349999999999998,201.57581431490732,10.000000000000085,0.29017280703648057,35.398997354946822]
[null,"supply_loop2-2",1,5.6905277260837579,4.87,201.57581431490394,10.000000000000028,0.29017280703647563,35.398997354946225]
[null,"return-1",0,4.4005872176408616,4.6420000000000003,201.57581431490689,10.000000000000064,0.29017280703647991,-33.355709230579784]
[null,"return-2",0,4.4005872176408616,3.93,201.57581431490561,10,0.29017280703647808,-36.174554144271063]
[null,"return-3",0,4.4349372224796184,3.93,403.15162862981248,20.000000000000064,0.58034561407295804,-69.530263374850847]
[null,"CD_return",0,4.4349372224796184,3.93,0,0,0,0]
[null,"baking_return",0,4.4349372224796184,3.93,0,0,0,0]
[null,"LP5-1",1,20.199182456827799,1.3,10343.73144972636,513.14347829284634,14.890028350869727,53469.981596656144]
[null,"baking_return-1",9.4229823129669908E-3,4.4962293561546858,1.3,0,0,0,0]
[null,"LP2-1",1,78.765470906926453,1.2650000000000001,10343.73144972636,513.14347829284623,14.890028350869727,210032.55169227373]
[null,"CD_return-2",1.9502753381903364E-2,4.4654298768693366,1.2650000000000001,0,0,0,0]
[null,"CL_inlet-2",1,49.781117464127021,13.41,530.1443916482018,26.3,0.76315448250593731,6840.5202833507055]
[null,"return_4",0,4.4349372224796184,3.93,0,0,0,0]
[null,"return_damper",0,4.4349372224796184,3.93,403.15162862981248,20.000000000000064,0.58034561407295804,-69.530263374850847]
[null,"HP7-5",1,8.832961959414547,13.15,403.15364438795439,20.000099999999996,0.58034851580102642,462.36212562851006]
[null,"return_damper-1",6.7296312945847162E-2,4.2979544376769354,1.0889999999999997,403.15162862981248,20.000000000000064,0.58034561407295804,-69.530263374850833]
[null,1,1,5.6987717047147157,8.1349999999999998,403.15364438795439,20.0001,0.58034851580102653,70.798348699866608]
[null,"CP1_inlet-1",0,4.4005872176408616,4.6420000000000003,9151.5419698967162,454.00000000000006,13.173845439456107,-1514.3491990683126]
[null,"CP2_Inlet-1",0,4.4005872176408616,3.93,19552.853988545845,970,28.146762282538372,-3508.9317519942933]
[null,"HP1-3",1,306.03542159212702,15.43,10965.92326337908,544.00987046233149,15.785687116760554,867199.35425040429]
[null,"LP2-2",1,79.186768802284689,1.2650000000000001,10781.329476612944,534.85233400918537,15.519960310945729,220088.87219305066]
[null,"VLP2",1,78.765472497017413,0.45500000000000002,470.50631677787362,23.341407220751176,0.67730416534268878,9549.1161265648461]
[null,"TS_outlet-2",1,99.291619545360788,13.5,8566.9721083834884,425,12.33234429905032,220744.39205445888]
[null,"HP2",1,88.5200027980664,15.345000000000001,10965.92326337908,544.00987046233149,15.785687116760554,252276.28868542984]
[null,"LP1",1,299.6522676452775,1.1300000000000001,10781.329476612944,534.85233400918548,15.519960310945729,832406.78908904816]
[null,"VLP1",1,299.65226766957397,0.40500000000000003,470.50631677787362,23.341407220751176,0.67730416534268878,36321.46796437716]
[null,"HP2_TS-1",1,88.5200027980664,13.47,8566.9721083834884,425,12.33234429905032,196875.24154547791]
[null,"LP1a",1,99.200831130008794,1.1300000000000001,10781.329476612944,534.85233400918537,15.519960310945729,275677.24305451539]
[null,"VLP1a",1,99.200796535813652,0.40500000000000003,470.50631677787362,23.341407220751176,0.67730416534268878,12025.983953390296]
[null,"HP1a",1,100.46237505439291,15.43,10965.92326337908,544.00987046233149,15.785687116760554,286173.96795642929]

{"sheet":"Dump_Case_E","index":9,"n_rows":191,"n_cols":9,"rows_kept":191,"cut":false,"hidden":true,"merged":[]}
[null,"Case:","1800\\(03)-JT60-CALCULE-OFFCase_A.HSC"]
[null,"Flowsheet:","Case (Main)"]
[null,"Current Flowsheet Environment:","Case (Main)"]
[]
[null,"Name","Vapour Fraction","Temperature","Pressure","Molar Flow","Mass Flow","Liquid Volume Flow","Heat Flow"]
[null,null,"<none>","K","bar","Nm3/h(gas)","g/s","m3/h","W*"]
[]
[null,"HP1-2",1,306.03542159212702,15.43,12460.544423803167,618.15672014783809,17.937227067376078,985395.92320663866]
[null,"LP2",1,78.381744161961677,1.2650000000000001,11276.920341132605,559.43816372313313,16.233374233087435,227865.84944852602]
[null,"HP3-2",1,42.177990163639492,13.41,8169.8754491508989,405.30038174062707,11.760714946263388,89045.490940642499]
[null,"LP3",1,39.17480153371983,1.28,11276.920341132605,559.43816372313313,16.233374233087435,113802.47260013444]
[null,"T1Inlet",1,42.180187324198357,14.77,3760.5245830040653,186.55633840721097,5.4133576386067537,41005.294115173652]
[null,"MP4",1,32.772458133977239,6.3573729374331274,3754.4773085746183,186.25633840721099,5.4046524543956602,31584.947169338277]
[null,"HP4",1,33.315713091595569,13.39,8169.8754491508989,405.30038174062707,11.760714946263388,69725.758988549991]
[null,"MP5",1,19.090124723132902,6.3073729374331275,3754.4773085746183,186.25633840721099,5.4046524543956602,17795.964808208191]
[null,"LP5",1,17.830043444131007,1.3,11276.920341132605,559.43816372313313,16.233374233087435,51302.73004766443]
[null,"HP6",1,12.245550984576653,13.16,8169.8754491508989,405.30038174062707,11.760714946263388,19668.890017473666]
[null,"LP6",1,12.118889941863415,1.33,7528.4903069874345,373.48182531592215,10.837426962902869,22864.959974264209]
[null,"HP7",1,7.8525953768332215,13.15,8169.8754491508989,405.30038174062707,11.760714946263388,6600.6615385528848]
[null,"LP7",1,6.3170804682339963,1.335,7528.4903069874345,373.48182531592215,10.837426962902869,10640.440567269834]
[null,"HP7-4",1,6.343824075045859,4.88,7752.0067703179566,384.57028174062702,11.159183815548698,4078.12091920699]
[null,"LP8",1,4.7845492132452137,1.34,7528.4903069874345,373.48182531592215,10.837426962902869,6588.7111479119394]
[null,"JT2-3",0.24156396565834024,4.2976731589902784,1.089,1469.2688042804718,72.889141451521155,2.1150446777466803,3.7486456489120354]
[null,"LHe 3,6K",0,3.6017715941583788,0.53,0,0,0,0]
[null,"HP5",1,19.090124723132902,13.370000000000001,8169.8754491508989,405.30038174062707,11.760714946263388,37332.142016566089]
[null,"GHe 4,3K",1,4.3005872176408388,1.089,7518.3838912347992,372.98045486198237,10.822878555704383,5759.0365325004896]
[null,"LHe 4,3K",0,4.3005872176408388,1.089,0,0,0,0]
[null,"GHe 3,6K",1,3.6017715941583788,0.53,568.06363020991216,28.181140289105922,0.81774005831786512,419.93598011351941]
[null,"HP8-3",0,5.1377011916186461,4.8600000000000003,7752.0067703179566,384.57028174062702,11.159183815548698,19.778223266722147]
[null,"HP8-5",0,5.1377011916186461,4.8600000000000003,6282.7379660374854,311.68114028910588,9.0441391378020164,16.029577617810112]
[null,"VLP0",0.18199060095933919,3.6022426364509101,0.53,568.06363020991216,28.181140289105922,0.81774005831786512,-109.86019039738672]
[null,"MP",1,1171.2569032781878,16,13095.393883109216,649.6510470572299,18.851106791878351,3953843.7756878179]
[null,"MP-1",1,306,16,13095.393883109216,649.6510470572299,18.851106791878351,1035600.6372041338]
[null,"TS_inlet",1,79.327486171150071,15,8566.9721083834884,425,12.33234429905032,176640.25517916342]
[null,"TS_outlet",1,99.289750964770576,13.5,8566.9721083834884,425,12.33234429905032,220740.2544821479]
[null,"To Comp LP",1,300.07082624747306,1.05,13095.393883109216,649.6510470572299,18.851106791878351,1012466.6199822836]
[null,"LIN-a",0,78.456626020214088,1.1499999999999999,647.14136020985984,224.66577485730394,1.0030045189680912,-26764.83708748042]
[null,"GAN-b",1,78.083516183046896,1.0999999999999999,687.80193485602751,238.78176260078882,1.0660243514521721,18573.536478724298]
[null,"HP2-5",1,79.326961734517852,15.01,12460.544423803163,618.15672014783809,17.937227067376078,256920.68379250896]
[null,"to_CL-1",1,79.256095211223084,13.41,109.73128040208782,5.4436729314491821,0.15796058551071024,2258.3494039740567]
[null,"CL_inlet",1,49.999851562746244,4,530.1443916482018,26.3,0.76315448250593731,6840.535769212207]
[null,"CL_outlet",1,300,1.05,530.1443916482018,26.3,0.76315448250593731,40978.289286214262]
[null,"GAN-c",1,297.73680235964594,1.0499999999999998,687.80193485602751,238.78176260078882,1.0660243514521721,73735.163249310557]
[null,"After Comp",1,306.03107160706776,15.5,13095.393883109216,649.6510470572299,18.851106791878351,1035600.6372041338]
[null,"LPbypass",1,306.03107160706776,15.5,392.86181649327648,19.489531411716893,0.56553320375635052,31068.019116124011]
[null,"Paliers",1,306.03107160706776,15.5,241.89097717788673,12,0.3482073684437737,19129.050438296072]
[null,"Recycle",1,307,1.05,268.70056048176917,13.330000000000002,0.3868003517796253,21254.115816195532]
[null,"To recycle",1,277.39469853235437,1.33,268.70056048176917,13.330000000000002,0.3868003517796253,19206.167439263809]
[null,"T1Outlet",1,32.772458133977239,6.3573729374331274,3760.5245830040653,186.55633840721097,5.4133576386067537,31635.82052071967]
[null,"T1Leak",1,32.772458133977239,6.3573729374331274,6.0472744294471683,0.3,8.7051842110943429E-3,50.873351381391892]
[null,"T2Outlet-1",1,12.202920775747202,1.33,3754.4773085746183,186.25633840721099,5.4046524543956602,11487.339985775619]
[null,"T2Leak",1,12.202920775747202,1.33,6.0472744294471683,0.3,8.7051842110943429E-3,18.502468292908652]
[null,"T3Outlet",1,6.343824075045859,4.88,7766.7218047629449,385.30028174062704,11.18036643046236,4085.8621005004229]
[null,"T3Leak",1,6.343824075045859,4.88,14.715034444988108,0.73,2.1182614913662898E-2,7.7411812934337849]
[null,"ColdComp_Outlet",1,4.7890911692025497,1.35,7528.4903069874345,373.48182531592215,10.837426962902869,6573.7111479119403]
[null,"VLP9-1",1,3.650797319391188,0.53,568.06363020991216,28.181140289105922,0.81774005831786512,429.93598011351941]
[null,"HP9",0,4.2364785420848534,4.7700000000000005,568.06363020991216,28.181140289105922,0.81774005831786512,-109.8601903973867]
[null,"VLP8",1,4.1006196253242138,0.51,568.06363020991216,28.181140289105922,0.81774005831786512,519.11754540164816]
[null,"HP2-9",1,79.257419962386223,13.43,8590.2885603970135,426.15670880917776,12.365908843258612,176799.43145630011]
[null,"HP2_TS-2",1,79.25467548007893,13.44,8566.9721083834884,425,12.33234429905032,176314.504705826]
[null,"HP8-4",0,5.1377011916186461,4.8600000000000003,1469.2688042804718,72.889141451521155,2.1150446777466803,3.7486456489120368]
[null,"VLP7",1,6.3170606596701759,0.495,568.06363020991216,28.181140289105922,0.81774005831786512,881.95276777621598]
[null,"VLP6",1,12.118951202437756,0.49,568.06363020991216,28.181140289105922,0.81774005831786512,1755.6618397026473]
[null,"VLP5",1,17.83008110768003,0.47500000000000003,568.06363020991216,28.181140289105922,0.81774005831786512,2599.9919085909214]
[null,"VLP4",1,32.858387580296124,0.47000000000000003,568.06363020991216,28.181140289105922,0.81774005831786512,4806.8817679225504]
[null,"VLP3",1,39.174801272245759,0.46500000000000002,568.06363020991216,28.181140289105922,0.81774005831786512,5732.5687503857525]
[null,"LP",1,549.14098412602323,1.18,569.82709612995222,28.268624292384473,0.82027860619807769,80616.729341435988]
[null,"CryoPumps_Inlet",0,3.6999999999999886,4.7,5714.6743358275735,283.5,8.2263990794841533,-1619.9808315339767]
[null,"CryoPumps_Outlet",0,3.9834400609200316,4.2,5714.6743358275735,283.5,8.2263990794841533,-1433.0808315339766]
[null,"LP9-2",0,4.1006265166047342,4.1950000000000003,5714.6743358275735,283.5,8.2263990794841533,-1317.7806625814108]
[null,"HP9-1",0,4.2364785420848534,4.7700000000000005,5714.6743358275735,283.5,8.2263990794841533,-1105.1846610230707]
[null,"HP1",1,306.03107160706776,15.5,12460.544423803167,618.15672014783809,17.937227067376078,985395.92320663866]
[null,"LP-4",1,299.65501146169703,1.05,11844.983971342517,587.61930401223901,17.051114291405298,914522.79860951938]
[null,"To Comp VLP",1,299.30724056803507,0.35000000000000003,569.82709612995222,28.268624292384473,0.82027860619807769,43937.54276162896]
[null,"to_TS",1,79.327486171150071,15,8566.9721083834884,425,12.33234429905032,176640.25517916342]
[null,"to_CL-2",1,79.25467548007893,13.44,109.73128040208782,5.4436729314491812,0.15796058551071024,2258.3494039740567]
[null,"HP2-7",1,79.328855148687438,14.97,3893.5723154196771,193.156720147838,5.6048827683257585,80280.542137651297]
[null,"HP2-8",1,79.328855148687438,14.97,3760.5245830040653,186.55633840721097,5.4133576386067537,77537.265983203091]
[null,"HP5-1",1,19.11853388336354,13.19,8169.8754491508989,405.30038174062707,11.760714946263388,37432.142016566089]
[null,"Piston",1,4.3005872176408388,1.089,10.106415752635304,0.50137045393981972,1.4548407198487073E-2,7.7414532662957729]
[null,"To Buffer",1,306.03107160706776,15.5,9.6665634885265347E-2,4.7954976748476597E-3,1.3915230214474493E-4,7.6444430749077021]
[null,"VLP8-1",1,4.175173924927094,0.5,568.06363020991216,28.181140289105922,0.81774005831786512,534.11754540164816]
[null,"HP2-4",1,79.25467548007893,15.23,12460.544423803167,618.15672014783809,17.937227067376078,256720.68379250891]
[null,"CP1_Inlet",0,4.4005872176408616,4.1199999999999992,15819.669907433792,784.8,22.7727618962228,-2781.7097698121902]
[null,"CP1_Outlet",0,4.6334156882931552,5.3639999999999999,15819.669907433792,784.8,22.7727618962228,-1665.4514112291488]
[null,"TF_Inlet",0,4.4005872176408616,5.3079999999999998,16021.245721748701,794.80000000000007,23.06293470325928,-2427.7409913464967]
[null,"TF_Outlet",0,4.9801987692833336,4.1769999999999996,16021.245721748701,794.80000000000007,23.06293470325928,-694.58474134649691]
[null,"HP9-0",0,4.2364785420848534,4.7700000000000005,6282.7379660374854,311.68114028910588,9.0441391378020164,-1215.0448514204575]
[null,"CP2_Inlet",0,4.4005872176408616,4.2159999999999993,19351.278174230942,960,27.856589475501899,-3366.6674697485869]
[null,"CP2_outlet",0,4.5611029697314507,5.1570000000000009,19351.278174230942,960,27.856589475501899,-2394.6982219556153]
[null,"PF_Inlet",0,4.4005872176408616,5.0869999999999997,19552.853988545845,970,28.146762282538372,-3054.8622178070914]
[null,"PF_Outlet",0,4.8895642774887165,4.2869999999999999,19552.853988545845,970,28.146762282538372,-1277.7372178070914]
[null,"HP8-6",0,4.4005872176408616,4.79,6282.7379660374854,311.68114028910588,9.0441391378020164,-1020.5631171797629]
[null,"MP6",1,12.202920775747202,1.33,3748.4300341451712,185.95633840721098,5.395947270184565,11468.837517482712]
[null,"LP9-3",9.6751781300541372E-3,4.2971293332262803,1.0889999999999997,5714.6743358275735,283.5,8.2263990794841533,-1317.7806625814108]
[null,"HP3-3",1,42.177990163639492,14.950000000000001,3760.5245830040653,186.55633840721097,5.4133576386067537,41005.294115173652]
[null,"GHe1-3",0.99807902472180998,4.2834637322512208,1.069,7528.4903069874345,373.48182531592215,10.837426962902869,5766.7779857667856]
[null,"T3Inlet",1,7.8513888527467088,13.07,7766.7218047629449,385.30028174062704,11.18036643046236,6274.9428943456987]
[null,"LP-1",1,307,1.1300000000000001,569.82709612995222,28.268624292384473,0.82027860619807769,45073.843667059904]
[null,"VLP1-1",1,299.28320920672206,0.35000000000000003,568.06363020991216,28.181140289105922,0.81774005831786512,43798.050996965758]
[null,"VLPbypass",1,307,1.1300000000000001,1.7634659200401357,8.7484003278548855E-2,2.5385478802124974E-3,139.49176466320543]
[null,"VLP-2",1,307.04844129479807,0.35000000000000003,1.7634659200401357,8.7484003278548855E-2,2.538547880212497E-3,139.49176466320543]
[null,"Conso.liq",0,4.2993665145158388,1.089,-68.712893261202666,-3.4087865895388654,-9.8913717327479542E-2,16.470299844412441]
[null,"HP2-6",1,79.326961734517852,15.01,3893.5723154196776,193.15672014783803,5.6048827683257594,80280.542137651297]
[null,"From_Buffer",1,307,1.05,58.706132802264982,2.9123599476350437,8.4508766110587094E-2,4643.6335803064039]
[null,"LPbypass-2",1,306.03107160706776,15.5,392.85882683446562,19.489383097355816,0.56552890007690271,31067.782690048032]
[null,"LPbypass-3",1,306.928788694204,1.05,392.85882683446562,19.489383097355816,0.56552890007690271,31067.782690048032]
[null,"GHe",1,4.3005870925301792,1.089,7528.4903069874345,373.48182531592215,10.837426962902869,5766.7779857667856]
[null,"LP6-2",1,12.146816514960733,1.33,11276.920341132605,559.43816372313313,16.233374233087435,34333.797491746918]
[null,"LP4",1,32.858388726395589,1.29,11276.920341132605,559.43816372313313,16.233374233087435,95378.427630505132]
[null,"HP3-4",1,42.177990163639492,13.41,420.41311124611394,20.856327068550819,0.60519389699522719,4582.1863652381498]
[null,"HP2_TS-3",1,79.25467548007893,13.44,8457.240827981399,419.55632706855079,12.174383713539607,174056.15530185189]
[null,"HP3-1",1,42.177990163639492,13.41,8590.2885603970153,426.15670880917781,12.365908843258614,93627.677305880643]
[null,"bypass",1,79.401794826144823,13.43,133.04773241561202,6.6003817406269931,0.19152512971900496,2743.2761544482069]
[null,"bypass-2",1,79.328855148687438,14.97,133.04773241561202,6.600381740626994,0.19152512971900501,2743.2761544482073]
[null,"T2Outlet",1,12.207623137003395,1.35,3754.4773085746183,186.25633840721099,5.4046524543956602,11487.339985775619]
[null,"HP8",0,5.1299999999999955,4.87,7752.0067703179566,384.57028174062702,11.159183815548698,4.7782232667221489]
[null,"LP-3",1,299.65003428578149,1.1300000000000001,11844.983971342517,587.61930401223901,17.051114291405298,914522.79860951938]
[null,"HP8-1",0,5.1299999999999955,8.1449999999999996,403.15364438795439,20.0001,0.58034851580102653,19.496698414990785]
[null,"HP7-2",1,7.5005434574860601,8.15,403.15364438795439,20.0001,0.58034851580102653,325.71864420718498]
[null,"HP7-3",1,7.8525953768332215,13.15,7766.7218047629449,385.30028174062704,11.18036643046236,6274.9428943456987]
[null,"to_damper",0.29207679324304436,4.2977209048991654,1.089,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,1.0748295466018067E-4]
[null,22,"<empty>","<empty>","<empty>","<empty>","<empty>","<empty>","<empty>"]
[null,"WaterInlet","<empty>",303,"<empty>","<empty>","<empty>","<empty>","<empty>"]
[null,"LP-2",1,307,1.1300000000000001,568.06363020991216,28.181140289105922,0.81774005831786512,44934.351902396695]
[null,"HP_BP1-b",1,306.03542159212702,15.43,940.14959796471976,46.64,1.3533659720181339,74348.242703510739]
[null,"HP_BP1-a",1,306.04163583935269,15.33,940.14959796471976,46.64,1.3533659720181339,74348.242703510739]
[null,"HP_BP1",1,306.04163583935269,15.33,940.14959796471976,46.64,1.3533659720181339,74348.242703510739]
[null,"HP2_MEF",1,87.776438989502964,15.345000000000001,0,0,0,0]
[null,"HP2_MEF-2",1,87.7771996248091,15.33,0,0,0,0]
[null,"HP2-1",1,87.776438989502964,15.345000000000001,11520.394825838446,571.5167201478381,16.583861095357943,262813.74781718821]
[null,"HP2-2",1,87.779735149337625,15.280000000000001,11520.394825838446,571.5167201478381,16.583861095357943,262813.74781718821]
[null,"HP_BP2",1,78.583286533593338,15.280000000000001,940.14959796471976,46.64,1.3533659720181339,19206.424290852625]
[null,"HP2-3",1,87.0853054065457,15.280000000000001,12460.544423803167,618.15672014783809,17.937227067376078,282020.17210804083]
[null,"to_TS-3",1,79.327435082842101,15,8566.9700926253445,424.99989999999997,12.332341397322249,176640.1000924714]
[null,"HP_CD2-1",1,79.326961734517852,15.01,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,4.1562386271731221E-2]
[null,"HP_CD2",1,79.327435082842101,15,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,4.1562386271731221E-2]
[null,"HP_CD1",1,297.73680236359218,15,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,0.1550866920212213]
[null,"to_TS-2",1,79.327486171150071,15,8566.9721083834884,425,12.33234429905032,176640.25517916342]
[null,"bypass_TS",1,79.327486171150071,15,0,0,0,0]
[null,"bypass_TS-1",1,79.398528644004728,13.5,0,0,0,0]
[null,"to_TS-4",1,79.326961734517852,15.01,8566.9700926253445,424.99990000000008,12.332341397322249,176640.1000924714]
[null,"bypass_HP_BP-2",1,88.39939951487213,1.2650000000000001,0,0,0,0]
[null,"HP2_TS",1,87.776438989502964,13.47,8566.9721083834884,425,12.33234429905032,195226.59407101234]
[null,"bypass_HP_BP",1,87.776438989502964,13.47,0,0,0,0]
[null,"LIN",5.9116691282176941E-2,78.456626020214088,1.1499999999999999,687.80193485602751,238.78176260078882,1.0660243514521721,-25662.983148267245]
[null,"GAN-a",1,78.068329195532272,1.0999999999999999,647.14136020985984,224.66577485730394,1.0030045189680912,17471.682539511126]
[null,"GAN",1,78.456626020214088,1.1499999999999999,40.660574646167689,14.115987743484872,6.3019832484080843E-2,1101.8539392131713]
[null,"N2-a",4.997647780650108E-3,83.590653866719492,1.99,687.80193485602751,238.78176260078882,1.0660243514521721,-25662.983148267245]
[null,"N2",0,83.644048867120603,2,687.80193485602751,238.7817626007888,1.0660243514521721,-25862.983148267242]
[null,"to_TS-1",1,79.327486171150071,15,8566.9721083834884,425,12.33234429905032,176640.25517916342]
[null,"HP_CD2-2",1,79.327486171150071,15,0,0,0,0]
[null,"HP2_TS-4",1,79.255148717964175,13.43,8457.240827981399,419.55632706855079,12.174383713539607,174056.15530185189]
[null,"HP_CD2-3",1,79.401845951013115,13.43,0,0,0,0]
[null,"HP2-10",1,79.255148717964175,13.43,8457.240827981399,419.55632706855079,12.174383713539607,174056.15530185189]
[null,"supply_loop",0,5.1550293922833248,8.1349999999999998,403.15162862981123,20,0.58034561407295615,21.496590932036124]
[null,"supply_loop1-1",1,5.3171127173159221,5.3639999999999999,201.57581431490732,10.000000000000085,0.29017280703648057,10.748295466018154]
[null,"CP1_outlet-2",0,4.6432985007247112,5.3639999999999999,16021.245721748701,794.80000000000007,23.06293470325928,-1654.7031157631307]
[null,"supply_loop2",0,5.1550293922833248,8.1349999999999998,201.57581431490394,9.9999999999999165,0.29017280703647563,10.748295466017971]
[null,2,0,4.5702723107128804,5.1570000000000009,19552.853988545845,970,28.146762282538372,-2383.9499264895971]
[null,"HP8-2",0,5.1550293922833248,8.1349999999999998,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,1.0748295466018063E-4]
[null,"supply_loop1",0,5.1550293922833248,8.1349999999999998,201.57581431490732,10.000000000000085,0.29017280703648057,10.748295466018154]
[null,"supply_loop2-2",1,5.3203297266544496,5.1570000000000009,201.57581431490394,10.000000000000028,0.29017280703647563,10.748295466017971]
[null,"return-1",0,4.4005872176408616,4.1199999999999992,201.57581431490803,10.000000000000121,0.29017280703648152,-35.444823774365744]
[null,"return-2",0,4.4005872176408616,4.2159999999999993,201.57581431490561,10,0.29017280703647808,-35.069452809881106]
[null,"return-3",0,4.4052509981457888,4.1199999999999992,403.15162862981362,20.000000000000117,0.58034561407295959,-70.514276584246858]
[null,"CD_return",0,4.4052509981457888,4.1199999999999992,0,0,0,0]
[null,"baking_return",0,4.4052509981457888,4.1199999999999992,0,0,0,0]
[null,"LP5-1",1,17.830043444131007,1.3,11276.920341132605,559.43816372313313,16.233374233087435,51302.73004766443]
[null,"baking_return-1",6.5781382561908809E-3,4.4968776985310797,1.3,0,0,0,0]
[null,"LP2-1",1,78.381744161961677,1.2650000000000001,11276.920341132605,559.43816372313313,16.233374233087435,227865.84944852602]
[null,"CD_return-2",1.655826016698695E-2,4.4664941725744143,1.2650000000000001,0,0,0,0]
[null,"CL_inlet-2",1,49.781228723068097,13.41,530.1443916482018,26.3,0.76315448250593731,6840.535769212207]
[null,"return_4",0,4.4052509981457888,4.1199999999999992,0,0,0,0]
[null,"return_damper",0,4.4052509981457888,4.1199999999999992,403.15162862981362,20.000000000000117,0.58034561407295959,-70.514276584246858]
[null,"HP7-5",1,7.8525953768332215,13.15,403.15364438795439,20.0001,0.58034851580102653,325.71864420718498]
[null,"return_damper-1",6.4179882382960879E-2,4.300338998150778,1.0889999999999997,403.15162862981362,20.000000000000117,0.58034561407295959,-70.514276584246844]
[null,1,0,5.1550293922833248,8.1349999999999998,403.15364438795439,20.0001,0.58034851580102653,21.496698414990785]
[null,"CP1_inlet-1",0,4.4005872176408616,4.1199999999999992,16021.245721748701,794.80000000000007,23.06293470325928,-2817.1545935865556]
[null,"CP2_Inlet-1",0,4.4005872176408616,4.2159999999999993,19552.853988545845,970,28.146762282538372,-3401.736922558468]
[null,"HP1-3",1,306.03542159212702,15.43,11520.394825838446,571.5167201478381,16.583861095357943,911047.68050312786]
[null,"LP2-2",1,78.381744161961677,1.2650000000000001,11276.920341132605,559.43816372313313,16.233374233087435,227865.84944852602]
[null,"VLP2",1,78.381751138447243,0.45500000000000002,568.06363020991216,28.181140289105922,0.81774005831786512,11472.917920442562]
[null,"HP1_TS",1,99.289750962368174,13.5,8566.9721083834884,425,12.33234429905032,220740.2544821479]
[null,"HP2",1,87.776438989502964,15.345000000000001,11520.394825838446,571.5167201478381,16.583861095357943,262813.74781718821]
[null,"LP1",1,299.27978719765315,1.1300000000000001,11276.920341132605,559.43816372313313,16.233374233087435,869588.44670712273]
[null,"VLP1",1,299.27978716212272,0.40500000000000003,568.06363020991216,28.181140289105922,0.81774005831786512,43798.050996965758]
[null,"HP2_TS-1",1,87.776438989502964,13.47,8566.9721083834884,425,12.33234429905032,195226.59407101234]
[null,"LP1a",1,98.758938103341052,1.1300000000000001,11276.920341132605,559.43816372313313,16.233374233087435,287065.40542776708]
[null,"VLP1a",1,98.758937412440616,0.40500000000000003,568.06363020991216,28.181140289105922,0.81774005831786512,14454.851165570131]
[null,"HP1a",1,99.972213235457616,15.43,11520.394825838446,571.5167201478381,16.583861095357943,299183.75171371276]

{"sheet":"Dump_Case_D2","index":10,"n_rows":194,"n_cols":9,"rows_kept":194,"cut":false,"hidden":true,"merged":[]}
[]
[]
[]
[null,"Case:","3000s\\(02)-JT60-CALCULD2-3000S-OFFCase_A.HSC"]
[null,"Flowsheet:","Case (Main)"]
[null,"Current Flowsheet Environment:","Case (Main)"]
[]
[null,"Name","Vapour Fraction","Temperature","Pressure","Molar Flow","Mass Flow","Liquid Volume Flow","Heat Flow"]
[null,null,"<none>","K","bar","Nm3/h(gas)","g/s","m3/h","W*"]
[]
[null,"HP1-2",1,306.03542159212702,15.43,12068.880640490366,598.72662211529644,17.373418458666425,954422.64609951153]
[null,"LP2",1,78.816791306767726,1.2650000000000001,10218.433492003709,506.9275561025529,14.709659191841951,207623.5101440289]
[null,"HP3-2",1,48.734381899369396,13.41,7523.397259425109,373.22916367694359,10.830095409201585,95006.842621471427]
[null,"LP3",1,45.461423069819972,1.28,10218.433492003709,506.9275561025529,14.709659191841951,119715.55519989763]
[null,"T1Inlet",1,48.738448280838668,14.77,3501.9085321068769,173.72662211529644,5.0410741596161053,44254.620327431126]
[null,"MP4",1,38.109081849077086,6.4008119036825404,3495.8612576774299,173.42662211529645,5.0323689754050118,34312.55062666587]
[null,"HP4",1,39.660441792738794,13.39,7523.397259425109,373.22916367694359,10.830095409201585,76975.044063341746]
[null,"MP5",1,22.104340272999593,6.3508119036825406,3495.8612576774299,173.42662211529645,5.0323689754050118,19454.063017639986]
[null,"LP5",1,20.527592708511094,1.3,10218.433492003709,506.9275561025529,14.709659191841951,53698.600409644219]
[null,"HP6",1,14.279360426494918,13.16,7523.397259425109,373.22916367694359,10.830095409201585,23272.358423315945]
[null,"LP6",1,14.129280301850713,1.33,6728.6195087557271,333.80093398725649,9.6859954006480322,24040.340199007671]
[null,"HP7",1,8.9574289736403898,13.15,7523.397259425109,373.22916367694359,10.830095409201585,8973.8941419173007]
[null,"LP7",1,6.8585666034487645,1.335,6728.6195087557271,333.80093398725649,9.6859954006480322,10613.125487354826]
[null,"HP7-4",1,6.8325997545469477,4.88,7105.5285805921667,352.49906367694354,10.228564278486894,6040.3276748172721]
[null,"LP8",1,4.7850843431276644,1.34,6728.6195087557271,333.80093398725649,9.6859954006480322,5890.2816661943707]
[null,"JT2-3",0.43490122193910075,4.2996909043073401,1.089,920.34792737951693,45.657656426069636,1.3248610327859716,181.80981331609902]
[null,"LHe 3,6K",0,3.6017715941583788,0.53,0,0,0,0]
[null,"HP5",1,22.104340272999593,13.370000000000001,7523.397259425109,373.22916367694359,10.830095409201585,40949.854995566544]
[null,"GHe 4,3K",1,4.3005872176408388,1.089,6675.2379407353428,331.15272104554953,9.6091514623554897,5113.19184015681]
[null,"LHe 4,3K",0,4.3005872176408388,1.089,0,0,0,0]
[null,"GHe 3,6K",1,3.6017715941583788,0.53,470.50631738507764,23.341407250874038,0.67730416621677225,347.81760534060965]
[null,"HP8-3",1,5.7453865055148867,4.8600000000000003,7105.5285805921667,352.49906367694354,10.228564278486894,1403.6591883549222]
[null,"HP8-5",1,5.7453865055148867,4.8600000000000003,6185.1806532126493,306.84140725087394,8.9037032457009229,1221.8493750388234]
[null,"VLP0",0.1692622314551607,3.6013106108186435,0.53,470.50631738507764,23.341407250874038,0.67730416621677225,-97.91442859719416]
[null,"MP",1,1173.4933240308192,16,12691.504714384801,629.61445833764003,18.26969947265847,3839209.6918891901]
[null,"MP-1",1,306,16,12691.504714384801,629.61445833764003,18.26969947265847,1003660.5608517649]
[null,"TS_inlet",1,79.329496160058028,15,8566.9721083834884,425,12.33234429905032,176644.7216128975]
[null,"TS_outlet",1,99.291768391580888,13.5,8566.9721083834884,425,12.33234429905032,220744.72163682172]
[null,"To Comp LP",1,300.64384085666757,1.05,12691.504714384801,629.61445833764003,18.26969947265847,983113.38347128639]
[null,"LIN-a",0,78.456533759698061,1.1499999999999999,721.03791313338775,250.32017950927104,1.1175368005926616,-29821.140085378611]
[null,"GAN-b",1,78.083399609408445,1.0999999999999999,765.98927485275851,265.92578460967508,1.1872069247888299,20684.887570967756]
[null,"HP2-5",1,79.32896989093922,15.01,12068.880640490366,598.72662211529644,17.373418458666425,248851.35785866377]
[null,"to_CL-1",1,79.256095211223084,13.41,18.332100715568163,0.90943949688971137,2.6389461164232991E-2,377.28793989182356]
[null,"CL_inlet",1,49.999937454417477,4,530.1443916482018,26.3,0.76315448250593731,6840.5475684398898]
[null,"CL_outlet",1,300,1.05,530.1443916482018,26.3,0.76315448250593731,40978.289286214262]
[null,"GAN-c",1,305.54333203805578,1.0499999999999998,765.98927485275851,265.92578460967508,1.1872069247888299,84277.592476034595]
[null,"After Comp",1,306.03107160706776,15.5,12691.504714384801,629.61445833764003,18.26969947265847,1003660.5608517649]
[null,"LPbypass",1,306.03107160706776,15.5,380.74514143154397,18.888433750129202,0.54809098417975399,30109.816825552945]
[null,"Paliers",1,306.03107160706776,15.5,241.89097717788678,12,0.34820736844377376,19129.050438296075]
[null,"Recycle",1,307,1.05,268.70056048176917,13.330000000000002,0.3868003517796253,21254.115816195532]
[null,"To recycle",1,277.63455822936652,1.33,268.70056048176917,13.330000000000002,0.3868003517796253,19222.76953026302]
[null,"T1Outlet",1,38.109081849077086,6.4008119036825404,3501.9085321068769,173.72662211529644,5.0410741596161053,34371.90578830395]
[null,"T1Leak",1,38.109081849077086,6.4008119036825404,6.0472744294471683,0.3,8.7051842110943429E-3,59.355161638080695]
[null,"T2Outlet-1",1,14.284505518147569,1.33,3495.8612576774299,173.42662211529645,5.0323689754050118,12634.042545048822]
[null,"T2Leak",1,14.284505518147569,1.33,6.0472744294471674,0.3,8.7051842110943412E-3,21.854849718487046]
[null,"T3Outlet",1,6.8325997545469477,4.88,7120.243615037155,353.22906367694355,10.249746893400559,6052.8367554276474]
[null,"T3Leak",1,6.8325997545469477,4.88,14.715034444988108,0.73,2.1182614913662898E-2,12.509080610375031]
[null,"ColdComp_Outlet",1,4.7890911692025497,1.35,6728.6195087557271,333.80093398725649,9.6859954006480322,5875.2816661943698]
[null,"VLP9-1",1,3.6610712458133321,0.53,470.50631738507764,23.341407250874038,0.67730416621677225,357.81760534060965]
[null,"HP9",0,4.1538860209378754,4.7700000000000005,470.50631738507769,23.341407250874038,0.67730416621677236,-97.91442859719416]
[null,"VLP8",1,4.1006180773754295,0.51,470.50631738507764,23.341407250874038,0.67730416621677225,429.96583672240422]
[null,"HP2-9",1,79.255148717964175,13.43,8035.209550357743,398.61972418005388,11.566860430543288,165370.44525830389]
[null,"HP2_TS-2",1,79.25467548007893,13.44,8053.5416510733112,399.5291636769436,11.593249891707522,165747.73319819572]
[null,"HP8-4",1,5.7453865055148867,4.8600000000000003,920.34792737951693,45.657656426069636,1.3248610327859716,181.809813316099]
[null,"VLP7",1,6.8584773930609799,0.495,470.50631738507764,23.341407250874038,0.67730416621677225,799.62055630016926]
[null,"VLP6",1,14.129365445229894,0.49,470.50631738507764,23.341407250874038,0.67730416621677225,1700.8701260459879]
[null,"VLP5",1,20.527547121656909,0.47500000000000003,470.50631738507764,23.341407250874038,0.67730416621677225,2482.2827587364895]
[null,"VLP4",1,38.919912344718341,0.47000000000000003,470.50631738507764,23.341407250874038,0.67730416621677225,4717.1459106682742]
[null,"VLP3",1,45.46142321547697,0.46500000000000002,470.50631738507764,23.341407250874038,0.67730416621677225,5510.8159985222655]
[null,"LP",1,552.34417924166758,1.18,566.52303744611595,28.104712828349673,0.81552234123563394,80616.737415128067]
[null,"CryoPumps_Inlet",0,3.6999999999999886,4.7,5714.6743358275735,283.5,8.2263990794841533,-1619.9808315339767]
[null,"CryoPumps_Outlet",0,3.8727213200608617,4.2,5714.6743358275735,283.5,8.2263990794841533,-1538.0808315339766]
[null,"LP9-2",0,4.1006253730501498,4.1950000000000003,5714.6743358275735,283.5,8.2263990794841533,-1317.7818191309252]
[null,"HP9-1",0,4.1538860209378754,4.7700000000000005,5714.6743358275735,283.5,8.2263990794841533,-1189.2487975961731]
[null,"HP1",1,306.03107160706776,15.5,12068.880640490366,598.72662211529644,17.373418458666425,954422.64609951153]
[null,"LP-4",1,300.13260530269707,1.05,11202.370266698963,555.73979967648324,16.126057765401516,866286.3166111965]
[null,"To Comp VLP",1,301.05320579736036,0.35000000000000003,566.52303744611595,28.104712828349673,0.81552234123563394,43937.574854157887]
[null,"to_TS",1,79.329496160058028,15,8566.9721083834884,425,12.33234429905032,176644.7216128975]
[null,"to_CL-2",1,79.25467548007893,13.44,18.332100715568163,0.90943949688971137,2.6389461164232991E-2,377.28793989182356]
[null,"HP2-7",1,79.330863341652048,14.97,3501.9085321068769,173.72662211529644,5.0410741596161053,72206.753821722174]
[null,"HP2-8",1,79.330863341652048,14.97,3501.9085321068769,173.72662211529644,5.0410741596161053,72206.753821722174]
[null,"HP5-1",1,22.141144325482628,13.19,7523.397259425109,373.22916367694359,10.830095409201585,41049.854995566551]
[null,"Piston",1,4.3005872176408388,1.089,53.381568020384897,2.6482129417069444,7.684393829254331E-2,40.889957847186437]
[null,"To Buffer",1,306.03107160706776,15.5,-1.2044714995489413E-2,-5.9752778558408437E-4,-1.7338631482522458E-5,-0.95251159572677591]
[null,"VLP8-1",1,4.1928491272246333,0.5,470.50631738507764,23.341407250874038,0.67730416621677225,444.96583672240428]
[null,"HP2-4",1,79.25467548007893,15.23,12068.880640490366,598.72662211529644,17.373418458666425,248651.35785866383]
[null,"CP1_Inlet",0,4.4005872176408616,4.6089999999999991,8949.9661555818093,444,12.883672632419628,-1487.0027840866271]
[null,"CP1_Outlet",0,4.5396838819543177,5.1449999999999987,8949.9661555818093,444,12.883672632419628,-1147.6240409748791]
[null,"TF_Inlet",0,4.4005872176408616,5.1269999999999998,9151.5419698967162,454.00000000000006,13.173845439456107,-1422.0590028549855]
[null,"TF_Outlet",0,5.1555101395992438,4.6269999999999998,9151.5419698967162,454.00000000000006,13.173845439456107,54.500997145014331]
[null,"HP9-0",0,4.1538860209378754,4.7700000000000005,6185.1806532126502,306.841407250874,8.9037032457009246,-1287.1632261933669]
[null,"CP2_Inlet",0,4.4005872176408616,3.9409999999999998,19351.278174230942,960,27.856589475501899,-3468.749525521077]
[null,"CP2_outlet",0,4.5626130659319415,4.8809999999999993,19351.278174230942,960,27.856589475501899,-2491.5759131629497]
[null,"PF_Inlet",0,4.4005872176408616,4.8109999999999999,19552.853988545845,970,28.146762282538372,-3167.6678467893171]
[null,"PF_Outlet",0,4.6368433322093097,4.0110000000000001,19552.853988545845,970,28.146762282538372,-2502.2278467893175]
[null,"HP8-6",0,4.4005872176408616,4.79,6185.1806532126493,306.84140725087394,8.9037032457009229,-1004.7159824085207]
[null,"MP6",1,14.284505518147569,1.33,3489.8139832479824,173.12662211529644,5.0236637911939175,12612.187695330334]
[null,"LP9-3",9.6707029571930503E-3,4.2971447651461858,1.0889999999999997,5714.6743358275735,283.5,8.2263990794841533,-1317.781819130925]
[null,"HP3-3",1,48.734381899369396,14.950000000000001,3501.9085321068769,173.72662211529644,5.0410741596161053,44254.620327431126]
[null,"GHe1-3",0.99807902472191512,4.2834637322509934,1.069,6728.6195087557271,333.80093398725649,9.6859954006480322,5154.0817980039965]
[null,"T3Inlet",1,8.9518918826453273,13.07,7120.243615037155,353.22906367694355,10.249746893400559,8493.0132309520668]
[null,"LP-1",1,307,1.1300000000000001,566.52303744611595,28.104712828349673,0.81552234123563394,44812.489607919015]
[null,"VLP1-1",1,299.82975187899069,0.35000000000000003,470.50631738507764,23.341407250874038,0.67730416621677225,36342.564615353614]
[null,"VLPbypass",1,307,1.1300000000000001,96.016720061038299,4.7633055774756361,0.13821817501886174,7595.0102388042742]
[null,"VLP-2",1,307.04844129479807,0.35000000000000003,96.016720061038299,4.7633055774756361,0.13821817501886174,7595.0102388042733]
[null,"Conso.liq",0,4.2993665145158388,1.089,-362.93796685970358,-18.005035380520148,-0.52245716571566347,86.995276365053428]
[null,"HP2-6",1,79.32896989093922,15.01,3501.9085321068769,173.72662211529644,5.0410741596161053,72206.753821722174]
[null,"From_Buffer",1,307,1.05,309.54511784638436,15.356262798611695,0.44559698818629978,24484.905328254154]
[null,"LPbypass-2",1,306.03107160706776,15.5,380.74437770948282,18.888395862545131,0.54808988478509191,30109.756429425932]
[null,"LPbypass-3",1,306.928788694204,1.05,380.74437770948282,18.888395862545131,0.54808988478509191,30109.756429425932]
[null,"GHe",1,4.3005870925301792,1.089,6728.6195087557271,333.80093398725649,9.6859954006480322,5154.0817980039965]
[null,"LP6-2",1,14.182282056631834,1.33,10218.433492003709,506.9275561025529,14.709659191841951,36652.527894338011]
[null,"LP4",1,38.919911131510645,1.29,10218.433492003709,506.9275561025529,14.709659191841951,102447.42672962195]
[null,"HP3-4",1,48.734381899369396,13.41,511.81229093263363,25.39056050311029,0.73676502134170441,6463.2596285480649]
[null,"HP2_TS-3",1,79.25467548007893,13.44,8035.209550357743,398.61972418005382,11.566860430543286,165370.44525830389]
[null,"HP3-1",1,48.734381899369396,13.41,8035.209550357743,398.61972418005388,11.566860430543288,101470.1022500195]
[null,"bypass",1,79.403804428759429,13.43,0,0,0,0]
[null,"bypass-2",1,79.330863341652048,14.97,0,0,0,0]
[null,"T2Outlet",1,14.288208553095387,1.35,3495.8612576774299,173.42662211529645,5.0323689754050118,12634.042545048822]
[null,"HP8",1,5.7409999999999854,4.87,7105.5285805921667,352.49906367694354,10.228564278486894,1388.6591883549224]
[null,"LP-3",1,300.12762868624355,1.1300000000000001,11202.370266698963,555.73979967648324,16.126057765401516,866286.3166111965]
[null,"HP8-1",1,5.7409999999999854,8.1449999999999996,403.15364438795439,20.0001,0.58034851580102653,75.050856689362277]
[null,"HP7-2",1,8.3402515434314637,8.15,403.15364438795439,20.0001,0.58034851580102653,480.88091096523175]
[null,"HP7-3",1,8.9574289736403898,13.15,7120.243615037155,353.22906367694355,10.249746893400559,8493.0132309520668]
[null,"to_damper",0.42886819732935649,4.298696310406001,1.089,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,3.8525235718502552E-4]
[null,22,"<empty>","<empty>","<empty>","<empty>","<empty>","<empty>","<empty>"]
[null,"WaterInlet","<empty>",303,"<empty>","<empty>","<empty>","<empty>","<empty>"]
[null,"LP-2",1,307,1.1300000000000001,470.50631738507764,23.341407250874038,0.67730416621677225,37217.479369114735]
[null,"HP_BP1-b",1,306.03542159212702,15.43,1138.9033508792168,56.5,1.6394763597561013,90065.945813644008]
[null,"HP_BP1-a",1,306.04163583935269,15.33,1138.9033508792168,56.5,1.6394763597561013,90065.945813644008]
[null,"HP_BP1",1,306.04163583935269,15.33,1138.9033508792168,56.5,1.6394763597561013,90065.945813644008]
[null,"HP2_MEF",1,88.650822194181984,15.345000000000001,0,0,0,0]
[null,"HP2_MEF-2",1,88.651587369709119,15.33,0,0,0,0]
[null,"HP2-1",1,88.650822194181984,15.345000000000001,10929.977289611148,542.22662211529644,15.733942098910324,251819.60500806433]
[null,"HP2-2",1,88.654138028777311,15.280000000000001,10929.977289611148,542.22662211529644,15.733942098910324,251819.60500806433]
[null,"HP_BP2",1,89.514575199655809,15.280000000000001,1138.9033508792168,56.5,1.6394763597561013,26493.336886811052]
[null,"HP2-3",1,88.735329827960584,15.280000000000001,12068.880640490366,598.72662211529644,17.373418458666425,278312.94189487537]
[null,"to_TS-3",1,79.32944324839886,15,8566.9700926253445,424.99989999999997,12.332341397322249,176644.56247350539]
[null,"HP_CD2-1",1,79.32896989093922,15.01,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,4.1563436243986264E-2]
[null,"HP_CD2",1,79.32944324839886,15,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,4.1563436243986264E-2]
[null,"HP_CD1",1,305.54328477135329,15,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,0.15913939211988004]
[null,"to_TS-2",1,79.329496160058028,15,8566.9721083834884,425,12.33234429905032,176644.7216128975]
[null,"bypass_TS",1,79.329496160058028,15,0,0,0,0]
[null,"bypass_TS-1",1,79.400540007026677,13.5,0,0,0,0]
[null,"to_TS-4",1,79.32896989093922,15.01,8566.9700926253445,424.99989999999997,12.332341397322249,176644.56247350539]
[null,"bypass_HP_BP-2",1,89.277502108746887,1.2650000000000001,513.43045731017719,25.47083632305641,0.73909440734279652,11816.387184494399]
[null,"HP2_TS",1,88.650822194181984,13.47,8053.5416510733112,399.5291636769436,11.593249891707522,185348.89194943794]
[null,"bypass_HP_BP",1,88.650822194181984,13.47,513.43045731017719,25.47083632305641,0.73909440734279652,11816.387184494399]
[null,"LIN",5.868406150727306E-2,78.456533759698061,1.1499999999999999,765.98927485275851,265.92578460967508,1.1872069247888299,-28603.012471049795]
[null,"GAN-a",1,78.068329195532272,1.0999999999999999,721.03791313338775,250.32017950927104,1.1175368005926616,19466.759956638933]
[null,"GAN",1,78.456533759698061,1.1499999999999999,44.951361719370794,15.605605100404029,6.9670124196168234E-2,1218.1276143288267]
[null,"N2-a",4.5190362406900093E-3,83.593268892293111,1.99,765.98927485275851,265.92578460967508,1.1872069247888299,-28603.012471049795]
[null,"N2",0,83.644048867120603,2,765.98927485275851,265.92578460967508,1.1872069247888299,-28803.012471049791]
[null,"to_TS-1",1,79.329496160058028,15,8566.9721083834884,425,12.33234429905032,176644.7216128975]
[null,"HP_CD2-2",1,79.329496160058028,15,0,0,0,0]
[null,"HP2_TS-4",1,79.255148717964175,13.43,8035.209550357743,398.61972418005388,11.566860430543288,165370.44525830389]
[null,"HP_CD2-3",1,79.403857378281316,13.43,0,0,0,0]
[null,"HP2-10",1,79.255148717964175,13.43,8035.209550357743,398.61972418005388,11.566860430543288,165370.44525830389]
[null,"supply_loop",1,5.7612824190487117,8.1349999999999998,403.15162862981123,20,0.58034561407295615,77.0504714370051]
[null,"supply_loop1-1",1,5.7501708560288876,5.1449999999999987,201.57581431490732,10.000000000000085,0.29017280703648057,38.52523571850287]
[null,"CP1_outlet-2",0,4.5750974520537966,5.1449999999999987,9151.5419698967162,454.00000000000006,13.173845439456107,-1109.0988052563762]
[null,"supply_loop2",1,5.7612824190487117,8.1349999999999998,201.57581431490394,9.9999999999999165,0.29017280703647563,38.52523571850223]
[null,2,0,4.5788694883636367,4.8809999999999993,19552.853988545845,970,28.146762282538372,-2453.0506774444475]
[null,"HP8-2",1,5.7612824190487117,8.1349999999999998,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,3.8525235718502547E-4]
[null,"supply_loop1",1,5.7612824190487117,8.1349999999999998,201.57581431490732,10.000000000000085,0.29017280703648057,38.52523571850287]
[null,"supply_loop2-2",1,5.7311045750525409,4.8809999999999993,201.57581431490394,10.000000000000028,0.29017280703647563,38.52523571850223]
[null,"return-1",0,4.4005872176408616,4.6089999999999991,201.57581431490689,10.000000000000064,0.29017280703647991,-33.491053695644972]
[null,"return-2",0,4.4005872176408616,3.9409999999999998,201.57581431490561,10,0.29017280703647808,-36.132807557511214]
[null,"return-3",0,4.4328192323414441,3.9409999999999998,403.15162862981248,20.000000000000064,0.58034561407295804,-69.623861253156193]
[null,"CD_return",0,4.4328192323414441,3.9409999999999998,0,0,0,0]
[null,"baking_return",0,4.4328192323414441,3.9409999999999998,0,0,0,0]
[null,"LP5-1",1,20.527592708511094,1.3,10218.433492003709,506.9275561025529,14.709659191841951,53698.600409644219]
[null,"baking_return-1",9.2976564344565901E-3,4.4958856499283684,1.3,0,0,0,0]
[null,"LP2-1",1,78.816791306767726,1.2650000000000001,10218.433492003709,506.9275561025529,14.709659191841951,207623.5101440289]
[null,"CD_return-2",1.8910490479863408E-2,4.4664357972342827,1.2650000000000001,0,0,0,0]
[null,"CL_inlet-2",1,49.781313495212544,13.41,530.1443916482018,26.3,0.76315448250593731,6840.5475684398898]
[null,"return_4",0,4.4328192323414441,3.9409999999999998,0,0,0,0]
[null,"return_damper",0,4.4328192323414441,3.9409999999999998,403.15162862981248,20.000000000000064,0.58034561407295804,-69.623861253156193]
[null,"HP7-5",1,8.9574289736403898,13.15,403.15364438795439,20.0001,0.58034851580102653,480.88091096523175]
[null,"return_damper-1",6.709312323176389E-2,4.2978578767403519,1.0889999999999997,403.15162862981248,20.000000000000064,0.58034561407295804,-69.623861253156193]
[null,1,1,5.7612824190487117,8.1349999999999998,403.15364438795439,20.0001,0.58034851580102653,77.050856689362277]
[null,"CP1_inlet-1",0,4.4005872176408616,4.6089999999999991,9151.5419698967162,454.00000000000006,13.173845439456107,-1520.4938377822721]
[null,"CP2_Inlet-1",0,4.4005872176408616,3.9409999999999998,19552.853988545845,970,28.146762282538372,-3504.8823330785885]
[null,"HP1-3",1,306.03542159212702,15.43,10929.977289611148,542.22662211529644,15.733942098910324,864356.70028586756]
[null,"LP2-2",1,79.317204829956694,1.2650000000000001,10731.863949313885,532.39839242560925,15.448753599184746,219439.89732852331]
[null,"VLP2",1,78.816792238754203,0.45500000000000002,470.50631738507764,23.341407250874038,0.67730416621677225,9555.3375569662421]
[null,"TS_outlet-2",1,99.291768389178571,13.5,8566.9721083834884,425,12.33234429905032,220744.72163682172]
[null,"HP2",1,88.650822194181984,15.345000000000001,10929.977289611148,542.22662211529644,15.733942098910324,251819.60500806433]
[null,"LP1",1,299.82633030834717,1.1300000000000001,10731.863949313885,532.39839242560913,15.448753599184746,829068.83724208188]
[null,"VLP1",1,299.82633027529363,0.40500000000000003,470.50631738507764,23.341407250874038,0.67730416621677225,36342.564615353614]
[null,"HP2_TS-1",1,88.650822194181984,13.47,8566.9721083834884,425,12.33234429905032,197165.27913393232]
[null,"LP1a",1,99.355548445453337,1.1300000000000001,10731.863949313885,532.39839242560925,15.448753599184746,274840.25613289437]
[null,"VLP1a",1,99.355560746758613,0.40500000000000003,470.50631738507764,23.341407250874038,0.67730416621677225,12044.743608184916]
[null,"HP1a",1,100.67264076507053,15.43,10929.977289611148,542.22662211529644,15.733942098910324,285830.10643510811]

{"sheet":"Dump_Baking","index":11,"n_rows":204,"n_cols":9,"rows_kept":204,"cut":false,"hidden":true,"merged":[]}
[null,"Case:","(03)-JT60-OFFCase_A-BAKING.HSC"]
[null,"Flowsheet:","Case (Main)"]
[null,"Current Flowsheet Environment:","Case (Main)"]
[]
[null,"Name","Vapour Fraction","Temperature","Pressure","Molar Flow","Mass Flow","Liquid Volume Flow","Heat Flow"]
[1,null,"<none>","K","bar","Nm3/h(gas)","g/s","m3/h","W*"]
[]
[null,"HP1-2",1,306.03542159212702,15.43,9160.1544745900392,454.42725883175001,13.186243328910109,724396.82956076425]
[null,"LP2",1,80.439465054284199,1.2650000000000001,8981.2633528673541,445.55262660810348,12.928725634534917,186242.42012707723]
[null,"HP3-2",1,37.432771880411025,12.71,6462.1159193714202,320.57992380356592,9.3023576369620979,62281.229439060829]
[null,"LP3",1,35.226972005856794,1.28,8981.2633528673541,445.55262660810348,12.928725634534917,81467.525636514794]
[null,"T1Inlet",1,37.435072403279634,9.3537449776458512,2545.3027327865598,126.27024434638965,3.6640191247173859,24531.3841548583]
[null,"MP4",1,29.362186216080232,4.0691562703658368,2539.2554583571127,125.97024434638965,3.655313940506292,19117.171156892844]
[null,"HP4",1,29.017642017738922,12.69,6462.115919371422,320.57992380356598,9.3023576369620997,47644.505218418417]
[null,"MP5",1,17.064229792003971,4.019156270365837,2539.2554583571127,125.97024434638965,3.655313940506292,10797.218147042446]
[null,"LP5",1,16.893338894618637,1.3,7647.9199714999795,379.40662660810347,11.009348585111431,32912.665710991467]
[null,"HP6",1,13.225287433572078,12.46,6462.1159193714238,320.57992380356609,9.3023576369621033,17908.383015733169]
[null,"LP6",1,13.125287433572055,1.33,5114.7117875723143,253.73638226171386,7.3627398288162329,16909.268974160037]
[null,"HP7",1,10.823703623356835,12.450000000000001,6462.1159193714238,320.57992380356609,9.3023576369621033,12441.434586447253]
[null,"LP7",1,9.1536887597515033,1.335,5114.7117875723143,253.73638226171386,7.3627398288162329,11412.306141278164]
[null,"HP7-4",1,8.4788974741975949,5.18,5114.0151726380536,253.7018238035661,7.3617370363354731,8099.6380858665643]
[null,"LP8",0.97715428772606594,4.5339367144378571,1.34,5114.7117875723143,253.73638226171386,7.3627398288162329,3733.5728737998097]
[null,"JT2-3",0.72185817352189463,4.70207527105498,1.5429999999999999,5113.7869411473539,253.69050143875381,7.361408492097488,2528.7757228642936]
[null,"LHe 3,6K",0,3.6017715941583788,0.53,0,0,0,0]
[null,"HP5",1,17.064229792003971,12.67,6462.1159193714229,320.57992380356603,9.3023576369621015,25726.011258298262]
[null,"GHe 4,3K",1,4.7015625248710649,1.5429999999999999,5114.9325015598188,253.74733168976184,7.3630575514434451,3718.7343412579744]
[null,"LHe 4,3K",0,4.7015625248710649,1.5429999999999999,0,0,0,0]
[null,"GHe 3,6K",1,3.6017715941583788,0.53,2.6655676384963477E-2,1.3223648122448594E-3,3.8371430949535615E-5,1.970497140289041E-2]
[null,"HP8-3",1,6.3624967397822161,5.16,5114.0151726380536,253.7018238035661,7.3617370363354731,2528.8885836970812]
[null,"HP8-5",1,6.3624967659199569,5.16,0.22823149069986909,1.132236481224486E-2,3.2854423798601371E-4,0.11286083278734829]
[null,"VLP0",0.17541265563825398,3.6017613654458955,0.53,2.6655676384963477E-2,1.3223648122448594E-3,3.8371430949535615E-5,-5.3577052816257947E-3]
[null,"MP",1,1117.3360677635683,16,9693.5532669583481,480.88870680759811,13.954082592650266,2792112.5778963696]
[null,"MP-1",1,306,16,9693.5532669583481,480.88870680759811,13.954082592650266,766578.69397745968]
[null,"TS_inlet",1,81.999999836740756,15,9160.1524588318953,454.42715883174998,13.186240427182039,195218.88000378708]
[null,"TS_outlet",1,142.02785884698983,12.8,9160.1524588318953,454.42715883174992,13.186240427182035,336968.88000378711]
[null,"To Comp LP",1,286.25525748751016,1.05,9693.5532669583481,480.88870680759811,13.954082592650266,714956.6382528122]
[null,"LIN-a",0,78.456049331378296,1.1499999999999999,1797.0092490873683,623.86133879780459,2.7851849816515952,-74322.464600083898]
[null,"Gan-c",1,78.068329195532272,1.0999999999999999,1904.4366468975827,661.15652815505553,2.9516867262313049,51416.4517323006]
[null,"HP2-5",1,81.999467431355811,15.01,9160.1544745900392,454.42725883175001,13.186243328910109,195218.8104193928]
[null,"to_CL-1",1,81.907008130587485,12.71,0,0,0,0]
[null,"CL_inlet",1,37.428027804218175,4,2.0157581431490559E-2,1E-3,2.9017280703647809E-5,0.19427676162660576]
[null,"CL_outlet",1,300,1.05,2.0157581431490559E-2,1E-3,2.9017280703647809E-5,1.5581098587914168]
[null,"Gan-d",1,298.53885221214023,1.0499999999999998,843.71846546021482,292.91075251713846,1.3076794122987125,90694.535991220851]
[null,"After Comp",1,306.03107160706776,15.5,9693.5532669583481,480.88870680759811,13.954082592650266,766578.69397745968]
[null,"LPbypass",1,306.03107160706776,15.5,290.80659800875043,14.426661204227942,0.41862247777950795,22997.360819323789]
[null,"Paliers",1,306.03107160706776,15.5,241.89097717788673,12,0.3482073684437737,19129.050438296072]
[null,"Recycle",1,307,1.05,268.70056048176917,13.330000000000002,0.3868003517796253,21254.115816195532]
[null,"To recycle",1,277.55217288461489,1.33,268.70056048176917,13.330000000000002,0.3868003517796253,19217.067159290229]
[null,"T1Outlet",1,29.362186216080232,4.0691562703658368,2545.3027327865598,126.27024434638965,3.6640191247173859,19162.698982744303]
[null,"T1Leak",1,29.362186216080232,4.0691562703658368,6.0472744294471683,0.3,8.7051842110943429E-3,45.527825851456527]
[null,"T2Outlet-1",1,12.623654234622165,1.33,2539.2554583571127,125.97024434638965,3.655313940506292,8054.9776826538173]
[null,"T2Leak",1,12.623654234622165,1.33,6.0472744294471674,0.3,8.7051842110943412E-3,19.183048483666788]
[null,"T3Outlet",1,8.4788974741975949,5.18,5128.7302070830419,254.43182380356609,7.3829196512491375,8122.9439325255953]
[null,"T3Leak",1,8.4788974741975949,5.18,14.715034444988108,0.73,2.1182614913662898E-2,23.305846659031705]
[null,"ColdComp_Outlet",0.92211207797773187,4.5402592950727012,1.35,2.0157581431225223E-2,9.9999999998683694E-4,2.9017280703265848E-5,1.3654574229334998E-2]
[null,"VLP9-1",1,1459.1949279870437,0.53,2.6655676384963477E-2,1.3223648122448594E-3,3.8371430949535615E-5,10.019704971402891]
[null,"HP9",0,4.1549872313548235,5.07,2.6655676384963477E-2,1.3223648122448594E-3,3.8371430949535615E-5,-5.3577052816257981E-3]
[null,"VLP8",1,1732.9096686039575,0.51,2.6655676384963477E-2,1.3223648122448594E-3,3.8371430949535615E-5,11.899148742161147]
[null,"HP2-9",1,81.905068029454412,12.75,6462.136076952851,320.58092380356601,9.3023866542428024,137377.74113496972]
[null,"HP2_TS-2",1,81.904582960503234,12.76,9007.4367939812691,446.85106814995561,12.966402877232118,191487.97003790303]
[null,"HP8-4",1,6.3624967659199569,5.16,5113.7869411473539,253.69050143875381,7.361408492097488,2528.7757228642936]
[null,"VLP7",1,9.1536648506100846,0.495,2.6655676384963477E-2,1.3223648122448594E-3,3.8371430949535615E-5,6.1615959219986305E-2]
[null,"VLP6",1,13.125195100012377,0.49,2.6655676384963477E-2,1.3223648122448594E-3,3.8371430949535615E-5,8.9384705961707736E-2]
[null,"VLP5",1,16.893340924498887,0.47500000000000003,2.6655676384963477E-2,1.3223648122448594E-3,3.8371430949535615E-5,0.11552460976474331]
[null,"VLP4",1,28.921093172645413,0.47000000000000003,2.6655676384963477E-2,1.3223648122448594E-3,3.8371430949535615E-5,0.19846498615732383]
[null,"VLP3",1,35.226974351623085,0.46500000000000002,2.6655676384963477E-2,1.3223648122448594E-3,3.8371430949535615E-5,0.24184862716660896]
[null,"LP",1,558.62162414618479,1.18,0.22823149069986909,1.132236481224486E-2,3.2854423798601371E-4,32.846604478345164]
[null,"CryoPumps_Inlet",0,3.6999999999999886,5,0.20157581431490562,0.01,2.9017280703647806E-4,-5.5578767494059954E-2]
[null,"CryoPumps_Outlet",1,1575.9633226535702,4.5,0.20157581431490562,0.01,2.9017280703647806E-4,81.844421232505951]
[null,"LP9-2",1,1732.9096691984241,4.4950000000000001,0.20157581431490562,0.01,2.9017280703647806E-4,89.99377450073365]
[null,"HP9-1",0,4.1549872313548235,5.07,0.20157581431490562,0.01,2.9017280703647806E-4,-4.0516090809543749E-2]
[null,"HP1",1,306.03107160706776,15.5,9160.1544745900392,454.42725883175001,13.186243328910109,724396.82956076425]
[null,"LP-4",1,284.98677068265323,1.05,9134.0258309757955,453.13103965471009,13.148630573196488,670703.5940247504]
[null,"To Comp VLP",1,304.47161803175317,0.35000000000000003,0.22823149069986909,1.132236481224486E-2,3.2854423798601371E-4,17.90182300833677]
[null,"to_TS",1,81.999999836740756,15,9160.1524588318953,454.42715883174998,13.186240427182039,195218.88000378708]
[null,"to_CL-2",1,81.904582960503234,12.76,0,0,0,0]
[null,"HP2-7",1,82.109663477933481,12.74,0,0,0,0]
[null,"HP2-8",1,81.905553060119075,12.74,2545.3027327865598,126.27024434638965,3.6640191247173859,54110.271862267109]
[null,"HP5-1",1,17.099179933944754,12.49,6462.1159193714238,320.57992380356609,9.3023576369621033,25826.011258298262]
[null,"Piston",1,4.7015625248710649,1.5429999999999999,-0.22071398750505836,-1.0949428047962874E-2,-3.1772262721213319E-4,-0.16046676758310005]
[null,"To Buffer",1,306.03107160706776,15.5,0.70121718167215141,3.4786771620165524E-2,1.0094175168760325E-3,55.453159075636059]
[null,"VLP8-1",1,3917.4399063352298,0.5,2.6655676384963477E-2,1.3223648122448594E-3,3.8371430949535615E-5,26.899148742161145]
[null,"HP2-4",1,81.904582960503234,15.23,9160.1544745900392,454.42725883175001,13.186243328910109,195018.81041939283]
[null,"CP1_Inlet",0,4.8015625248710876,5.83,2.0157581431490559E-2,1E-3,2.9017280703647809E-5,-1.2532757405334567E-3]
[null,"CP1_Outlet",0,4.8517222807333269,6.07,2.0157581431490559E-2,1E-3,2.9017280703647809E-5,-9.5535831041355891E-4]
[null,"TF_Inlet",0,4.8015625248710876,6,867.78388062566853,43.05,1.249193934292038,-51.264029538452348]
[null,"TF_Outlet",1,12.07978683496583,5.9,867.78388062566853,43.05,1.249193934292038,2374.2359704615478]
[null,"HP9-0",0,4.1549872313548235,5.07,0.22823149069986909,1.132236481224486E-2,3.2854423798601371E-4,-4.5873796091169539E-2]
[null,"CP2_Inlet",0,4.8015625248710876,5.83,2.0157581431490559E-2,1E-3,2.9017280703647809E-5,-1.2532757405334567E-3]
[null,"CP2_outlet",0,4.842863922354411,6.07,2.0157581431490559E-2,1E-3,2.9017280703647809E-5,-9.9259798917854616E-4]
[null,"PF_Inlet",0,4.8015625248710876,6,465.64013106743204,23.1,0.67029918425426449,-27.507528045023221]
[null,"PF_Outlet",1,11.404724027332463,5.9,465.64013106743204,23.1,0.67029918425426449,1175.7924719549769]
[null,"HP8-6",0,4.8015625248710876,5.09,0.22823149069986909,1.132236481224486E-2,3.2854423798601371E-4,-1.7076757104585203E-2]
[null,"MP6",1,12.623654234622165,1.33,2533.2081839276657,125.67024434638965,3.6466087562951981,8035.7946341701499]
[null,"LP9-3",1,1733.0511489173764,1.5429999999999995,0.20157581431490562,0.01,2.9017280703647806E-4,89.99377450073365]
[null,"HP3-3",1,37.432771880411025,12.72,2545.3027327865598,126.27024434638965,3.6640191247173859,24531.3841548583]
[null,"GHe1-3",0.99663028041859592,4.6856906649691723,1.5229999999999999,2.0157581431225223E-2,1E-3,2.9017280703265848E-5,1.4655264811831192E-2]
[null,"T3Inlet",1,10.596601799815971,10.76301784585384,5128.7302070830419,254.43182380356609,7.3829196512491375,9874.2830025194708]
[null,"LP-1",1,307,1.1300000000000001,0.22823149069986909,1.132236481224486E-2,3.2854423798601371E-4,18.053319334186007]
[null,"VLP1-1",1,284.98514585729544,0.35000000000000003,2.6655676384963477E-2,1.3223648122448594E-3,3.8371430949535615E-5,1.9569920180282923]
[null,"VLPbypass",1,307,1.1300000000000001,0.20157581431490562,0.01,2.9017280703647806E-4,15.944830990308478]
[null,"VLP-2",1,307.04844129479807,0.35000000000000003,0.20157581431490562,0.01,2.9017280703647806E-4,15.944830990308478]
[null,"Conso.liq",0,4.6997314701835649,1.5429999999999999,0.92181125857661861,4.5730251008017628E-2,1.3269675301479206E-3,-0.10227840595282686]
[null,"HP2-6",1,81.999467431355811,15.01,0,0,0,0]
[null,"From_Buffer",1,307,1.05,0,0,0,0]
[null,"LPbypass-2",1,306.03107160706776,15.5,290.80671791935021,14.426667152888013,0.41862265039344704,22997.370302007555]
[null,"LPbypass-3",1,306.928788694204,1.05,290.80671791935021,14.426667152888013,0.41862265039344704,22997.370302007555]
[null,"GHe",1,4.7015618958930077,1.5429999999999999,5114.7117875723143,253.73638226171386,7.3627398288162329,3718.5738744903915]
[null,"LP6-2",1,12.958980545143277,1.33,7647.9199714999795,379.40662660810347,11.009348585111431,24945.063608330187]
[null,"LP4",1,28.921085402831551,1.29,8981.2633528673541,445.55262660810348,12.928725634534917,66800.844799513463]
[null,"HP3-4",1,37.432771880411025,12.71,2.0157581431490559E-2,1E-3,2.9017280703647799E-5,0.19427676162660579]
[null,"HP2_TS-3",1,81.904582960503234,12.76,9007.4367939812691,446.85106814995561,12.966402877232118,191487.97003790303]
[null,"HP3-1",1,37.432771880411025,12.71,6462.136076952851,320.5809238035659,9.3023866542428024,62281.423715822457]
[null,"bypass",1,81.905553060119075,12.74,2545.3027327865598,126.27024434638965,3.6640191247173859,54110.271862267109]
[null,"bypass-2",1,81.905068029454412,12.75,2545.3027327865598,126.27024434638965,3.6640191247173859,54110.271862267109]
[null,"T2Outlet",1,12.628128268029286,1.35,2539.2554583571127,125.97024434638965,3.655313940506292,8054.9776826538173]
[null,"HP8",1,6.3600000000000136,5.17,5114.0151726380536,253.7018238035661,7.3617370363354731,2513.8885836970812]
[null,"LP-3",1,284.98177705796519,1.1300000000000001,9134.0258309757955,453.13103965471009,13.148630573196488,670703.5940247504]
[null,"HP8-1",1,6.3600000000000136,12.445,1333.3857122883808,66.148100000000014,1.9194379857129658,521.00535140184775]
[null,"HP7-2",1,10.823703623359052,12.450000000000001,1333.385712288381,66.148100000000014,1.9194379857129662,2567.1515839277795]
[null,"HP7-3",1,10.823703623356835,12.450000000000001,5128.7302070830419,254.43182380356609,7.3829196512491375,9874.2830025194708]
[null,"to_damper",0.60054630159035471,4.6984414329057245,1.5429999999999999,2.0157581432345027E-3,1.0000000000423896E-4,2.9017280704877835E-6,7.876346432080934E-4]
[null,22,"<empty>","<empty>","<empty>","<empty>","<empty>","<empty>","<empty>"]
[null,"WaterInlet","<empty>",303,"<empty>","<empty>","<empty>","<empty>","<empty>"]
[null,"LP-2",1,307,1.1300000000000001,2.6655676384963481E-2,1.3223648122448596E-3,3.8371430949535622E-5,2.108488343877529]
[null,"HP_BP1-b",1,306.03542159212702,15.43,1159.0609323107071,57.499999999999993,1.668493640459749,91660.033350168669]
[null,"HP_BP1-a",1,306.04163583935264,15.33,1159.0609323107074,57.5,1.6684936404597488,91660.033350168669]
[null,"HP_BP1",1,306.04163583935264,15.33,1159.0609323107074,57.5,1.668493640459749,91660.033350168669]
[null,"HP2_MEF",1,110.02559149210194,15.345000000000001,0,0,0,0]
[null,"HP2_MEF-2",1,110.02643846391265,15.33,0,0,0,0]
[null,"HP2-1",1,110.02559149210194,15.345000000000001,8001.0935422793318,396.92725883175001,11.517749688450358,228566.49073297071]
[null,"HP2-2",1,110.02926177405956,15.280000000000001,8001.0935422793318,396.92725883175001,11.517749688450358,228566.49073297071]
[null,"HP_BP2",1,78.868321790884295,15.280000000000001,1159.0609323107074,57.5,1.668493640459749,23764.304673571074]
[null,"HP2-3",1,106.08000751275932,15.280000000000001,9160.1544745900392,454.42725883175001,13.186243328910109,252330.79540654176]
[null,"to_TS-3",1,81.999952442318261,15,9160.1524588318953,454.42715883174998,13.186240427182039,195218.76746008376]
[null,"HP_CD2-1",1,81.999467431355811,15.01,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,4.2959309025885663E-2]
[null,"HP_CD2",1,81.999952442318261,15,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,4.2959309025885663E-2]
[null,"HP_CD1",1,298.53878065626901,15,2.0157581432345027E-3,1.0000000000423894E-4,2.9017280704877835E-6,0.15550303711558977]
[null,"to_TS-2",1,81.999999836740756,15,9160.1544745900392,454.42725883175001,13.186243328910109,195218.92296312089]
[null,"bypass_TS",1,81.999999836740756,15,0,0,0,0]
[null,"bypass_TS-1",1,82.106795633936201,12.8,0,0,0,0]
[null,"to_TS-4",1,81.999467431355811,15.01,9160.1524588318953,454.42715883174998,13.186240427182039,195218.76746008376]
[null,"bypass_HP_BP-2",1,110.68009704821515,1.2650000000000001,152.71566485062704,7.5760906817943781,0.219837549949918,4356.9202281255848]
[null,"HP2_TS",1,110.02559149210194,12.790000000000001,9007.4367939812691,446.85106814995555,12.966402877232118,256978.76907156405]
[null,"bypass_HP_BP",1,110.02559149210194,12.790000000000001,152.71566485062704,7.5760906817943781,0.219837549949918,4356.9202281255848]
[null,"LIN",5.6409016275347855E-2,78.456049331378296,1.1499999999999999,1904.4366468975827,661.15652815505553,2.9516867262313049,-71411.332288509497]
[null,"GAN-a",0.99989530331288767,78.071359804953033,1.0999999999999999,1797.0092490873683,623.86133879780459,2.7851849816515952,48505.319420726199]
[null,"GAN",1,78.456049331378296,1.1499999999999999,107.42739781021459,37.29518935725099,0.16650174457970982,2911.132311574398]
[null,"N2-a",2.1444120058220452E-3,83.594041030844352,1.99,1904.4366468975827,661.15652815505553,2.9516867262313049,-71411.332288509497]
[null,"N2",0,83.644048867120603,2,1904.4366468975827,661.15652815505553,2.9516867262313049,-71611.332288509497]
[null,"to_TS-1",1,81.999999836740756,15,9160.1524588318953,454.42715883174998,13.186240427182039,195218.88000378708]
[null,"HP_CD2-2",1,81.999999836740756,15,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,4.2959333791945775E-2]
[null,"HP2_TS-4",1,81.90506798376731,12.75,9007.4367939812691,446.85106814995561,12.966402877232118,191487.97003790303]
[null,"HP_CD2-3",1,82.109225026625268,12.75,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,4.2959333791945775E-2]
[null,"HP2-10",1,81.905068029454412,12.75,9007.4388097394094,446.85116814995564,12.966405778960187,191488.0129972368]
[null,"supply_loop",1,6.3600000010278563,12.445,1333.3836965302376,66.14800000000001,1.9194350839848955,521.00456376720444]
[null,"supply_loop1-1",1,6.3182531345607345,6.07,867.76372304423705,43.048999999999999,1.2491649170113344,339.06883754027916]
[null,"CP1_outlet-2",1,6.3182304457917553,6.07,867.78388062566853,43.05,1.249193934292038,339.06788218196874]
[null,"supply_loop2",1,6.3600000010278563,12.445,465.61997348600056,23.099000000000004,0.6702701669735609,181.9357262269254]
[null,2,1,6.3182106723973561,6.07,465.64013106743204,23.1,0.67029918425426449,181.93473362893619]
[null,"HP8-2",1,6.3600000010278563,12.445,2.0157581432345027E-3,1E-4,2.9017280704877835E-6,7.8763464320809329E-4]
[null,"supply_loop1",1,6.3600000010278563,12.445,867.76372304423717,43.048999999999992,1.2491649170113341,339.06883754027922]
[null,"supply_loop2-2",1,6.3182531345607345,6.07,465.61997348600056,23.099,0.6702701669735609,181.9357262269254]
[null,"return-1",0,4.8015625248710876,5.83,1.4615460081675511E-14,7.2506020284968109E-16,2.1039275433133019E-17,-9.0870036265777227E-16]
[null,"return-2",0,4.8015625248710876,5.83,8.4602341944745514E-14,7.6664952055986724E-15,1.217869273027735E-16,-5.2600587581416614E-15]
[null,"return-3",1,11.827469424697028,5.83,1333.3836965302376,66.147999999999996,1.919435083984895,3549.9223916481783]
[null,"CD_return",1,11.827469424697028,5.83,2.0157581431505173E-2,1E-3,2.9017280703668846E-5,5.3666360156781036E-2]
[null,"baking_return",1,11.827469424697028,5.83,1333.3433813673746,66.146000000000001,1.9193770494234879,3549.8150589278648]
[null,"LP5-1",1,15.967193466663502,1.3,8981.2633528673541,445.55262660810348,12.928725634534917,36462.480769919333]
[null,"baking_return-1",1,10.719214801989949,1.3,1333.3433813673746,66.146000000000001,1.9193770494234879,3549.8150589278648]
[null,"LP2-1",1,80.439307666770389,1.2650000000000001,8981.2835104487858,445.55362660810346,12.928754651815622,186242.47379343736]
[null,"CD_return-2",1,10.709299857962492,1.2650000000000001,2.0157581431505173E-2,1.0000000000007249E-3,2.9017280703668846E-5,5.3666360156781036E-2]
[null,"CL_inlet-2",1,37.432771868024901,12.71,2.0157581431490559E-2,1E-3,2.9017280703647809E-5,0.19427676162660576]
[null,"return_4",1,11.827469424697028,5.83,1333.3635389488061,66.146999999999991,1.9194060667041914,3549.8687252880218]
[null,"return_damper",1,11.827469424697028,5.83,2.0157581431505173E-2,1E-3,2.9017280703668846E-5,5.3666360156781036E-2]
[null,"HP7-5",1,10.823703623356835,12.450000000000001,1333.385712288381,66.148099999999999,1.9194379857129655,2567.1515839277795]
[null,"return_damper-1",1,10.787440183251363,1.5429999999999995,2.0157581431505173E-2,1.0000000000007249E-3,2.9017280703668846E-5,5.3666360156781036E-2]
[null,1,1,6.3600000010278563,12.445,1333.3857122883808,66.148100000000014,1.9194379857129658,521.00535140184775]
[null,"CP1_inlet-1",0,4.8015625248710876,5.83,2.0157581431505173E-2,1.0000000000007249E-3,2.9017280703668846E-5,-1.253275740534365E-3]
[null,"CP2_Inlet-1",0,4.8015625248710876,5.83,2.0157581431575162E-2,1.000000000004197E-3,2.9017280703769592E-5,-1.253275740538717E-3]
[null,"HP1-3",1,306.03542159212702,15.43,8001.0935422793318,396.92725883175001,11.517749688450358,632736.79621059541]
[null,"LP2-2",1,80.944816623784732,1.2650000000000001,9133.9991752994119,453.12971728989783,13.14859220176554,190599.39402156294]
[null,"VLP2",1,80.439464663802539,0.45500000000000002,2.6655676384963477E-2,1.3223648122448594E-3,3.8371430949535615E-5,0.55248462133089904]
[null,"HP1_TS",1,142.02785884698983,12.8,9160.1524588318953,454.42715883174992,13.186240427182035,336968.88000378711]
[null,"HP2",1,110.02559149210194,15.345000000000001,8001.0935422793318,396.92725883175001,11.517749688450358,228566.49073297071]
[null,"LP1",1,284.98171280243156,1.1300000000000001,9133.9991752994119,453.12971728989783,13.14859220176554,670701.48553640652]
[null,"VLP1",1,284.9817127594473,0.40500000000000003,2.6655676384963477E-2,1.3223648122448594E-3,3.8371430949535615E-5,1.9569920180282923]
[null,"HP2_TS-1",1,110.02559149210194,12.790000000000001,9160.1524588318953,454.42715883174998,13.186240427182039,261335.68929968963]
[null,"LP1a",1,139.66975678458522,1.1300000000000001,9133.9991752994119,453.12971728989783,13.14859220176554,328790.96747138951]
[null,"VLP1a",1,139.66975566642535,0.40500000000000003,2.6655676384963477E-2,1.3223648122448594E-3,3.8371430949535615E-5,0.95920608078094083]
[null,"HP1a",1,140.16975694767098,15.43,8001.0935422793318,396.92725883175001,11.517749688450358,290825.28035964142]
[null,"GHe1-2",1,4.7015618958930077,1.5429999999999999,2.0157581431225223E-2,9.9999999998683694E-4,2.9017280703265848E-5,1.4655264811831192E-2]
[null,"bypass_CC",1,4.7015618958930077,1.5429999999999999,5114.6916299908826,253.73538226171388,7.3627108115355293,3718.5592192255799]
[null,"bypass_CC-1",0.97511077991539863,4.5421903203312581,1.35,5114.6916299908826,253.73538226171388,7.3627108115355293,3718.5592192255799]
[null,"LP8-1",0.97511057167164528,4.5421903118645446,1.35,5114.7117875723143,253.73638226171386,7.3627398288162329,3718.5728737998093]
[null,3,1,12.07978683496583,5.9,2.0157581431505173E-2,1E-3,2.9017280703668846E-5,5.5150661334802994E-2]
[null,4,1,12.07978683496583,5.9,867.76372304423705,43.048999999999999,1.2491649170113344,2374.1808198002127]
[null,5,1,11.404724027332463,5.9,2.0157581431575162E-2,1E-3,2.9017280703769592E-5,5.0900107011251576E-2]
[null,6,1,11.404724027332463,5.9,465.61997348600045,23.099,0.67027016697356079,1175.7415718479656]
[null,7,1,11.389432313685745,5.83,465.61997348600056,23.099000000000004,0.6702701669735609,1175.7415718479656]
[null,8,1,11.827469424697028,5.83,1333.3836965302376,66.147999999999996,1.919435083984895,3549.9223916481783]
[null,"Gan-B",1,78.068329195532272,1.0999999999999999,843.71846546021482,292.91075251713846,1.3076794122987125,22778.919858350542]
[null,"Gan-e",1,78.068329195532272,1.0999999999999999,1060.718181437368,368.24577563791712,1.6440073139325924,28637.531873950058]
[null,"Gan-f",1,174.60139018777872,1.0499999999999998,1904.4366468975827,661.15652815505553,2.9516867262313049,119332.06786517089]

{"sheet":"Dump_STS","index":12,"n_rows":198,"n_cols":9,"rows_kept":198,"cut":false,"hidden":true,"merged":[]}
[null,"Case:","STS\\(03)-JT60-STS-OFFCase_A.HSC"]
[null,"Flowsheet:","Case (Main)"]
[null,"Current Flowsheet Environment:","Case (Main)"]
[]
[null,"Name","Vapour Fraction","Temperature","Pressure","Molar Flow","Mass Flow","Liquid Volume Flow","Heat Flow"]
[1,null,"<none>","K","bar","Nm3/h(gas)","g/s","m3/h","W*"]
[]
[null,"HP1-2",1,306.03542159212702,15.43,8387.5696336432229,416.1,12.074090500787854,663299.82394791639]
[null,"LP2",1,78.690199487455914,1.2050000000000001,7548.4284770220447,374.47094050825683,10.866128396087088,153121.11166714306]
[null,"HP3-2",1,40.721761355137318,13.51,4622.9907898746324,229.34253325909961,6.6548966648649763,48603.952358973562]
[null,"LP3",1,37.379758877707872,1.22,7548.4284770220447,374.47094050825683,10.866128396087088,72673.632253082498]
[null,"T1Inlet",1,40.73161437206312,12.392774202834453,3220.3924446049482,159.76085501874689,4.6358255755337598,33857.730911600236]
[null,"MP4",1,32.072557221351502,5.241793770895856,3214.3451701755012,159.46085501874691,4.6271203913226655,26464.855444661389]
[null,"HP4",1,31.943646708454082,13.49,4622.9907898746324,229.34253325909961,6.6548966648649763,37740.692449992923]
[null,"MP5",1,17.747829672376838,5.1917937708958561,3214.3451701755012,159.46085501874691,4.6271203913226655,14146.819609955441]
[null,"LP5",1,16.235231472817418,1.24,7548.4284770220447,374.47094050825683,10.866128396087088,31196.002775362223]
[null,"HP6",1,12.112075312407285,13.26,4622.9907898746324,229.34253325909961,6.6548966648649763,10894.556599303443]
[null,"LP6",1,12.013068985941914,1.27,4340.1305812759911,215.31008548950993,6.2477131889755162,13075.196104322948]
[null,"HP7",1,8.6228740036812042,13.25,4622.9907898746324,229.34253325909961,6.6548966648649763,4939.9375521666534]
[null,"LP7",1,7.0774411420318302,1.2750000000000001,4340.1305812759911,215.31008548950993,6.2477131889755162,7164.2660955648835]
[null,"HP7-4",1,7.1705164036235374,5.18,4588.1161582400109,227.61243325909962,6.604693867519595,4530.1161416447567]
[null,"LP8",1,4.4846096521197865,1.28,4340.1305812759911,215.31008548950993,6.2477131889755162,3289.3281159786839]
[null,"JT2-3",0.35317552342465347,4.4983395887518327,1.3,4319.9689683282131,214.30988548950992,6.2186901048157281,645.9953776007992]
[null,"LHe 3,6K",0,3.6017715941583788,0.53,0,0,0,0]
[null,"HP5",1,17.747829672376838,13.47,4622.9907898746324,229.34253325909961,6.6548966648649763,19264.058705992564]
[null,"GHe 4,3K",1,4.4989261292418519,1.3,4340.1305812759911,215.31008548950993,6.2477131889755162,3274.3280472143661]
[null,"LHe 4,3K",0,4.4989261292418519,1.3,0,0,0,0]
[null,"GHe 3,6K",1,3.6017715941583788,0.53,56.492584881145461,2.8025477695896424,8.1322315315564733E-2,41.761640315616987]
[null,"HP8-3",1,5.6342659426870227,5.16,4588.11615824001,227.61243325909962,6.604693867519595,686.0933149863771]
[null,"HP8-5",1,5.6342659426870227,5.16,268.14718991179637,13.302547769589644,0.38600376270386672,40.097937385577865]
[null,"VLP0",0.24889065054135465,3.599010089722583,0.53,56.492584881145461,2.8025477695896424,8.1322315315564733E-2,-6.6565807225444713]
[null,"MP",1,1140.1311357897196,16,8896.3509402624277,441.34019601996386,12.806492353714239,2614720.5241796752]
[null,"MP-1",1,306,16,8896.3509402624277,441.34019601996386,12.806492353714239,703534.90584278037]
[null,"TS_inlet",1,79.357536309709303,15,8387.5696336432229,416.1,12.074090500787854,173006.57684196884]
[null,"TS_outlet",1,99.401439316055786,13.6,8387.5696336432229,416.1,12.074090500787854,216371.57685386698]
[null,"To Comp LP",1,292.09579776665601,1.05,8896.3509402624277,441.34019601996386,12.806492353714239,669542.79308842623]
[null,"LIN-a",0,78.456665731170233,1.1499999999999999,619.79234440161235,215.17111386677163,0.96061627409357686,-25633.703424378753]
[null,"GAN-b",1,78.083566366962032,1.0999999999999999,658.86490445056052,228.73579620481411,1.0211748424472331,17792.128257875025]
[null,"HP2-5",1,79.357010599682042,15.01,8387.5696336432229,416.09999999999997,12.074090500787852,173006.46322265262]
[null,"to_CL-1",1,79.257041628566526,13.51,79.462079910219785,3.9420443459592129,0.11438740733292622,1635.5042542912606]
[null,"CL_inlet",1,51.99999596400869,4,275.15098653984614,13.65,0.39608588160479258,3692.8854448049274]
[null,"CL_outlet",1,300,1.05,275.15098653984614,13.65,0.39608588160479258,21268.199572502839]
[null,"GAN-c",1,297.95007782054984,1.0499999999999998,658.86490445056052,228.73579620481411,1.0211748424472331,70683.764408073883]
[null,"After Comp",1,306.03107160706776,15.5,8896.3509402624277,441.34019601996386,12.806492353714239,703534.90584278037]
[null,"LPbypass",1,306.03107160706776,15.5,266.89052820787288,13.240205880598916,0.38419477061142721,21106.047175283413]
[null,"Paliers",1,306.03107160706776,15.5,241.89097717788673,12,0.3482073684437737,19129.050438296072]
[null,"Recycle",1,307,1.05,268.70056048176917,13.330000000000002,0.3868003517796253,21254.115816195532]
[null,"To recycle",1,277.47669619542427,1.27,268.70056048176917,13.330000000000002,0.3868003517796253,19211.583344633462]
[null,"T1Outlet",1,32.072557221351502,5.241793770895856,3220.3924446049482,159.76085501874689,4.6358255755337598,26514.644821699814]
[null,"T1Leak",1,32.072557221351502,5.241793770895856,6.0472744294471683,0.3,8.7051842110943429E-3,49.789377038427517]
[null,"T2Outlet-1",1,12.01080097197331,1.27,3214.3451701755012,159.46085501874691,4.6271203913226655,9681.6726506635114]
[null,"T2Leak",1,12.01080097197331,1.27,6.0472744294471683,0.3,8.7051842110943429E-3,18.214512864976097]
[null,"T3Outlet",1,7.1705164036235374,5.18,4602.8311926849992,228.34243325909961,6.6258764824332586,4544.6451580787416]
[null,"T3Leak",1,7.1705162325517335,5.18,14.715034444988108,0.73,2.1182614913662898E-2,14.529016433984561]
[null,"LP8-1",0.99802585572431401,4.4919813978085585,1.29,4340.1305812759911,215.31008548950993,6.2477131889755162,3274.3281159786839]
[null,"VLP9-1",1,4.1282635357984532,0.53,56.492584881145461,2.8025477695896424,8.1322315315564733E-2,51.761640315616994]
[null,"HP9",0,4.5989261292418746,5.07,56.492584881145461,2.8025477695896424,8.1322315315564733E-2,-6.6565807225444713]
[null,"VLP8",1,4.7022274543303411,0.51,56.492584881145461,2.8025477695896424,8.1322315315564733E-2,61.925724579207063]
[null,"HP2-9",1,79.255148699904339,13.55,4818.6796965042586,239.05048891314038,6.936595139136843,99179.019132194197]
[null,"HP2_TS-2",1,79.25467548007893,13.56,8118.5342210194258,402.75338827784645,11.686808122003526,167097.27799836706]
[null,"HP8-4",1,5.6342659426870227,5.16,4319.9689683282131,214.30988548950992,6.2186901048157281,645.9953776007992]
[null,"VLP7",1,7.07742959132446,0.495,56.492584881145461,2.8025477695896424,8.1322315315564733E-2,99.343844554521411]
[null,"VLP6",1,12.013066980520307,0.49,56.492584881145461,2.8025477695896424,8.1322315315564733E-2,173.03288293324846]
[null,"VLP5",1,16.235227939242748,0.47500000000000003,56.492584881145461,2.8025477695896424,8.1322315315564733E-2,235.18639303185594]
[null,"VLP4",1,31.842769367980111,0.47000000000000003,56.492584881145461,2.8025477695896424,8.1322315315564733E-2,463.22542363777666]
[null,"VLP3",1,37.379759008053725,0.46500000000000002,56.492584881145461,2.8025477695896424,8.1322315315564733E-2,543.93448976633726]
[null,"LP",1,546.63629574861523,1.1200000000000001,558.46641554061478,27.705030855942262,0.80392465725010054,78648.6474916304]
[null,"CryoPumps_Inlet",0,3.6999999999999886,5,211.65460503065091,10.5,0.30468144738830205,-58.357705868762956]
[null,"CryoPumps_Outlet",1,119.99369880879487,4.5,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,6.2444212325059402E-2]
[null,"LP9-2",0,4.7023184059559071,4.4950000000000001,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,-2.1374285176654974E-4]
[null,"HP9-1",0,4.5989261292418746,5.07,211.65460503065091,10.5,0.30468144738830205,-24.939484830601497]
[null,"HP1",1,306.03107160706776,15.5,8387.5696336432229,416.1,12.074090500787854,663299.82394791639]
[null,"LP-4",1,290.84191669439696,1.05,8085.6090637994957,401.12000000000006,11.63941163584721,605914.44624316099]
[null,"To Comp VLP",1,305.39441368189028,0.35000000000000003,558.46641554061478,27.705030855942262,0.80392465725010054,43937.25564743593]
[null,"to_TS",1,79.357536309709303,15,8387.5696336432229,416.1,12.074090500787854,173006.57684196884]
[null,"to_CL-2",1,79.25467548007893,13.56,79.462079910219785,3.9420443459592129,0.11438740733292622,1635.5042542912606]
[null,"HP2-7",1,79.426887991507471,13.535,0,0,0,0]
[null,"HP2-8",1,79.255858541264843,13.535,3220.3924446049482,159.76085501874689,4.6358255755337598,66282.754611881581]
[null,"HP5-1",1,17.805031249332472,13.290000000000001,4622.9907898746324,229.34253325909961,6.6548966648649763,19364.058705992567]
[null,"Piston",1,4.4989261292418519,1.3,0,0,0,0]
[null,"To Buffer",1,306.03107160706776,15.5,-1.9876655471697533E-4,-9.8606350862340264E-6,-2.8612881621349114E-7,-1.5718715493183551E-2]
[null,"VLP8-1",1,5.6269544798210518,0.5,56.492584881145461,2.8025477695896424,8.1322315315564733E-2,76.925724579207071]
[null,"HP2-4",1,79.25467548007893,15.23,8387.5696336432229,416.09999999999997,12.074090500787852,172806.46322265264]
[null,"CP1_Inlet",0,4.5989261292418746,3.9399999999999995,4031.5162862981128,200,5.8034561407295628,-554.15758485697359]
[null,"CP1_Outlet",0,4.6935500765744109,4.1099999999999994,4031.5162862981128,200,5.803456140729562,-458.68681753605574]
[null,"TF_Inlet",0,4.5989261292418746,4.0999999999999996,4041.5950770138579,200.5,5.8179647810813861,-545.31208170584671]
[null,"TF_Outlet",1,5.6332510208197846,3.9499999999999997,4041.5950770138579,200.5,5.8179647810813861,788.68791829415341]
[null,"HP9-0",0,4.5989261292418746,5.07,268.14718991179637,13.302547769589644,0.38600376270386672,-31.596065553145966]
[null,"CP2_Inlet",0,4.5989261292418746,3.9399999999999995,2015.758143149056,100,2.9017280703647805,-277.07879242848674]
[null,"CP2_outlet",0,4.7883262533170523,4.1099999999999994,2015.758143149056,100,2.9017280703647805,-185.01769536903029]
[null,"PF_Inlet",0,4.5989261292418746,4.0999999999999996,2025.8369338648013,100.5,2.9162367107166047,-273.33598110442682]
[null,"PF_Outlet",1,5.5967489421520327,3.9499999999999997,2025.8369338648013,100.5,2.9162367107166047,356.66401889557318]
[null,"HP8-6",0,4.5989261292418746,5.09,268.14718991179637,13.302547769589644,0.38600376270386672,-31.494639244732724]
[null,"MP6",1,12.01080097197331,1.27,3208.2978957460541,159.1608550187469,4.6184152071115721,9663.458137798536]
[null,"LP9-3",8.0350974845240924E-2,4.4967127871474304,1.3,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,-2.1374285176654971E-4]
[null,"HP3-3",1,40.721761355137318,13.515000000000001,3220.3924446049482,159.76085501874689,4.6358255755337598,33857.730911600236]
[null,"GHe1-3",0.99801575229190786,4.4816891239068468,1.28,2.0157581431785126E-2,1.0000000000146129E-3,2.9017280704071837E-5,1.5207499638570075E-2]
[null,"T3Inlet",1,7.912441645983165,7.3690143964340757,4602.8311926849992,228.34243325909961,6.6258764824332586,4918.3958369177844]
[null,"LP-1",1,307,1.07,558.46641554061478,27.705030855942262,0.80392465725010054,44174.667396835364]
[null,"VLP1-1",1,290.73040221248732,0.35000000000000003,56.492584881145461,2.8025477695896424,8.1322315315564733E-2,4231.1490773000878]
[null,"VLPbypass",1,307,1.07,501.97383065946934,24.902483086352618,0.72260234193453576,39706.106570135846]
[null,"VLP-2",1,307.04471501606474,0.35000000000000003,501.97383065946934,24.902483086352618,0.72260234193453576,39706.106570135846]
[null,"Conso.liq",0,4.4977054261168519,1.3,0,0,0,0]
[null,"HP2-6",1,79.357010599682042,15.01,0,0,0,0]
[null,"From_Buffer",1,307,1.05,0,0,0,0]
[null,"LPbypass-2",1,306.03107160706776,15.5,266.89032944131748,13.240196019963797,0.38419448448261001,21106.031456566845]
[null,"LPbypass-3",1,306.92878869420406,1.05,266.89032944131748,13.240196019963797,0.38419448448261001,21106.031456566845]
[null,"GHe",1,4.4989257404402565,1.3,4340.1305812759911,215.31008548950993,6.2477131889755162,3274.3280472143661]
[null,"LP6-2",1,12.012105011159974,1.27,7548.4284770220447,374.47094050825683,10.866128396087088,22738.654242121484]
[null,"LP4",1,31.842768838200357,1.23,7548.4284770220447,374.47094050825683,10.866128396087088,61861.081410230421]
[null,"HP3-4",1,40.721761355137318,13.51,195.68890662962639,9.7079556540407879,0.28169847427186634,2057.3811905136663]
[null,"HP2_TS-3",1,79.25467548007893,13.56,8039.0721411092054,398.81134393188728,11.572420714670603,165461.77374407582]
[null,"HP3-1",1,40.721761355137318,13.51,4818.6796965042595,239.05048891314041,6.9365951391368439,50661.33354948723]
[null,"bypass",1,79.255858541264843,13.535,3220.3924446049482,159.76085501874689,4.6358255755337598,66282.754611881581]
[null,"bypass-2",1,79.255148699904339,13.55,3220.3924446049482,159.76085501874689,4.6358255755337598,66282.754611881581]
[null,"T2Outlet",1,12.015621297876407,1.29,3214.3451701755012,159.46085501874691,4.6271203913226655,9681.6726506635114]
[null,"HP8",1,5.625,5.17,4588.1161582400109,227.61243325909962,6.604693867519595,671.09331498637687]
[null,"LP-3",1,290.84066988536102,1.07,8085.6090637994957,401.12000000000006,11.63941163584721,605914.44624316099]
[null,"HP8-1",1,5.625,8.245000000000001,20.159597189633711,1.0001,2.9020182431718174E-2,3.2084423457331712]
[null,"HP7-2",1,8.0841187985830629,8.25,20.159597189633711,1.0001,2.9020182431718174E-2,21.541715248869345]
[null,"HP7-3",1,8.6228740036812042,13.25,4602.8311926849992,228.34243325909964,6.6258764824332586,4918.3958369177853]
[null,"to_damper",0.46992046789186837,4.497665885403876,1.3,2.0157581431490563E-3,1.0000000000000002E-4,2.9017280703647812E-6,5.2079215535778161E-4]
[null,22,"<empty>","<empty>","<empty>","<empty>","<empty>","<empty>","<empty>"]
[null,"WaterInlet","<empty>",303,"<empty>","<empty>","<empty>","<empty>","<empty>"]
[null,"LP-2",1,307,1.07,56.492584881145433,2.802547769589641,8.1322315315564692E-2,4468.560826699525]
[null,"HP_BP1-b",1,306.03542159212702,15.43,901.44704161625782,44.72,1.29765279306713,71287.594633383371]
[null,"HP_BP1-a",1,306.04163583935269,15.33,901.44704161625782,44.72,1.29765279306713,71287.594633383371]
[null,"HP_BP1",1,306.04163583935269,15.33,901.44704161625782,44.72,1.29765279306713,71287.594633383371]
[null,"HP2_MEF",1,89.76395501991513,15.345000000000001,0,0,0,0]
[null,"HP2_MEF-2",1,89.76472580717143,15.33,0,0,0,0]
[null,"HP2-1",1,89.76395501991513,15.345000000000001,7486.1225920269653,371.38000000000005,10.776437707720724,174633.10904021189]
[null,"HP2-2",1,89.767295172495665,15.280000000000001,7486.1225920269653,371.38000000000005,10.776437707720724,174633.10904021189]
[null,"HP_BP2",1,78.584944773220258,15.280000000000001,901.44704161625782,44.72,1.29765279306713,18416.15315864297]
[null,"HP2-3",1,88.564396546422302,15.280000000000001,8387.5696336432229,416.09999999999997,12.074090500787852,193049.26219885485]
[null,"to_TS-3",1,79.357484084643431,15,8387.567617885079,416.09989999999999,12.074087599059782,173006.42164455526]
[null,"HP_CD2-1",1,79.357010599682042,15.01,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,4.1578097385881432E-2]
[null,"HP_CD2",1,79.357484084643431,15,2.0157581431490563E-3,1E-4,2.9017280703647812E-6,4.1578097385881432E-2]
[null,"HP_CD1",1,297.9500778236411,15,2.015758144354307E-3,1.0000000005979144E-4,2.9017280720997659E-6,0.15519741359191644]
[null,"to_TS-2",1,79.357536309709303,15,8387.5696336432229,416.1,12.074090500787854,173006.57684196884]
[null,"bypass_TS",1,79.357536309709303,15,0,0,0,0]
[null,"bypass_TS-1",1,79.423859249528078,13.6,0,0,0,0]
[null,"to_TS-4",1,79.357010599682042,15.01,8387.567617885079,416.09989999999999,12.074087599059782,173006.42164455526]
[null,"bypass_HP_BP-2",1,90.404546585291769,1.2050000000000001,269.03541262379707,13.346611722153568,0.38728237878432636,6269.6620268698407]
[null,"HP2_TS",1,89.76395501991513,13.59,8118.5342210194258,402.7533882778464,11.686808122003526,189196.15534236369]
[null,"bypass_HP_BP",1,89.76395501991513,13.59,269.03541262379707,13.346611722153568,0.38728237878432636,6269.6620268698407]
[null,"LIN",5.9302840058739294E-2,78.456665731170233,1.1499999999999999,658.86490445056052,228.73579620481411,1.0211748424472331,-24574.882211339595]
[null,"GAN-a",1,78.068329195532272,1.0999999999999999,619.79234440161235,215.17111386677163,0.96061627409357686,16733.30704483587]
[null,"GAN",1,78.456665731170233,1.1499999999999999,39.072560048948098,13.564682338042463,6.0558568353656514E-2,1058.8212130391537]
[null,"N2-a",5.179708388925953E-3,83.591707086899845,1.99,658.86490445056052,228.73579620481411,1.0211748424472331,-24574.882211339598]
[null,"N2",0,83.644048867120603,2,658.86490445056052,228.73579620481408,1.0211748424472331,-24774.882211339595]
[null,"to_TS-1",1,79.357536309709303,15,8387.5696336432229,416.1,12.074090500787854,173006.57684196884]
[null,"HP_CD2-2",1,79.357536309709303,15,0,0,0,0]
[null,"HP2_TS-4",1,79.255148699904339,13.55,8039.0721411092054,398.81134393188722,11.572420714670601,165461.77374407582]
[null,"HP_CD2-3",1,79.426229237147368,13.55,0,0,0,0]
[null,"HP2-10",1,79.255148699904339,13.55,8039.0721411092081,398.81134393188722,11.572420714670601,165461.77374407579]
[null,"supply_loop",1,6.0152826555746515,8.2349999999999994,20.157581431490559,1,2.9017280703647803E-2,5.2079215535778136]
[null,"supply_loop1-1",1,5.770577743248964,4.1099999999999994,10.078790715745251,0.49999999999999861,1.4508640351823863E-2,2.6039607767888997]
[null,"CP1_outlet-2",0,4.6976391565390827,4.1099999999999994,4041.5950770138579,200.5,5.8179647810813861,-456.08285675926686]
[null,"supply_loop2",1,6.0152826555746515,8.2349999999999994,10.078790715745308,0.50000000000000144,1.4508640351823945E-2,2.6039607767889144]
[null,2,0,4.7956471386789872,4.1099999999999994,2025.8369338648013,100.5,2.9162367107166047,-182.41373459224135]
[null,"HP8-2",1,6.0152826555746515,8.2349999999999994,2.0157581431490563E-3,1E-4,2.9017280703647807E-6,5.207921553577815E-4]
[null,"supply_loop1",1,6.0152826555746515,8.2349999999999994,10.078790715745251,0.49999999999999861,1.4508640351823863E-2,2.6039607767888997]
[null,"supply_loop2-2",1,5.7705778584670497,4.1099999999999994,10.078790715745308,0.50000000000000144,1.4508640351823945E-2,2.6039607767889144]
[null,"return-1",0,4.5989261292418746,3.9399999999999995,10.078790715745289,0.50000000000000044,1.4508640351823917E-2,-1.3853939621424349]
[null,"return-2",0,4.5989261292418746,3.9399999999999995,10.07879071574528,0.5,1.4508640351823901E-2,-1.3853939621424338]
[null,"return-3",0,4.598930481339778,3.9399999999999995,20.15758143149057,1.0000000000000004,2.9017280703647817E-2,-2.7707879242848685]
[null,"CD_return",1,120.02642219348837,3.9399999999999995,211.65258927250775,10.499900000000002,0.30467854566023161,6556.5798499189123]
[null,"baking_return",1,120.02642219348837,3.9399999999999995,0,0,0,0]
[null,"LP5-1",1,16.235231472817418,1.24,7548.4284770220447,374.47094050825683,10.866128396087088,31196.002775362223]
[null,"baking_return-1",1,120.18437665478177,1.24,0,0,0,0]
[null,"LP2-1",1,79.821711346901992,1.2050000000000001,7760.0810662945523,384.97084050825686,11.170806941747319,159677.69151706196]
[null,"CD_return-2",1,120.18642620055169,1.2050000000000001,211.65258927250775,10.499900000000002,0.30467854566023161,6556.5798499189123]
[null,"CL_inlet-2",1,51.753763761969367,13.51,275.15098653984614,13.65,0.39608588160479258,3692.8854448049274]
[null,"return_4",1,120.02642219348837,3.9399999999999995,211.65258927250775,10.499900000000002,0.30467854566023161,6556.5798499189123]
[null,"return_damper",0,4.598930481339778,3.9399999999999995,20.15758143149057,1.0000000000000004,2.9017280703647817E-2,-2.7707879242848685]
[null,"HP7-5",1,8.6228740036812042,13.25,20.159597189633711,1.0001,2.9020182431718174E-2,21.541715248869345]
[null,"return_damper-1",4.6354519024926447E-2,4.4977104852241041,1.3,20.15758143149057,1.0000000000000004,2.9017280703647817E-2,-2.7707879242848685]
[null,1,1,6.0152826555746515,8.2349999999999994,20.159597189633711,1.0000999999999998,2.9020182431718167E-2,5.2084423457331717]
[null,"CP1_inlet-1",0,4.5989261292418746,3.9399999999999995,4041.5950770138579,200.5,5.8179647810813861,-555.54297881911612]
[null,"CP2_Inlet-1",0,4.5989261292418746,3.9399999999999995,2025.8369338648013,100.5,2.9162367107166047,-278.46418639062921]
[null,"HP1-3",1,306.03542159212702,15.43,7486.1225920269653,371.38000000000005,10.776437707720724,592012.22931453295]
[null,"LP2-2",1,80.176285773588006,1.2050000000000001,8029.1164789183495,398.31745223041042,11.558089320531646,165947.35354393179]
[null,"VLP2",1,78.690199321149009,0.45500000000000002,56.492584881145461,2.8025477695896424,8.1322315315564733E-2,1145.4442255760325]
[null,"TS_outlet-2",1,99.401439316055786,13.6,8387.5696336432229,416.1,12.074090500787854,216371.57685386698]
[null,"HP2",1,89.76395501991513,15.345000000000001,7486.1225920269653,371.38000000000005,10.776437707720724,174633.10904021189]
[null,"LP1",1,290.72697347869365,1.07,8029.1164789183495,398.31745223041042,11.558089320531646,601445.8854164615]
[null,"VLP1",1,290.72697343745159,0.40500000000000003,56.492584881145461,2.8025477695896424,8.1322315315564733E-2,4231.1490773000878]
[null,"HP2_TS-1",1,89.76395501991513,13.59,8387.5696336432229,416.1,12.074090500787854,195465.81736923355]
[null,"LP1a",1,98.789469282311984,1.07,8029.1164789183495,398.31745223041042,11.558089320531646,204445.67707451287]
[null,"VLP1a",1,98.789445948916011,0.40500000000000003,56.492584881145461,2.8025477695896424,8.1322315315564733E-2,1437.9447904562699]
[null,"HP1a",1,98.837927523277017,15.43,7486.1225920269653,371.38000000000005,10.776437707720724,192218.2538816774]
[null,"return-4",1,119.99369880879487,4.5,211.65258927250775,10.499900000000002,0.30467854566023161,6556.5798499189123]
[null,"CryoPumps_Outlet-1",1,119.99369880879487,4.5,211.65460503065091,10.5,0.30468144738830205,6556.6422941312376]
[null,3,0,4.598930481339778,3.9399999999999995,0,0,0,0]
[null,"GHe1-2",1,4.4989257404402565,1.3,2.0157581431785126E-2,1E-3,2.9017280704071837E-5,1.5207499638570075E-2]
[null,"bypass_CC",1,4.4989257404402565,1.3,4340.1104236945584,215.30908548950993,6.2476841716948126,3274.3128397147275]
[null,"ColdComp_Outlet",1,4.4948311730637442,1.29,2.0157581431785126E-2,1.0000000000146129E-3,2.9017280704071837E-5,1.5276263956224367E-2]
[null,"bypass_CC-1",0.9980258553982122,4.4919813694237405,1.29,4340.1104236945584,215.30908548950993,6.2476841716948126,3274.3128397147275]